
DPMI-capable
 DPMI host without extender
 Automatic DPMI entrypoint hook detection
 Display exception address
 Display hooking DPMI entry
DI command
DM command
D string commands
S match dumps line of following data
Access SDA current PSP field
Load NTVDM VDD for sector access
RM command and reading MMX registers as variables
Expression evaluator
 Indirection in expressions
Variables with user-defined purpose
Debugger option and status variables
PSP variables
Conditional jump notice in register dump
TSR mode (Process detachment)
Loadable device driver
Boot loader
Permanent breakpoints
Intercepted 86M interrupts: 00, 01, 03, 06, 0C, 0D, 18, 19
Processed 86M interrupts: 08, 2F.1687
Intercepted DPMI exceptions: 00, 01, 03, 06, 0C, 0D, 0E
Processed DPMI interrupts: 21.4C
Extended built-in help pages
