;LABEL Utility
;Message Service Routine

:util  LABL                             ;BEGIN UTIL                     ;AN000;

:class 1                                ;EXTENDED ERRORS                ;AN000;
;-------                                 ---------------
;:use  EXTEND4                          ;Too many files open
;:use  EXTEND15                         ;Invalid drive specification
;:use  EXTEND82                         ;Can not make directory entry

:class A                                ;COMMON & DEFINED MSGS          ;AN000;
;-------                                 ------------
:use 01 COMMON1                         ;Incorrect DOS version
:use 02 COMMON14                        ;Cannot %1 a SUBSTed or ASSIGNed drive
:use 03 COMMON21                        ;Invalid characters in volume label
:use 04 COMMON33                        ;Volume in drive %1 has no label
:use 05 COMMON34                        ;Volume in drive %1 is %2
:use 06 COMMON35                        ;Vol label (11 chars, ENTER for none)?
:use 07 COMMON36                        ;Volume Serial Number is %1-%2
:use 08 COMMON12                        ;Cannot %1 a network drive
:def 09 CR,LF,"Delete current volume label (Y/N)?"                      ;AN001;
:use 10 COMMON38                        ;CR,LF                          ;AN001;

:end                                    ;END UTIL                       ;AN000;
