                               lDebug manual
                               =============

2020 by C. Masloch. Usage of the works is permitted provided that this
instrument is retained with the works, so that any entity that uses the
works is notified of this instrument. DISCLAIMER: THE WORKS ARE WITHOUT
WARRANTY.

This document has been compiled on 2023-08-03.

1: Overview and highlights
--------------------------

    lDebug is a 86-DOS debugger based on the MS-DOS Debug clone FreeDOS
    Debug. It features DPMI client support for 32-bit and 16-bit segments, a
    686-level assembler and disassembler, an expression evaluator, an InDOS
    and a bootloaded mode, script file reading, serial port I/O, permanent
    breakpoints, conditional tracing, buffered tracing, and auto-repetition
    of some commands. There is also a symbolic debugging option being
    developed.

1.1 Quick start for reading this manual

     -  The interface reference explains the basics of the debugger's
        interface and lists some common commands.

     -  The parameter reference lists the types of parameters used by the
        available commands.

     -  The command reference describes most commands in detail.

     -  The expression reference details how numeric parameters are parsed
        by the expression evaluator.

     -  The variable reference lists a subset of the debugger's variables
        and what they can be used for.

     -  The interrupt reference lists what interrupt hooks the debugger sets
        up.

     -  The service reference lists what services are called by the
        debugger, which may be useful for developers of the debugger, or of
        kernels, ROM-BIOSes, or DPMI hosts.

     -  The online help pages provide some additional descriptions not found
        elsewhere in the manual, as well as overviews of many different
        topics.

     -  The command help lists most of the switches and parameters accepted
        by the debugger and the instsect program.

     -  The news lists an overview of changes since prior releases of
        lDebug.

     -  Invoking the debugger states how to start the debugger, either
        bootloaded, as a device driver, as an application, or through the
        test suite.

     -  Building the debugger lists components, build options, and
        instructions on how to build.

     -  Debugging the debugger itself lists some considerations for working
        with CDebug or DDebug as a debuggee.

     -  The additional usage conditions section lists attribution and
        licenses for the various depackers that can be used for the
        compressed debugger executable.

     -  Source Control Revision ID gives the Mercurial hash of the manual's
        source revision, and links to that revision in ecm's repository.

    For a tour, definitely start with the interface reference. To help
    invoke the debugger read the section on "Invoking the debugger as an
    application". It may help to read the manual while testing the debugger
    on another terminal. Use the main page of the online help as a reference
    to what is possible, then check the command reference for details. To
    explain what parameter types are used refer to the parameter reference.
    For how to calculate refer to the expression reference.

    Reconfiguring the debugger can be done using variables, including
    the Debugger Assembler Options (DAO) and the Debugger Common Options
    (DCO) 1 to 6. Use the variable reference and the online help pages on
    the options for those. Change variables using the R commands, such as
    "r dco or= 800" or "r ior := #50".

1.2 Some tips for using the debugger

     -  At a "[more]" prompt for pagination, entering Ctrl-C aborts the
        current command and returns to the debugger command line.

     -  Use the GT or GNT commands to skip past conditionals

     -  Use G ABO to skip past calls or loops if P would not work

     -  T, P, G, U, and D commands have autorepeat to repeat the same
        command if an empty line (only blanks) is entered after they return
        control to the debugger prompt

     -  The POINTER type expression allows using a 32-bit number as a 16:16
        segmented address whereever an address parameter is parsed

     -  The assembler can access the expression evaluator by surrounding an
        expression with parentheses "(...)"

     -  The A, E, D, and U commands write to the AAO, AEO, ADO, and AUO
        variables to point past the end of their last read or write

     -  The ABO variable points past the last instruction disassembled by an
        R command

     -  Permanent breakpoints can be set up using the B commands, including
        as pass points or conditionally

     -  The G command can repeat the prior list by specifying the AGAIN
        keyword as the first breakpoint, and can save to the list without
        actually executing the debuggee by ending the breakpoint list with a
        REMEMBER keyword

     -  T, P, and G commands can change either the instruction pointer only
        or also the code segment using an equals-sign-prefixed address as
        the first prameter. The TTEST command will change the CS:IP without
        actually executing anything.

     -  The machine type can be viewed or changed with an M command.
        Assembly and disassembly will note if a required machine level is
        absent according to the machine type.

     -  DCO option 800 enables the line editor and input history even when
        using DOS for input

     -  DCO6 option 200 will use the ROM-BIOS for output instead of DOS,
        including for register change highlighting

     -  DCO option 8 will act as if the debugger is always running with the
        InDOS flag set, avoiding DOS calls from the debugger itself

     -  The INSTALL AMIS and INSTALL TIMER commands can be used to provide
        the debugger's AMIS interface and hook the timer interrupt

     -  The DW ss:sp command is useful to view the current stack formatted
        as words

     -  The debugger is largely capitalisation-insensitive

     -  The LFSR variable allows to generate a stream of pseudo-random
        numbers

     -  The DIM command shows MCB names of blocks pointed to by interrupt
        vectors, while DIL (or DIML) will query AMIS multiplexers for their
        interrupt entrypoints to find hidden chains

     -  Long output of many commands is paged by default, displaying a
        "[more]" prompt that pauses the output until a keypress is received

     -  The VALUE IN construct allows to match one numeric value or range
        against many match values or match ranges

     -  A breakpoint can be set up on an interrupt handler by issuing for
        example "BP NEW ptr ri2Dp", if the interrupt handler is writeable

     -  If given a single expression the H command displays the result as
        hexadecimal and as decimal

     -  Decimal numbers can be entered with a # prefix, and binary with 2#.
        Character codes can be used as numbers with #"..."

     -  Script files can be run with the Y command

     -  A program can be traced until it tries
        to modify interrupts 1 or 3 using
        "tp FFFFF while ! value from linear 0:1*4 length 3*4 in writing silent".
        Add a conditional breakpoint like
        "bp new ptr ri21p when value ax in 2501, 2503" beforehand to
        intercept DOS calls to change these interrupts

     -  If at its entrypoint and you want to return from a near function,
        use "g word [ss:sp]". For a 16-bit far or interrupt function use
        "g ptr [ss:sp]"

     -  In a loop with several exit conditons, trace with T or P and
        accumulate exits with "G AGAIN address REMEMBER" (insert an offset
        or (NOT)TAKEN keywords for the address), then finally run "G AGAIN"

     -  The L and W commands for reading and writing sectors accept drive
        letters for their second parameter, specified with a trailing colon

     -  The RV, RVM, RVP, and RVD commands will show some information on
        modes, memory segment locations, processes, and device headers

     -  RX toggles the 32-bit register view for the R command

     -  The RE buffer can contain many different commands, which are run on
        RE commands or when T, P, or G initiate a register dump

     -  The DCO options are described in the full ?O help page as well as
        individual pages like ?O6 for DCO6

     -  Not sure what version of lDebug is running? The command ?BUILD
        displays the description and source control revision IDs. The
        description includes a build date or release number.

     -  Setting a breakpoint at the current instruction pointer with the
        G command will trace past this instruction once then write the
        breakpoint and run at full speed

     -  There's a TSR mode converting the application-mode debugger into a
        resident program, allowing to debug the debugger's parent process

     -  The symbolic F register for the R command allows dumping and
        modifying the flags using the abbreviated flag states

     -  The R command can modify variables using binary operators suffixed
        by an equal sign, both on the command line of the R command as well
        as after the R variable prompt

     -  By adding a trailing dot after a variable name for the R command,
        a variable's value can be inspected without bringing up a variable
        prompt that requires submitting a second input line

2: News
-------

2.1 Release 6 (future)

     -  Add TOP keyword for D, DB, DW, DD, and DX commands.

     -  Add DCO2 40_0000h for unconditional linebreak before R dump, changed
        DCO6 8000_0000h to be conditional on int 10h being used and the
        current column being nonzero.

     -  Add DCO2 20_0000h for underscores in 32-bit R variable display.

     -  Add "?VERSION" help page.

     -  Add "END" keyword to range parameter parsing.

     -  Add new INSTALL command keywords to aid reconfiguring the debugger.

     -  Application and device mode will now detect a startup Script for
        lDebug file, intended for configuration. The /IN switch disables
        this detection.

     -  Bugfix: Y command may have failed due to a line overflow.

     -  Improve detection of invalid DD commands that may be valid when
        interpreted as D commands.

     -  Display H command remainder if the last operation is a division.

     -  Add LISTLENGTH command and variable.

     -  In getinput allow Ctrl-A (like Home) and Ctrl-E (like End).

     -  DT command (ASCII table if empty, else text of specified byte
        values). Additionally, DTT command (dump text table top half).

     -  lDebugX bugfix: If dumping for example 8 bytes at 1FFF0h in a large
        segment the debugger would loop infinitely.

     -  AS SIZE keywords for E, F, S strings.

     -  Added DAO option 400h for MSDebug style opcode field width in
        disassembly.

     -  Added DCO2 10_0000h to do some R command variable prompts in MSDebug
        style.

     -  Added DCO2 option 8_0000h to display additional blanks in R command
        register dump for MSDebug style.

     -  Added DCO2 option 40000h to treat explicit length 0 as 64 KiB,
        except U treats it as length 1, to improve MSDebug compatibility.

     -  Bugfix: In F RANGE command forbid large destination lengths if the
        source range is specified in a 16-bit (limit <= 64 KiB) segment
        without a length specified. Would truncate the source to up to
        offset 0FFFFh.

     -  Quotemarks added as expression separators to improve MSDebug
        compatibility.

     -  Add lDebug ad section to manual (in section 16), comparing lDebug to
        MSDebug and original MS-DOS Debug.

     -  Allow to read .HEX files. Only record type 00h and 04h used. Can
        read files larger than 64 KiB, unlike MS Debug.

     -  Add K command (same as our default N command), and DCO2 options for
        MS Debug compatible N command.

     -  Add RC.ABORT command to allow a Script for lDebug file called from
        the RC command line buffer to modify the RC buffer itself.

     -  Add DCO6 options for style 2 and style 3 alternative flag state
        dump.

     -  Add DCO6 option to display a linebreak before R dump.

     -  New _EXPRDUALCODE build option to save some 5 kB in the first code
        segment. Disabled by default.

     -  Fix: Device mode debugger should not retain an open handle for
        FDCONFIG.SYS.

     -  Trying to open the LDEBUG$$ device will now cause a critical error.

     -  Some code in the run exit and entrypoints can be moved into entry
        segment, saving about 250 bytes in the first code segment.

     -  DPMI exception entrypoint handlers can be moved into entry segment,
        saving nearly 300 bytes in the first code segment.

     -  Fix: When a symbol table is allocated in DOS memory and the debugger
        quits with a QD command, the table would stay allocated.

     -  Add ATTACH command to attach to a PSP, can be used while application
        mode or device mode debugger is resident. (Opposite of TSR command.)

     -  MMX register support in expression evaluator optimised to take up
        less run time of other expression terms

     -  mktables program extended, allowing for builds of the debugger that
        do not contain table entries above specified machine level.

     -  Non-boot-loaded modes now discard the ?BOOT help page, saving 2.7 kB
        of resident memory use.

     -  Refactor to store long help messages in another segment, reducing
        the pressure of the data entry segment by 22 kB.

     -  Fix QC command if not last in container, would corrupt MCB chain

     -  Application and device driver mode now discard most of the boot
        loaded mode code, saving about 9 kB of resident memory use.

     -  Fix an lDebugX D command bug on non-386 machines

     -  Add build option _APPLICATION, to create special-purpose builds if
        disabled. (Not provided pre-built as yet.) $RESULTEXT variable for
        mak.sh can set a filename extension other than ".com".

     -  getinput redraw optimised, fewer complete redraws

     -  Add DCO3 option 0100_0000h to highlight prefix/suffix in getinput if
        text parts are not visible

     -  Improve handling of very narrow displays

     -  RE.LIST and RC.LIST use the IOCLINE setting now

2.2 Release 5 (2023-03-08)

     -  Client PSP is now stored internally as a segment, even when lDebugX
        is in Protected Mode. DM command now shows this segment rather
        than a selector. (The PSPSEL variable can be read for a selector
        instead.)

     -  RM command now accepts an optional size keyword

     -  "IF EXISTS R variable THEN" command added

     -  MMX support of the machine is re-detected after lDebugX switched
        modes

     -  Fix: RM command and MMxy variable read and R MMxy variable write
        work now

     -  Fix: In /E+ mode a zero word is now pushed to the initial stack

     -  dosemu2 -dumb mode now detected specifically when needed for
        register change highlighting to ROM-BIOS interrupt 10h

     -  Fix: Bootloaded init could have corrupted part of its image during
        second relocation, if needed. (This case cannot occur during normal
        load at 200h:0 on a machine with 512 KiB or more of available LMA.)

     -  Fix: Creating a process resets the DTA to PSP:80h

     -  Fix: "R VD" accesses VD variable, rather than run "RVD" command

     -  Improvements to support NEC V20 machine

     -  Add CIP and CSP variables, use CIP for EXECUTING keyword

     -  Fix error handling if S command search area is shorter than search
        mask

     -  IOCLINE variable added to support display on the HP 95LX's narrow
        screen

     -  Fix: Stack access variables set wrongly for interrupt instructions

     -  Fix: In DPMI protected mode QA or Q command sometimes would not work

     -  Immediate assembler merged. Currently defaults to disabled at build
        time.

     -  Bootable lDebug: Allow to access small FAT32 file system (less than
        64 Ki clusters)

     -  Add timer configuration variables and default the SDELTALIMIT
        variable to 5 to improve wait performance

     -  Serial I/O: Add option to always do EOI after calling downlink for
        IRQ sharing. Autodetect in KEEP prompt if this option must be used
        or if IRQ sharing must not be used.

     -  Query patch support for ldosboot iniload can be used to set the
        BOOTUNITFLx variable for the debugger load unit

     -  Change: DCO6 option 200h only makes output go to ROM-BIOS, new DCO6
        option 0100_0000h makes all Input/Output use ROM-BIOS. (The 200h
        flag still allows to read script files from DOS.)

     -  lDebugX: Fix, allow to use TSR command in PM (expected a segment
        where a selector was read)

     -  lDebugX: Fix PSP variables and TSR command expecting higher limit in
        PM (getsegmented now sets limit 0)

     -  lDebugX: Fix getexpression not preserving the scratch selector

     -  Add FL.xF variables to read flag status in expressions, eg FL.CF
        which reads as 1 if CY and 0 if NC

     -  When creating an empty process (eg after QA command) also write the
        current command line tail to it (instead of the debugger's internal
        N buffers)

     -  Display amount of ancestors for the symsnip revision ID

     -  A pair of 32-bit E command fixes

     -  Write AES:AEO (e_addr) in E command and allow E command without an
        address

     -  lDebugX: Add DESCTYPE keyword in expressions

     -  lDebugX: Add descriptor modification commands and DARESULT variable,
        refer to section 10.15

     -  Add XARESULT variable for XA command

     -  Allow to share the serial IRQ so eg two lDebug instances can be
        connected to two serial ports that use the same IRQ, like COM2 and
        COM4 (both use IRQ #3 by default)

     -  Do not simulate repeated string scan/compare instructions when
        disassembling them using the U command (only do so for R command
        disassembly)

     -  Disassembler handles o32/o16 OSIZE prefixes as belonging to push and
        pop with segregs, instead of displaying the prefix as "unused".

     -  If simulation of repeated string scan/compare instructions is
        disabled in DAO then the access variables will now be set up
        assuming a count of 1, rather than the maximum possible count.

     -  Add convenience entrypoints for debuggable mode at CODE:1,
        CODE2:0, and CODE2:1. The offset 0 entrypoints will return to the
        main command loop, called "cmd3". The offset 1 entrypoints will
        additionally display a linebreak.

     -  Allow switching lCDebugX to debuggable mode upon putrunint and allow
        running a breakpoint early in putrunint.

     -  Add AMIS private function 33h, provided by lDebugX by default and
        can be used by lDDebugX/lCDebugX by default

     -  Add INSTALL and UNINSTALL commands

     -  Allow to specify length of D command with LINES keyword

     -  Add DEFAULTDLEN, DEFAULTDLINES, DEFAULTULEN, and DEFAULTULINES
        variables to modify default sizes of D and U commands

     -  Display long numeric constants with underscore separators for
        readability in online help pages and documentation

     -  Allow to disable disassembler memory access for referenced memory
        and repeated string instruction simulation, using four new DAO flags

     -  Change HP 95LX 40-column friendly mode support in the disassembler
        to use two DAO flags rather than two DCO6 flags (one of which was
        shared)

     -  Allow to specify variable RIxP/S/O/L with x as a single-digit
        hexadecimal number

     -  Bugfix: Allow operators between ?? and :: in a ternary operator
        expression for H command

     -  Allow to specify SILENT keyword followed by a number before the S
        command's range or list, display only up to a certain amount of
        results

     -  Add CLR operator, bitwise AND with the bitwise NOT of the right hand
        operand. Precedence above bitwise AND.

     -  Bugfix: Absolute value operator ? should always give its result an
        unsigned type

     -  Allow switching lCDebugX to debuggable mode upon debugger exception
        and allow running a breakpoint early or late in debugger exception.

     -  Add debugger exception areas to display the cause of a memory
        access which may fault in the debugger. Also adds a linebreak for
        eg referenced memory reads to work in tandem with the partial
        disassembler output. (Idea from FreeDOS Debug/X, though there it
        only does a linebreak and implements it differently.)

     -  Bugfix: Disassemble mov with segreg and memory operand always with
        m16, ignoring the operand size selected. In assembler never emit an
        osize prefix and reject an explicit dword size keyword.

     -  In disassembler display instruction and referenced memory address
        before accessing memory, so partial output is displayed in case a
        fault occurs in the debugger (FreeDOS Debug/X pick)

     -  Document side effects of expression evaluator

     -  Bugfix, allow all valid address parameter formats for the source
        address of an M move memory command (suggested by FreeDOS Debug/X)

     -  Add AMIS private function 31h to instruct lDebugX to try to install
        its DPMI hook, make use of this in lDDebugX and lCDebugX

     -  Add descriptions of BOOT commands to manual

     -  Fix HIDDEN= keyword for BOOT READ/WRITE with partition specified,
        add HIDDENADD= keyword to modify rather than replace hidden sectors

     -  Fix a bug in BOOT PROTOCOL= command that could disallow use of ENTRY
        and BPB parameters if running a non-DPMI build on a 386+ machine

     -  Avoid faults in the debugger if a code selector with a low limit
        gets used for writing, eg by A or E commands

     -  Fix bug setting wrong debuggee CS limit if _DUALCODE build

     -  Add variables DSTACKSEG/SEL, DENTRYSEG/SEL, DCODE1/2SEG/SEL,
        DAUXBUFSEG/SEL, DHISBUFSEG/SEL, DSCRATCHSEL, DSYM1/2SEL (selector
        variables only for lDebugX, symsels only for symbolic lDebugX)

     -  RVM command shows second code segment if _DUALCODE build

     -  In C, E, and A commands in PM display original selector, not the
        scratch selector as replacement. Variable AAS is also affected by
        this.

     -  Fix a bug with different selectors for lDebugX C and M commands
        (picked from FreeDOS Debug/X version 2.00)

     -  Add taken keywords to address parsing, refer to section 8.2. (This
        effectively adds the GT and GNT commands, as well as TTEST=TAKEN and
        TTEST=NOTTAKEN to change (e)ip.)

     -  Bugfix: Allow entering double-slash to disable second file search
        for the BOOT PROTOCOL= command even if no command line follows

     -  Application /C= switch and kernel command line will now skip leading
        blanks following a semicolon that is converted to a linebreak

     -  Modify serial interrupt handler to pass on interrupt call if the PIC
        does not indicate an interrupt in the In-Service Register (ISR)

     -  Add /M switch and interrupt 7, 0Ch, 0Dh hooks (for R86M exceptions),
        though build options for all of them are disabled by default

     -  Add force BPB CHS geometry (4) and force LBA access (2) flags to the
        BOOTUNITFLx flag variables

     -  Add switches /F and /E

     -  Allow zero as parenthetical partition specification, allow to access
        partition u(bootldpunit).(bootldppart) if LDP is equal to FDA

     -  Bugfix: Reading with BOOT command that crossed 64 KiB DMA boundary
        would copy too much or too little from the sector segment to target

     -  Start of HP 95LX support (NEC disassembly repeat rules, narrower
        R/U/D command output, do not intercept interrupt 6)

     -  Bugfix: Command r f . no longer displays garbage

     -  Use test_high_limit to check segment limits, to determine whether to
        use 32-bit offsets in several spots

     -  Disable calling XMS by Protected Mode far call by default

     -  Add dual code segment support to allow code size beyond 64 KiB

     -  Introduce dash prefix to commands to disable symbolic debugging
        features (no-op if not symbolic build)

     -  Introduce U address LENGTH length LINES keyword to disassemble a
        number of lines rather than bytes

     -  Add BS command for swapping permanent breakpoint indices

     -  Document doubled delimiter quote mark for lists and string literals

     -  Add string literal escaping of delimiter quote mark by doubling the
        delimiter quote mark

     -  Add /2 switch to use alternative video adapter for debugger output
        if available (pick from FreeDOS Debug)

     -  Add ?OPTIONS help page and specific pages for DCO1, DCO2, DCO3,
        DCO4, DCO6, DIF, and DAO

     -  Set new INICOMP_WINNER build variable so as to use lzsa2 compression
        for current releases

     -  Add _DEBUG_COND build option to allow toggling debug mode on and off
        at run time

     -  Add INT8CTRL variable which contains number of ticks to wait for
        Control pressed entrypoint; set to zero to disable

     -  Fix: Control-C also aborts RC command buffer execution

     -  Fix: Default operand for AAM and AAD instructions is omitted in
        disassembler

     -  Enhancement: If at the end of a stdin-redirected file the debugger
        cannot quit it will now enable InDOS mode and allow the user to
        control the debugger afterwards

     -  Fix: Do not crash or loop infinitely upon encountering the end of a
        stdin-redirected file

     -  Extract more source files from debug.asm

     -  Allow appending 00 to a 16-bit register name to get a 32-bit value
        with the register value in the high word

     -  Do not cause error from empty /C='' switch

     -  Use ampersand prompt to display commands run from RC buffer

     -  When loading a .BIN file set the process's command line buffer the
        same way as if loading a .COM file

     -  Add heading hash links to every heading in the ldebug.htm manual
        (requires patched Halibut)

     -  Add LFSR and LFSRTAP variables

     -  Run unix2dos on ldebug.txt manual

     -  Add QD (quit from device initialisation) and QC (quit from device in
        container MCB) commands

     -  Add RVD command to display device header address and allocation
        size, as well as DEVICEHEADER and DEVICESIZE variables to read same

     -  Bugfix, on pass or non-pass permanent breakpoint hit while running
        with T/TP/P command do not check WHILE condition

     -  Add PARAS keyword to range length parsing, to multiply a count by 16
        (size of a paragraph)

     -  Bugfix, should allow to run if int 2Fh is invalid

     -  Add device-driver mode to allow loading the debugger in CONFIG.SYS

     -  Fix, do not crash if no UMCB but int 21.5803 works

     -  Add V commands and /V command-line switch (video screen swapping)

     -  Add RIxxP variables to read IVT entries in a way suitable to be used
        as POINTER type expressions

     -  Work around FreeDOS kernel bug prior to 2022 May so as to fail on
        loading an empty executable

     -  Fix, also use SDA manipulation to change current PSP when lDebugX is
        in Protected Mode

     -  Add TERMCODE variable to read int 21.4D return after debuggee
        process terminated

     -  Add QB command (run breakpoint late in debugger quit)

     -  Add RVP command to display debugger mode and current debuggee and
        debugger process addresses

     -  Add (D)PSP|PARENT|PRA|PSPSEL variables

     -  Do not try to proceed past a call near immediate if the called
        functions consists of a retf instruction. (This supports a method
        for relocation, used for example by the debugger itself.)

     -  Add command-line switch /B to run a breakpoint early

     -  Add RC commands to view, change, and run RC buffer commands, re-
        using the command line buffer

     -  Add MACHX86 and MACHX87 variables to read machine type

     -  Allow M machine type command to parse an expression for the machine
        level number to set

     -  Add QA command (try to terminate attached process)

     -  Fix int 19h and debuggee termination handling. Int 19h in a DOS
        application mode now sets up registers to terminate the current
        process when running the debuggee again.

     -  Add an lDebugX option DCO3 20_0000 to break on entering PM

     -  Add an lDebugX option DCO3 10_0000 to use a 32-bit stack segment for
        the debugger itself (can help compatibility)

     -  Fix so that semicolon is allowed as End Of Line in getrange

     -  Fix R size [mem] := val causing a fault in the debugger if value
        ends in FFFFh

     -  Implement POINTER types for handling a 32-bit expression as a 16:16
        far pointer

     -  Implement basic handling of expression types (signed/unsigned)

     -  Revision IDs in ?BUILD command list the amount of ancestors to help
        to compare revisions

     -  Fix a segment addressing bug when switching modes (eg have a
        breakpoint in a DPMI allocation while the client is running in 86
        Mode)

     -  Fix some cases of detecting 32-bit offsets incorrectly

2.3 Release 4 (2022-03-08)

     -  Recognise LF as linebreak in serial input

     -  E interactive mode fixes:

         -  Support LF to exit interactive mode (that is, accept Linux style
            linebreaks)

         -  Support DEL sent by serial terminal

         -  In lDebugX correctly handle 32-bit offsets

         -  Also write new value when minus is entered

         -  Honour blank for continue to next byte, CR or dot for exit
            interactive mode

         -  Always correctly read value even if blank is entered afterwards

         -  Improve E interactive mode compatibility across different input
            sources (like stdin file, script file, serial terminal)

         -  Display linebreak upon new address displayed

     -  Fix: Register variable "CH" would be misparsed as "CHAR" type
        instead of the expected variable

     -  Allow DI command to receive an IN value list similar to the y in a
        VALUE x IN y construct

     -  Fix: Allow to set a breakpoint on an interrupt 21h handler and do
        not crash or corrupt state if the debuggee then terminates. (That
        is, do not call service 4Dh before restoring breakpoints.)

     -  Fix: Too long N command could crash the debugger

     -  Fix: DDebug TSR quit would not work correctly due to overflowing a
        rel8 jmp

     -  Add R, M, and L key letters to DI command (always 86 Mode, show MCB
        names, follow AMIS interrupt lists)

     -  Fix: R WORD [memory] prompt would not consider the size keyword as
        part of the input line prompt

     -  Add AMIS private function 30h - Update IISP Header

     -  In DI command in 86 Mode follow IISP headers

     -  Add QQCODE variable

     -  Add BOOT[L|Y|S][UNIT|PART] variables, BOOTUNITFL(x) variables

     -  Add bzpack compression method

     -  Drop DPS variable when building without DPMI support

     -  Fix PSP variables in Protected Mode: PSP is always a 86 Mode
        segment, PSPS is a segment or selector, and PPR and PPI work

     -  Add HHRESULT variable

2.4 Release 3 (2021-08-15)

     -  Add workaround with extra int 23h and int 22h handlers and raw mode-
        switching to use interrupt 21h service 0Ah in PM. DCO2 flag 800h
        clear by default.

     -  Add TRYAMISNUM variable to try a specific AMIS multiplex number
        first

     -  Add DCO4 flag 2 to allow disabling lDebugX's int 2Fh hook

     -  Build option _MEMREF_AMOUNT enabled by default

     -  mktables switches direction and stackhinting enabled by default

     -  Fix DOS application script file reading to honour InDOS status

     -  Fix H BASE= command with GROUP= sometimes displaying trailing
        garbage

     -  Fix DDebugX hooking random PM interrupts

     -  Fix trailing blanks in DI command

     -  Added a number of automated acceptance tests

     -  Add variable AMISNUM to read the multiplex number

     -  Fix an old bug in the assembler that happened to make instructions
        like "mov ax, 0" fail to assemble now

     -  Made interrupt 8 hook optional, default-off

     -  Added optional, default-off interrupt 2Dh hook

     -  Properly unhook interrupts utilising IISP header chains, if the
        debugger's interrupt handlers are reachable. Added DCO4 flags (upper
        16 bits) to force unhooking if a handler is unreachable. If a
        handler is both unreachable and not forcibly unhooked then it stays
        hooked. The Q command fails in that case.

     -  Fix to allow "$" prefix to segments in DebugX while in Real/Virtual
        86 Mode

     -  Debugger's 86 Mode entrypoints now use the IBM Interrupt Sharing
        Protocol header. (However, it is still assumed that the debugger
        _owns_ the interrupt entrypoints.)

     -  Add WIDTH= keyword handling to H BASE=

     -  Introduce variables IOL and IOF to control how many levels of
        execution are cancelled by Control-C

     -  Scripts with CR LF linebreaks at the end or after calling another
        script no longer cause superfluous empty lines to be processed

     -  Control-C aborts script file reading that is in progress

     -  Bugfix, when calling three nested levels of Y script files while
        bootloaded then the outermost script's already buffered content
        would not rewind properly

     -  Fix so that Control-C from ROM-BIOS keypress buffer is consumed
        properly while reading script file, instead of looping forever

     -  Check for Control-C in ROM-BIOS's circular keypress buffer, add
        variables IOS and IOE

     -  Extend Control-C handling so RE buffer execution is aborted by it

     -  Add a simple BOOT DIR command (SFN name only, attributes, size
        (using FAT+), datetime)

     -  Add string literals #"..." to expression evaluator

     -  Add H BASE= command

     -  Add merge and debug switches to mktables. Both are default off for
        now. Merging means redundant operand list tails are merged.

     -  Bugfix, accessing the variable SRC caused an infinite loop

     -  LZMA-lzip depacker fixed to not use cs xlatb, as the segment
        override prefix may be ignored on CPUs below 386

     -  Added conditional ?? :: construct operator

     -  Merged branch uumemref and made memrefs available in default branch.
        The build option _MEMREF_AMOUNT must be enabled to use them.

     -  Memory access direction and stack hinting in the assembler and
        disassembler tables. Switches named direction and stackhinting to
        mktables program. (Default off for now.)

     -  LINEAR term allowed in expressions

     -  VALUE IN construct allowed in expressions

     -  Commas are only allowed between expressions, no longer within
        expressions

     -  If DCO2 flag 8000h is set during RE buffer execution and SILENT 1
        was used do actually only display last RE output

2.5 Release 2 (2021-05-05)

     -  Documented SLEEP command

     -  Line editing history for raw terminal/serial input (in a fixed
        segment of size 8 KiB currently)

     -  Fix missing register dump after T/TP/P which ends up matching a non-
        pass non-hit breakpoint

     -  Fix: Entering a literal as 3#102002022201221111211 or #4294967296
        would overflow silently to zero instead of causing an error

     -  Reset high words of EIP and ESP when trying to terminate client
        process

     -  Add change highlighting to R register dump

     -  Assembler internals: Allow ASM_ESCAPE usage when needed

     -  If BL command is given an unused index do not display incorrect WHEN

     -  Reset segment registers when trying to terminate client process

     -  Handle unusual SIB bytes correctly in P command's disassembly

     -  Bugfix, Y script file called by another Y script file would turn
        quiet

     -  Bugfix, if permanent breakpoint WHEN condition was in use then the
        wrong index and ID would be displayed in the pass/hit message

     -  Acknowledge IRQ to secondary PIC too if applicable (if using a high
        IRQ for the serial I/O interrupt)

     -  Bugfix, in BOOT commands do not prepend a word to the auxbuff
        anymore

     -  Only create manual in HTML, text, and PDF formats

     -  Add files doc/fdbuild.txt and doc/LDEBUG.LSM for FreeDOS packages

     -  BOOT: work around qemu bug with "LOOPNZ"

     -  BOOT: retry CHS reads up to 16 times

     -  Add instsect and lDebug command help to manual

     -  Expression evaluator allows "OR=" as synonym for "|=" (especially
        useful if shell does not allow specifying pipe symbol for /C)

     -  Assembler: Allow specifying "LOOPxx destination, (E)CX" as in NASM
        instruction reference to specify address size

     -  For assembler allow specifying "INT BYTE 3" to get CDh encoding and
        display it this way in disassembler

     -  Only adjust offset saved in PSP's SPSAV variable if it points to our
        stack

     -  In assembler do not allow sizeless memory operand when immediate
        matches IMMS8 (eg "add [100], 12")

2.6 Release 1 (2021-02-15) and earlier

     -  "G REMEMBER" command to work with the saved temporary breakpoint
        list

     -  WHEN conditions for permanent breakpoints

     -  RIxxO/S/L variables (read-only view of IVT entry)

     -  3BYTE type for "R var" and indirection in expression evaluator

     -  In disassembler handle unusual SIB byte contents correctly

     -  IDs for listing permanent breakpoints

     -  In disassembler correctly dump far memory operands, double memory
        operands (BOUND), and do a32 addressing

     -  Add "S range REVERSE" command

     -  Fix corner case of S command: The commands "f 100 l 10 0" \
        "s 100 l 10 0" should result in 16 matches

     -  SROx and SRC search result variables

     -  SLEEP command

     -  H command displays decimal numeric value (when given a single
        expression)

     -  In disassembler display WORD keyword when o16 in 32-bit CS

     -  Bugfix, in XR do not skip first digit of allocation size

     -  G and T/TP/P breakpoints work reliably in DebugX when the client
        enters, leaves, or switches from/to Protected Mode

     -  F and S command allow accepting "RANGE" specifications for source
        data

     -  Add TTC/TPC/PPC default step counts for T/TP/P commands

     -  DW/DD commands to dump memory in words or doublewords

     -  Manual added (this document)

     -  RE buffer execution to run almost arbitrary commands when T/TP/P/G
        intend to dump register contents

     -  Conditional control flow with IF and GOTO in a script file

     -  /C command line option to pass commands to the debugger on startup

     -  In assembler allow specifying SHORT/NEAR/FAR for jumps and calls

     -  Script file reading

     -  Pass point functionality (inspired by DR-DOS's SID) using counters

     -  G LIST command to list the saved temporary breakpoint list

     -  Auto-repetition for G command, G AGAIN command

     -  DebugX's DPMI entrypoint hooking automatically checked instead of
        always avoiding it on MSW and dosemu

     -  Serial port I/O, with defaults (for COM2) that can be reconfigured
        using debugger variables

     -  Permanent breakpoints

     -  Buffered tracing using "P/TP/T ... SILENT" which writes to an
        internal buffer during the run then replays the last entries from it
        upon finishing the run

     -  TP command which is like T except it handles repeated string
        operations like P

     -  DM command lists MCB sizes in decimal Bytes/KiB

     -  Conditional tracing using "P/TP/T ... WHILE" conditions

     -  L and W commands allow drive letters instead of numbers

     -  Bootloaded mode and its BOOT commands

     -  NASM style address disassembly, blanks after commas, keywords
        uncapitalised

     -  TSR mode and command to enter it

     -  R command allows treating flags (CF, ZF, etc), debugger variables,
        registers, and memory variables (byte, word, 3byte, dword) as
        variables

     -  Conditional "jumping" and "not jumping" notices in register dump's
        single-line disassembly

     -  Options DCO1, DCO2, DCO3, DAO to modify some behaviour

     -  Extended online help pages

     -  _DEBUG option which swaps the exception handlers and thus allows
        debugging most of the debugger itself (_DEBUG builds are not
        included in the package and have to be created by building them
        specifically)

     -  Arbitrary unsigned 32-bit expression evaluator

     -  Paging for long command output

     -  Usage conditions changed to Fair License (having asked Paul Vojta
        and received his confirmation), prior conditions also allowed as
        alternatives

3: Building the debugger
------------------------

    Building lDebug is not supported on conventional DOS-like systems.
    (DJGPP environments may suffice but are not tested.) Assembling the main
    debugger executable may require up to 1 GiB of memory.

3.1 Components for building

    The following components are required to build with the provided
    scripts:

     -  bash - to run mak* scripts

     -  perl - to patch binaries (overwrite unused revision IDs)

     -  grep - to detect whether boot loading is in use, and to export
        variables

     -  sed - to filter dosemu2 output

     -  hg (Mercurial) - to retrieve revision IDs

     -  wc - to count amount of ancestors

     -  GNU time - when $use_build_time is enabled, to display main
        assembler run's memory use and wall time

     -  python - to run hg and to run the test suite

     -  C compiler - to compile supporting programs

     -  dosemu2 - to run build decompression tests (optional)

     -  qemu - to run build decompression tests (optional)

     -  nasm - to assemble. NASM versions to choose:

         -  NASM versions up to 2.07 fail -- "%deftok" is not supported

         -  NASM versions prior to 2.09.02 fail -- "%deftok" is implemented
            wrongly

         -  NASM version 2.09.02 works (last tested 2019-11)

         -  NASM versions 2.09.03 to 2.09.10 all fail --
            "%assign %$foo%[bar] quux" doesn't function right

         -  NASM version 2.10.09 works (last tested 2019-11)

         -  NASM version 2.14.03 works (last tested 2020-12)

         -  NASM version 2.15.03 works (last tested 2020-12)

         -  NASM version 2.16 (current git head) fails, due to a bug with
            %strcat and a bug with %assign ?%1 and a bug with %00

         -  (As of 2022-08-23) Current git head with a patch for the %strcat
            bug and with a patch for the %00 bug works (last tested 2022-08)

         -  NASM version 2.16rc10 works (last tested 2022-11)

         -  Upcoming NASM version beyond 2.16.01 works (last tested 2023-
            07), with a patch to fix a major memory leak

     -  halibut - to build this manual

     -  supporting programs:

         -  mktables (included in debugger source)

         -  tellsize (included in separate repo called tellsize)

         -  mktmpinc.pl (included in separate repo called mktmpinc, to
            create temporary include files, optional)

         -  crc16-t/iniload/checksum (included in separate repo called
            crc16-t, to add checksumming, optional)

         -  a 86-DOS kernel and shell (to run build decompression tests or
            the test suite, optional)

     -  additional sources (must be referenced in cfg.sh or ovr.sh):

         -  lmacros (macro collection)

         -  scanptab (partition table scanning for bootable debugger)

         -  ldosboot (iniload frame for bootable debugger, boot sector
            loaders)

         -  instsect (application to install boot sector loaders)

         -  bootimg (to run decompression test with qemu and create boot
            image for qemu to use for the test suite)

         -  inicomp (if to use compression support), also needs one of:

             -  brieflz (blzpack)

             -  lz4 (lz4c)

             -  snappy (snzip)

             -  exomizer -- recommended as this usually results in the
                smallest files

             -  x-compressor

             -  heatshrink

             -  lzip -- usually even smaller than Exomizer but takes longer
                to decompress

             -  lzop

             -  lzsa

             -  apultra

             -  bzpack

         -  crc16-t/iniload (if to add checksumming)

         -  symsnip (only if symbolic option is enabled)

3.2 How to build

     1. Clone the mercurial repo from https://hg.pushbx.org/ecm/ldebug or in
        an existing repo use "hg pull" to update the repo

     2. Update the repo with "hg up" or "hg up default" or any other
        available commit you want to build

     3. Clone the other needed repos from https://hg.pushbx.org/ecm/ or in
        existing repos use "hg fetch" or the sequence of "hg pull" then
        "hg up" to update the repos. (Usually the additional source repos do
        not have multiple branches.)

     4. Copy the ldebug/source/cfg.sh file to ovr.sh in the same directory

     5. Edit ovr.sh to point to the repos

     6. Edit INICOMP_METHOD in ovr.sh to select none, one, or several
        compression methods. Surround multiple values with quotes and
        delimit with blanks. If the value "none" is used no compression will
        occur. If several values are given the smallest of the resulting
        files will be used as the ldebug.com result. This favours LZMA-
        lzip (lzd) and Exomizer 3 (exodecr) compression as they result in
        the best ratios. The uncompressed ldebugu.com file will always
        be generated, you can rename or copy or symlink it to use it as
        ldebug.com if you want.

     7. If you have dosemu2 or qemu, you may enable the
        use_build_decomp_test option. This insures that the compressed
        executables will actually succeed in decompression when entered in
        EXE mode, and will lower the required minimum allocation given in
        the EXE header to the minimally required value so that decompression
        will still succeed. This defaults to using dosemu2, which must have
        a DOS installed that allows filesystem redirection. DEFAULT_MACHINE
        can be used to select qemu instead. The options BOOT_KERNEL,
        BOOT_COMMAND, and BOOT_PROTOCOL must be set up then to allow
        building a bootable diskette. (This is needed because qemu does not
        offer filesystem redirection for DOS.)

     8. The use_build_revision_id option is by default on. It requires that
        the sources are in hg (Mercurial) repos and that the hg command is
        available to run "hg id". The resulting revision IDs are embedded
        into the executable and will be shown for the ?B (long) and ?BUILD
        (short) commands.

     9. In ovr.sh you can also specify which tools to use. For example, the
        variable $NASM specifies the nasm executable to use, with path if
        needed.

     10.If you want to rebuild debugtbl.inc you should compile mktables then
        run it. While in the ldebug/source directory, run "./makec" (or
        use whatever C compiler to build mktables) then "./mktables" next.
        Note that mktables only needs to be used if either the source files
        (instr.*) changed or the mktables program itself has been altered.
        If the assembler and disassembler tables are not to change then
        mktables need not be used.

     11.Finally, run "./mak.sh" from the ldebug/source directory.
        You may pass environment variables to it, such as
        "INICOMP_METHOD=exodecr ./mak.sh" to select Exomizer compression.
        You may also pass it parameters which will be passed to the main
        assembly command, such as "./mak.sh -D_DEBUG4" to enable debugging
        messages.

    The mak.sh script expects that the current working directory is equal
    to the directory that it resides in. So you'll always want to run it as
    "./mak.sh" from that directory. The same is true of the make* scripts.

    The make* scripts work as follows:

    make

        calls mak.sh to create debug and debugx

    maked

        calls mak.sh to create ddebug and ddebugx

    maker

        calls mak.sh to create only debug

    makerd

        calls mak.sh to create only ddebug

    makex

        calls mak.sh to create only debugx

    makexd

        calls mak.sh to create only ddebugx

    ldebug/tmp, ldebug/lst, and ldebug/bin will receive the files created by
    the mak script. The following filenames are for the default when running
    mak.sh on its own which is to create debug. (When ddebug, debugx, or
    ddebugx are created, the names change accordingly.) In the ldebug/bin
    subdirectory, debug.com will be a nonbootable executable (even if the
    _BOOTLDR option is enabled). This executable can safely be compressed
    using EXE packers such as the UPX. (In cfg.sh the option use_build_shim
    now controls whether debug.com is created. It defaults to disable this
    output file.) If the _BOOTLDR option is enabled, ldebug.com will be a
    compressed bootable executable (if any compression method is selected),
    whereas ldebugu.com will be an uncompressed bootable executable.
    These bootable executables must not be compressed using any other
    programs. Doing that would render the kernel mode entrypoints unusable.
    Incidentally, UPX rejects these files because their "last page size" MZ
    EXE header field holds an invalid value.

    The bootable executables can be used as MS-DOS 6 protocol IO.SYS, MS-
    DOS 7/8 IO.SYS, PC-DOS 6/7 IBMBIO.COM, FreeDOS KERNEL.SYS, RxDOS.3
    RXDOS.COM, or as a Multiboot specification or Multiboot2 specification
    kernel. In any kernel load protocol case, the root FS that is being
    loaded from should be a valid FAT12, FAT16, or FAT32 file system on
    an unpartitioned (super)floppy diskette (unit number up to 127) or
    MBR-partitioned hard disk (unit number above 127). In addition, the
    bootable executables also are valid 86-DOS application programs that
    can be loaded in EXE mode either as application or as device driver.
    (Internally, all the .com files are MZ executables with a header, but
    they are named with a .COM file name extension for compatibility.)

    It is valid to append additional data, such as a .ZIP archive, to any of
    the executables. However, if too large this may render loading with the
    FreeDOS load protocol impossible. All the other protocols work even in
    the presence of arbitrarily large appended data.

3.2.1 How to build the instsect application

     1. Clone the mercurial repo from https://hg.pushbx.org/ecm/ldebug or in
        an existing repo use "hg pull" to update the repo

     2. Update the repo with "hg up" or "hg up default" or any other
        available commit you want to build

     3. Clone the other needed repos (lmacros, ldosboot, instsect) from
        https://hg.pushbx.org/ecm/ or in existing repos use "hg fetch" or
        the sequence of "hg pull" then "hg up" to update the repos. (Usually
        the additional source repos do not have multiple branches.)

     4. Copy the ldebug/source/cfg.sh file to ovr.sh in the same directory

     5. Edit ovr.sh to point to the repos

     6. In ovr.sh you can also specify which tools to use. For example, the
        variable $NASM specifies the nasm executable to use, with path if
        needed.

     7. Finally, run "./makinst.sh" from the ldebug/source directory.
        You may pass environment variables to it. You may also pass it
        parameters which will be passed to the assembly commands.

    The makinst.sh script expects that the current working directory is
    equal to the directory that it resides in. So you'll always want to run
    it as "./makinst.sh" from that directory.

    ldebug/tmp, ldebug/lst, and ldebug/bin will receive the files created
    by the makinst script. ldebug/bin/instsect.com will be the instsect
    application, which has boot sector loaders for FAT12, FAT16, and
    FAT32 embedded. The default protocol is lDOS and the default kernel
    name LDEBUG.COM. Read the instsect help page for instructions on how
    to use it. Refer to section 14.2 for the instsect help. The help can
    also be obtained by running instsect.com /? from DOS. The kernel
    name can be modified with the /F= switch to instsect. For instance,
    "instsect.com /f=lddebugu.com a:" installs the loader onto drive A: with
    the name set up to load the uncompressed lDDebug.

    Current lDOS boot32 uses the FSIBOOT4 protocol for an additional stage.
    This is interoperable with the upcoming RxDOS version 7.25's use of the
    FSIBOOT4 protocol, as well as with loaders that use a different sector
    for their additional stage (like Microsoft's), or those that do not use
    an additional stage (like FreeDOS's).

3.2.2 How to prepare the test suite

    The test suite (test/test.py) by default uses qemu. (dosemu2 tends to
    need more than 5 seconds to start while qemu manages in 2 seconds or
    less.)

    If the debugger is run as a DOS application and qemu is used then a boot
    image containing a DOS kernel, shell, autoexec.bat, and quit program
    must be created. If the build option use_build_qimg is enabled then
    calls to mak.sh will create such an image. The script file makqimg.sh
    carries out this task.

    If the debugger is run as a DOS application and dosemu2 is used then the
    DOS installed in dosemu is used. The -K and -E switches to dosemu2 are
    used to mount a host directory and execute the debugger.

    If the debugger is bootloaded (in either qemu or dosemu2) then a boot
    image with only the debugger executable and a startup boot script file
    must be created. If the build option use_build_bimg is enabled then
    calls to mak.sh will create such an image. The script file makbimg.sh
    carries out this task.

    The test script creates symlinks to bin/ and tmp/qemutest/ and
    tmp/bdbgtest/ on its own. It can be executed from any directory, as
    it should find its files based on its own location. The test suite
    uses pseudoterminals, qemu or dosemu2, and the default Python unittest
    module.

    Some tests may require having executed the script file
    test/scripts/mak.sh from within the test/scripts directory. When booting
    the debugger or using qemu, this must be run before makbimg.sh or
    makqimg.sh is run.

    The DPMI tests currently require manual setup, with a directory
    test/dpmitest/ containing the dpmitest programs (for dosemu2) or a
    diskette image test/dpmi.img containing the programs as well as the
    HDPMI host executable (for qemu).

3.3 Build options

    _DEBUG

        Make the program debuggable. A "D" is usually prepended to the
        program name. This means that the program's handlers are only
        installed within the function run, and are uninstalled within the
        function intrtn1_code. This allows debugging everything except this
        section. This is intended to be used with a default build of lDebug
        as the outer debugger. However, there is nothing preventing usage of
        a different debugger. To indicate that the debuggable debugger is
        running, its default command prompts are prepended by a tilde "~".

        (To debug everything including the section from run to intrtn1_code,
        or the DPMI entry of lDebugX, a lower-level debugger must be used,
        such as dosemu's dosdebug or other debuggers that are integrated
        into emulators.)

    _DEBUG_COND

        Only takes effect if _DEBUG option is also enabled. Allow to enable
        or disable debuggable mode within the same process. A "C" is usually
        prepended to the program name. To indicate that the debuggable mode
        is enabled, the debugger's default command prompts are prepended by
        a tilde "~".

        The command-line switch /D+ can be used to start up in debuggable
        mode. /D- instead insures to start up in non-debuggable mode. The
        DCO6 flag 100h can be toggled subsequently to toggle debuggable
        mode.

    _PM

        Make the program DPMI-capable. An "X" is usually appended to the
        program name. If possible, the interrupt 2Fh function 1687h is
        hooked and made to return lDebugX's entrypoint. Otherwise, the
        initial entry into protected mode must be traced. Upon entry lDebugX
        will install itself as if it is the actual client, initialise
        itself, then set up the original client as if that had entered
        protected mode. The assembler and disassembler will detect and
        support 32-bit code segments. Other commands will also use 32-bit
        addressing to allow using 32-bit segments. To indicate that the
        debugger is in protected mode, its default command prompt changes
        from the dash "-" to a hash sign "#". (lDDebugX or lCDebugX in
        debuggable mode prepends its tilde to that resulting in "~#".)

    _APPLICATION

        Enabled by default. Enables to use the executable as a DOS
        application. Disabling allows to save a little memory for a special-
        purpose build.

    _DEVICE

        Enabled by default. Enables to use the executable as a DOS device
        driver. Disabling allows to save a little memory for a special-
        purpose build.

    _BOOTLDR

        Makes the program support being bootloaded. This additionally
        requires the lDOS iniload stage wrapped around the MZ .EXE image
        of the debugger. The mak.sh script prepends an "l" to the base
        filename to create the names for the bootable files. For building
        debug, this results in ldebugu.com and ldebug.com. In bootloaded
        mode, I/O is never done using DOS, as if InDOS mode was always on.
        The DOS's current PSP is not switched during debugger operation. The
        MCB chain can only be displayed using the DM command by specifying
        the start segment explicitly. The BOOT commands are supported, refer
        to section 15.11. Disabling allows to save a little memory for a
        special-purpose build.

    _HISTORY

        Enables the line editing history for raw terminal and serial
        input. Defaults to on. Size can be specified using _HISTORY_SIZE.
        Whether a separate segment is used can be controlled using the
        _HISTORY_SEPARATE_FIXED option. Defaults to an 8 KiB separate
        segment buffer.

    _MEMREF_AMOUNT

        Indicates number of memref structures to include. Default 4
        (on). If enabled without a value, the default (4) is selected.
        When enabling this option, you most likely want to first
        rebuild the assembler and disassembler tables using the command
        ./mktables direction stackhinting. (These mktables switches are
        now default enabled.) This allows for memrefs to indicate whether
        an explicit memory operand is a read or write (direction), as well
        as for stack accesses like push, pop, call, retn to be recognised
        in memrefs (stackhinting). Memrefs are initialised by disassembly.
        Memrefs can be accessed using the access variables like READADR0,
        READLEN0, etc. Refer to section 11.18. The access variables are
        written after an R command's register dump and disassembly (refer
        to section 10.35). Access variables can be accessed using special
        keywords behind the IN of a VALUE x IN y construct (refer to section
        9.8).

        Note that memrefs are not always exact. For instance, accesses by
        some instructions are not detected (eg lgdt, sgdt, fsave). Some
        instructions' accesses are not always correctly detected, such as
        enter with non-zero second operand, string instructions spanning
        segment boundaries, or instructions using ss after a write to ss
        that causes disassembly repetition. Some types of accesses are never
        detected either, such as GDT/LDT accesses to load descriptors.
        The stack access of software interrupt instructions is correctly
        detected only when tracing interrupts (Trace Mode set to 1, refer to
        section 10.48); if the interrupt call is proceeded past then like
        any proceeded-past function call it may use more stack space.

    _SYMBOLIC

        Enables the symbolic debugging support. This currently defaults to
        off. Documentation about the symbolic debugging support is still
        lacking. This may require the _DUALCODE build option to be enabled.

    _IMMASM

        Enable the immediate assembler. Refer to section 10.4. This
        currently defaults to off. This may require the _DUALCODE build
        option to be enabled.

    _DUALCODE

        Enable the second code segment of the debugger. Most of the symbolic
        and immediate assembler code will be put into the second code
        segment if it is enabled. Currently defaults to on if both _PM and
        _SYMBOLIC are enabled.

    _BOOTLDR_DISCARD

        Discard boot loaded mode specific code when installing the debugger
        as a DOS application or DOS device driver. This saves about 9 kB of
        resident memory use. Enabled by default.

    _BOOTLDR_DISCARD_HELP

        Discard boot loaded mode ?BOOT help page when installing the
        debugger as a DOS application or DOS device driver. This saves about
        2.7 kB of resident memory use. Enabled by default. Only takes effect
        if option _MESSAGESEGMENT is enabled.

    _MESSAGESEGMENT

        Adds an additional segment for storing long messages like the help
        pages. This moves about 20 kB out of the data entry segment. Enabled
        by default.

    _EXPRDUALCODE

        Moves most code of the expression evaluator into the second code
        segment, if _DUALCODE is also enabled. This moves 5 kB out of
        the first code segment. Performance may suffer from this option.
        Disabled by default.

    _SYMBOLASMDUALCODE

        Moves most code of the symbols.asm file into the second code
        segment, if _DUALCODE is also enabled. Disabled by default.

    _CHECKSECTION

        Sets default value for the following three options. Disabled by
        default.

    _CHECKCALLSECTION

    _CHECKJMPSECTION

    _CHECKJCCSECTION

        These options enable detection of invalid cross-section branches.
        Enabling all of these options makes the build take a long time,
        possibly in excess of two and a half minutes (versus 30 seconds).
        Further, memory use of the assembler may as much as triple easily.
        (166 MiB seen, versus 66 MiB.) The patch for the %rep leak for NASM
        versions beyond 2.16.01 is a must for enabling any of these options.
        These options are not useful if the _DUALCODE option is not enabled.

4: Getting started with the release
-----------------------------------

    The stand-alone and FreeDOS release packages contain the following
    files:

    In the bin or BIN directory:

    ldebugu.com

        Uncompressed bootable debugger, build without DPMI support

    ldebug.com

        Compressed bootable debugger, build without DPMI support

    ldebugxu.com

        Uncompressed bootable debugger, build with DPMI support

    ldebugx.com

        Compressed bootable debugger, build with DPMI support

    instsect.com

        Application to install boot sector loaders, with lDOS loaders that
        default to load LDEBUG.COM from a FAT12, FAT16, or FAT32 file system

    The tmp or SOURCE/LDEBUG/ldebug/tmp directory contains subdirectories
    for each used compression method. For example, there is a subdirectory
    named lz4. These subdirectories contain the compressed executables
    ldebug.com and ldebugx.com built with the corresponding compression
    method.

    NB: The default choice of compression method (LZMA-lzip) is chosen based
    purely on the smallest possible executable size. It may be unsuitable
    for use on low-end systems where it may take several minutes to
    decompress the application. In this case, the uncompressed executables
    may be used, or those compressed with another method (as found in the
    tmp subdirectories).

    In the doc directory, or DOC/LDEBUG:

    ldebug.htm

        This manual in HTML, preferred form

    ldebug.txt

        Manual in plain text (FreeDOS package: with CR LF line endings)

    ldebug.pdf

        Manual in PDF

    fdbuild.txt

        FreeDOS package build instructions

    LDEBUG.LSM

        LSM file for lDebug FreeDOS package

    In the root directory, or also DOC/LDEBUG:

    license.txt

        Full license texts for lDebug

    In the APPINFO directory, only for FreeDOS package:

    LDEBUG.LSM

        LSM file for lDebug FreeDOS package

    In the lst or SOURCE/LDEBUG/ldebug/lst directory:

    debug.lst

        Assembly listing corresponding to ldebug.com and ldebugu.com

    debug.map

        Assembly map corresponding to ldebug.com and ldebugu.com

    debugx.lst

        Assembly listing corresponding to ldebugx.com and ldebugxu.com

    debugx.map

        Assembly map corresponding to ldebugx.com and ldebugxu.com

5: Invoking the debugger
------------------------

5.1 Invoking the debugger in boot loaded mode

    The debugger can be loaded as a variety of kernel formats.

    The Multiboot1 and Multiboot2 entrypoints will expect that a kernel
    command line is provided. The FreeDOS, RxDOS.3, and lDOS load protocols
    allow specifying a kernel command line, but it is optional.

    If a kernel command line is detected then its contents are entered
    into the command line buffer. Unescaped semicolons are translated
    into Carriage Returns. Semicolons and backslashes may be escaped with
    backslashes.

    If no kernel command line is given, the debugger assumes a default. It
    is equivalent to checking for a file and label using the IF command
    (section 10.23), then if found to execute that script file. The IF
    condition is like "if exists y ldp/LDEBUG.SLD :bootstartup then" and the
    subsequent script command is "y ldp/LDEBUG.SLD :bootstartup" (section
    10.56). The filename is however "LDDEBUG.SLD" for DDebug builds, and
    "LCDEBUG.SLD" for CDebug builds.

    Executing the Q command (section 10.32) makes the debugger uninstall
    itself then continue running whatever code the debuggee is in. Executing
    the BOOT QUIT command (section 15.11) makes the debugger attempt to shut
    down the machine. First it will try to call a dosemu-specific callback.
    Next it will attempt shutting down with APM. (This works in qemu.)
    Finally it will give up if no attempt worked.

5.2 Invoking the debugger as an application

    The debugger is internally an MZ .EXE style application. It may need MS-
    DOS version 3 level features. A few switches are supported:

    /?

        Show the command help page about invoking the debugger. Refer to
        section 14.1 for a copy of that help.

    /C

        Put the text following this switch into the command line buffer.
        Unquoted unescaped blanks indicate the end of the text. Parts
        may be quoted using single quote marks or double quote marks.
        Unescaped semicolons are translated into Carriage Returns.
        Semicolons, backslashes, quote marks, and blanks may be escaped with
        backslashes.

    /S

        This switch is only used if the symbolic option is enabled. It can
        be used to set the size of the symbol tables early, before loading a
        debuggee application.

    /B

        Run a breakpoint within the debugger's initialisation.

    /F

        Enable/disable treating file as a flat binary. Enable if a blank
        or plus sign follows this switch. Disable if a minus sign follows
        this switch. This controls the DCO6 option 400h. If enabled, .EXE
        and .COM files will be loaded as flat binaries even if they contain
        an MZ executable header. Writing the files back as flat binaries is
        also enabled by this. (Note that the file has to fit into memory for
        this.) /F implies /E+, but /F+ and /F- do not imply anything about
        /E.

    /E

        Enable/disable setting Stack Segment != PSP for loading flat
        binaries. Enable if a blank or plus sign follows this switch.
        Disable if a minus sign follows this switch. This controls the
        DCO6 option 800h. If enabled then loading a flat binary file (with
        filename extensions such as .bin or using the /F switch) will set up
        a Stack Segment at the end of the process memory block. That is, in
        a different segment than the process segment. If disabled, then flat
        binaries always get SS = PSP even if that leaves the stack pointing
        into the binary image. /F implies /E+.

    /V

        Enable/disable video screen swapping. Enable if a blank or plus sign
        follows this switch. Disable if a minus sign follows this switch.
        Refer to section 10.52.

    After the switches a filename may follow. After the filename, command
    line contents for the process to be debugged may follow. These are both
    passed to the N command. Then, an L command for loading an application
    is run.

    Executing the Q command (section 10.32) makes the debugger try to
    terminate the debuggee application and to then terminate itself. The
    debugger returns to whatever application called it.

    If the TSR command (section 10.49) is used, the debugger patches the
    parent of the currently running application to be the debugger's parent.
    A subsequent Q command will then behave much like it does in boot loaded
    mode: The debugger uninstalls itself and continues execution in the
    current debuggee context.

    The debugger detects its configuration directory as follows:

     1. If the environment variable LDEBUGCONFIG is set, read it.

     2. Else, if the path to the debugger's executable can be determined,
        use that.

     3. Else, the current directory on the current drive is used.

    The command line buffer receives a command that uses the configuration
    directory. This command is written before any /C= switch contents.

    It is equivalent to checking for a file and label
    using the IF command (section 10.23), then if found
    to execute that script file. The IF condition is like
    "if exists y ::config::LDEBUG.SLD :applicationstartup then"
    and the subsequent script command is
    "y ::config::LDEBUG.SLD :applicationstartup" (section 10.56). The
    filename is however "LDDEBUG.SLD" for DDebug builds, and "LCDEBUG.SLD"
    for CDebug builds.

5.3 Invoking the debugger as a device driver

    The debugger's MZ .EXE style executable can also be loaded as a device
    driver. Loading as a device driver requires an MS-DOS version 5 level
    feature. Namely, the loader has to initialise and pass the pointer to
    the end of memory available to the device driver. (The debugger attempts
    to detect whether this pointer is passed and indicates enough memory,
    but it is unclear how well that works.)

    Device drivers can be loaded from CONFIG.SYS using a DEVICE= directive.
    Other loaders such as DEVLOAD may work too. (DEVLOAD 3.25 specifically
    needs a patch to fix some problems keeping track of memory and to allow
    DEVLOAD to report more than 64 KiB of memory available to the device
    driver.)

    DOS device loaders generally convert the device driver's command line
    to allcaps. To work around this, the debugger will interpret the
    exclamation mark in a special way: An exclamation mark indicates to
    convert the next letter to a small letter, if it is a capital letter. To
    pass a literal exclamation mark, double it.

    All command line switches of the application mode are also accepted
    by the device mode debugger. In particular, /C= can be used to pass
    commands to execute. The configuration Script for lDebug file is
    detected in the same way as for application mode, except the label used
    is :devicestartup.

    The debugger will start up with debuggee client registers set up from
    the way they were passed by the device loader. CS:IP will point to
    a far return instruction in the debugger's entry segment. The stack
    will be preserved from what the device loader passed, too. That means
    running the debuggee allows to return control to DOS and have it finish
    installation of the debugger as a device. Subsequently, DOS and other
    device drivers and applications can be debugged, just like when resident
    in TSR mode.

    The device mode debugger can terminate in two different modes. Both
    require a specific command letter appended to the Q command.

    QD may be used if control did not return to the device loader yet. The
    debugger checks this condition by stashing away a copy of all regular
    registers to compare to their current values. This includes all GPRs,
    all segment registers, EIP, and EFL. Also, the debugger's device header
    fields for pointing to the next device header are compared to FFFFh. If
    both match, it is assumed that we can still modify the request header
    passed by the device loader. This allows to report an error and set up
    an empty memory block to keep, so that the loader will know to discard
    the device.

    QC may be used if control has returned to the device loader already and
    the debugger device has been installed into the system. It requires
    locating the device header in the chain of devices that starts with the
    NUL device in the DOS data segment. It also requires to find the memory
    block containing the debugger. It must be either a PSP-alike MCB (self-
    owned regular MCB containing exactly the debugger allocation) or an "SD"
    (System Data) container MCB with one or more sub-MCBs (one of which
    contains exactly the debugger allocation). If these conditions are met,
    the debugger can be quit. It re-uses parts of the TSR application mode
    termination.

    *NOTE:* Using QC currently assumes that no system file handles are left
    allocated to the placeholder character device that the debugger installs
    to keep itself resident. This device is currently called "LDEBUG$$". If
    this rule is not followed the system might crash.

5.4 Invoking the test suite

    Use the test.py script in the test subdirectory. Use the -v switch to do
    verbose output. Specify test name patterns to use with -k, or omit to
    run all tests. The script uses the following environment variables:

    build_name

        Build name to use. Either debug (default), debugx, ddebug, ddebugx,
        cdebug, or cdebugx.

    test_booting

        If set to a nonzero number, boot into the debugger. Otherwise, a DOS
        is loaded and the debugger is run as an application. Some tests are
        booting only, some other tests are non-booting only. The unsupported
        tests are skipped automatically.

    test_initialise_commands

        Commands to be executed by the test set up method right after
        establishing serial I/O. Semicolons are replaced by Carriage
        Returns. This should include the command "r dco6 clr= 100" if
        testing lCDebug to disable its debuggable mode.

    test_sleepduration

        Floating point number which defines the default sleep duration, in
        seconds, for read calls that do not override it. This defaults to
        0.05.

    test_addsleepduration

        Floating point number which defines a duration, in seconds, to add
        to the duration of overridden read calls. This defaults to 0.0.

    DEFAULT_MACHINE

        qemu or dosemu

    DOSEMU

        dosemu executable to use

    QEMU

        qemu executable to use

    DEBUG

        If set to a nonzero number, dump all serial I/O and all debugging
        messages.

    The most common reason for random failures is timing. If this is
    suspected to be the case, the duration variables allow increasing the
    time spent waiting on debugger output. They were added to replace the
    workflow of editing durations manually in the test script.

6: Interface Reference
----------------------

6.1 Interface Output

    The debugger provides a line-based text interface. The interface is
    written to DOS standard output by default. If InDOS mode is entered or
    the debugger is bootloaded then the interface is written to the terminal
    using interrupt 10h. Serial I/O can be enabled to write the interface to
    the serial port.

6.2 Interface Input

    The default command prompt indicates that a command may be entered. It
    is a dash "-" by default, or a hash sign "#" when DebugX is in Protected
    Mode. An exclamation point "!" is prepended by a DOS application
    debugger (not bootloaded) while DOS's InDOS flag is set. A tilde "~" is
    prepended for DDebug, or CDebug while in debuggable mode.

    If DOS command line input is done as raw input (eg if DCO option 800h is
    set) or the input is from a raw (ROM-BIOS) terminal, or from a serial
    port, then the line editing history is enabled. Prior commands may be
    recalled using the Up arrow key. The Down arrow key may also be used
    to reverse the recall. As soon as any prior or new line is edited the
    history recall is disabled.

    Long command output may be paged. In that case, once a screenful has
    been displayed, a "[more]" prompt is displayed to pause the output.
    After pressing any key the output is continued. If Control-C is pressed,
    the current command is aborted.

6.3 Enabling serial I/O

    Refer to section 11.10 for the serial configuration variables. Setting
    the DCO flag 4000h enables serial I/O. Upon enabling serial I/O a
    prompt is sent to the serial port. This prompt looks like the following
    example:

      lDebug connected to serial port. Enter KEEP to confirm.
      =

    (The name of the debugger is modified to indicate DebugX, DDebug,
    DDebugX, CDebug, or CDebugX. The prompt indicator is "~= " for DDebug
    or CDebug while in debuggable mode.) If the keep prompt is successfully
    displayed by the serial terminal and is responded to with the requested
    "KEEP" keyword then serial I/O is established.

    If the confirmation does not occur after a timeout then serial I/O is
    disabled again. The timeout defaults to about 15 seconds. In this case
    the debugger itself clears the DCO flag 4000h.

    If the DCO flag 4000h is cleared then serial I/O is disabled.

6.4 Register dumping

    The R command (refer to section 10.35) without any parameters dumps the
    current register values. Then it disassembles a single instruction,
    or occasionally more than one. The register dump looks like this by
    default:

      -r
      AX=0000 BX=0001 CX=58A0 DX=0000 SP=0800 BP=0000 SI=0000 DI=0000
      DS=1BEC ES=1BEC SS=35A9 CS=1BEC IP=0140 NV UP EI PL ZR NA PE NC
      1BEC:0140 8CC8              mov     ax, cs
      -

    If the "RX" command was used to switch on 32-bit register dumping, then
    the register dump looks like this:

      -r
      EAX=00000000 EBX=00000001 ECX=000058A0 EDX=00000000 ESP=00000800 EBP=00000000
      ESI=00000000 EDI=00000000 NV UP EI PL ZR NA PE NC
      DS=1BEC ES=1BEC SS=35A9 CS=1BEC FS=0000 GS=0000 EIP=00000140
      1BEC:0140 8CC8              mov     ax, cs
      -

    The RE command (section 10.35.1) runs the RE buffer commands. The
    default RE buffer content is a single "@R" command. After running the
    program being debugged, usually the RE buffer commands are also being
    run. This includes a step with the T, TP, or P commands. (Section
    10.47, section 10.47.1, section 10.31.) It also includes a run with
    the G command. (Section 10.19.) Further, a permanent breakpoint which
    is configured as a pass point being passed also runs the RE buffer
    commands. (Section 10.7.)

    Setting the flags 1_0000 or 4_0000 in the DCO3 variable enables register
    change highlighting. When output is written to DOS standard output or
    to a serial port then ANSI escape sequences are used to highlight.
    Specifically, "\x1B[7m" is used to reverse video and then "\x1B[m" to
    reset the colours.

    For DOS standard output it may be needed to install an ANSI escape
    sequence parser.

    For serial I/O the terminal connected to the debugger is expected to
    handle the escape sequences.

    If the output is to a terminal using interrupt 10h and DCO3 flag 2_0000
    is clear and the terminal is detected as functional then highlighting is
    done using interrupt 10h video attributes.

    The functionality check is done by calling interrupt 10h service 03h. If
    the indicated current column is nonzero then the terminal is considered
    functional. (Current dosemu2 in -dumb terminal mode is detected as not
    being functional.)

    If this check fails or the DCO3 flag 2_0000 is set then escape sequences
    are written using interrupt 10h.

6.5 Memory dumping

    Another basic command is the D command (section 10.11). It is used to
    dump memory contents. For example, to dump part of a program:

      -d
      1BEC:0140  8C C8 31 DB 05 70 14 50-53 CB 70 03 91 67 BC 45 ..1..p.PS.p..g.E
      1BEC:0150  3F 10 C1 6F F9 70 BA 22-7C 71 C3 72 0A 81 0A 81 ?..o.p."|q.r....
      1BEC:0160  47 74 68 76 6C 77 32 72-A7 2F BD 78 4B 16 9F 7B Gthvlw2r./.xK..{
      1BEC:0170  C9 2B 09 37 0A 81 81 7D-E2 7E AC A0 00 00 00 00 .+.7...}.~......
      1BEC:0180  10 49 00 00 0F 00 00 00-00 00 00 00 10 49 00 00 .I...........I..
      1BEC:0190  0F 00 00 00 F8 30 80 00-00 00 00 00 80 00 00 00 .....0..........
      1BEC:01A0  07 00 00 00 07 00 00 00-00 00 00 00 00 00 00 00 ................
      1BEC:01B0  00 00 00 00 97 65 00 00-00 00 00 00 00 00 00 00 .....e..........
      -

    Or, to dump the stack as words:

      -dw ss:sp
      header     0    2    4    6    8    A    C    E    0123456789ABCDEF
      35A9:0800  0000 0000 0000 0000-0000 0000 0000 0000 ................
      35A9:0810  0000 0000 0000 0000-0000 0000 0000 0000 ................
      35A9:0820  0000 0000 0000 0000-0000 0000 0000 0000 ................
      35A9:0830  0000 0000 0000 0000-0000 0000 0000 0000 ................
      35A9:0840  0000 0000 0000 0000-0000 0000 0000 0000 ................
      35A9:0850  0000 0000 0000 0000-0000 0000 0000 0000 ................
      35A9:0860  0000 0000 0000 0000-0000 0000 0000 0000 ................
      35A9:0870  0000 0000 0000 0000-0000 0000 0000 0000 ................
      -

6.6 Disassembly

    The U command is used to disassemble one or several instructions.
    Example:

      -u
      305C:0000 8CD0              mov     ax, ss
      305C:0002 8CDA              mov     dx, ds
      305C:0004 29D0              sub     ax, dx
      305C:0006 31D2              xor     dx, dx
      305C:0008 B90400            mov     cx, 0004
      305C:000B D1E0              shl     ax, 1
      305C:000D D1D2              rcl     dx, 1
      305C:000F E2FA              loop    000B
      305C:0011 50                push    ax
      305C:0012 01E0              add     ax, sp
      305C:0014 83D200            adc     dx, +00
      305C:0017 83C00F            add     ax, +0F
      305C:001A 83D200            adc     dx, +00
      305C:001D 24F0              and     al, F0
      305C:001F 83FA01            cmp     dx, +01
      -

6.7 Loading the debuggee

    A program to examine can be loaded using the N and L commands. If the
    debugger is loaded as a DOS application with a filename specified in its
    command line, it will run the N and L commands on its own.

    The N command sets up some buffers internal to the debugger. One of
    those specifies the pathname of the executable file to load. The
    pathname must include the filename extension, if any. The pathname must
    be relative to the current directories at the time the L command runs,
    or it must be absolute. The tail of the N command after the pathname is
    used as the command line tail for a new debuggee process.

    The L command without any parameters attempts to load the program
    specified to the last N command into a new process. If the L command
    does not display any messages this indicates success.

6.8 Running the debuggee

    Once a program is loaded into the debugger it can be run in several
    ways:

    G command

        Runs at full speed until a breakpoint is encountered. Temporary
        breakpoints can be specified to the G command. Refer to section
        10.19.

    T command

        Traces a single instruction, except for software interrupts which
        are by default run at full speed with a breakpoint after them. Refer
        to section 10.47.

    P command

        Either runs at full speed with a breakpoint behind the current
        instruction, or traces a single instruction. Software interrupts,
        call instructions, repeated string instructions, and loop
        instructions are proceeded past by using a breakpoint. Refer to
        section 10.31.

    TP command

        Like the T command except that repeated string instructions are
        proceeded past like the P command would. Refer to section 10.47.1.

    All run commands support auto-repeat: Submitting an empty line to the
    debugger (blanks allowed but no comment) will make the debugger run
    the last command again. For the G command auto-repeat, the specified
    temporary breakpoints will be used again. Refer to section 10.1.

    Permanent breakpoints can be set up and changed using the B commands.
    They can be configured to behave as pass points as well. Refer to
    section 10.7.

    The ?RUN help page in section 15.8 lists some additional features of the
    T, P, and TP commands.

6.9 Help

    The online help can be accessed using the "?" command. Refer to section
    15 for copies of the online help.

7: Debugging the debugger itself
--------------------------------

    There are debuggable builds of the debugger, called lDDebug
    (unconditionally debuggable) and lCDebug (conditionally debuggable).

    The debuggable mode works by installing the mandatory interrupt handlers
    of the debuggable debugger only within the "run" function, so as to
    return the control flow to this instance when it runs its debuggee code.
    On return into this instance, it uninstalls its mandatory handlers
    again. This mechanism allows to debug most of the debugger using a
    different instance of lDebug (or potentially another debugger).

    In debuggable mode, an additional command is supported, the BU command
    (which stands for "Break Upwards"). It will run a breakpoint within the
    debugger's code segment which will break into the other debugger. Its
    code was updated so it will break at the command dispatcher after the
    label cmd4. This means if the outer debugger is also an lDebug then
    it can be instructed to skip to the next command being dispatched by
    entering the command "G ip".

    lDDebugX (or lCDebugX) can also install its exception areas into the
    other lDebugX instance. For this, the other debugger needs to have run
    an "INSTALL AMIS" command. Then the debuggable debugger can run its
    "INSTALL AREAS". Afterwards, faults in the debuggable debugger will make
    the other lDebugX indicate the area of the fault.

    After lDebugX has caught a fault in the CODE or CODE2 segment, it
    can be instructed to resume the lDDebugX (or lCDebugX) command input
    loop (cmd3) by running a "G=0" command. If "G=1" is used instead, an
    additional linebreak will be displayed by the debuggable debugger before
    it starts prompting for input. This is useful if the fault occurred
    with some partial output currently displayed. The offset 0 and offset 1
    entries are also supported by non-DPMI builds and can of course be used
    at any point in time other than after a fault, too.

    There are some DCO6 flags to control breakpoints and entering lCDebug's
    debuggable mode in the functions debuggerexception and putrunint. They
    can be displayed using a "?O6" command.

    Other than for the most trivial sessions it is recommended to control
    the outer debugger by serial I/O, separately from the I/O of the
    debuggable debugger. If the latter also should be controlled by serial
    I/O then two different ports can be used. The terminal connected to the
    outer debugger can also be set up for TracList, the lDebug companion
    application which traces a listing file. For instance, if lDDebugX is
    to be traced, TracList should be run with the ldebug/lst/ddebugx.lst
    listing file.

7.1 Initialising the debuggable debugger

    To allow the debuggable debugger to relocate and initialise its code
    sections, the outer debugger should generally start running the
    debuggable debugger with a plain "G" command. The debuggable debugger
    can then return control to the outer debugger using its "BU" command.

    If the initialisation of the debuggable debugger is to be debugged, the
    "/B" switch may be of use. Otherwise, note that the NEC V20/V30 and 486
    CPU detections may fail when traced using an outer lDebug.

    The NEC detection may lock the machine up if its specially encoded
    "pop cx" is traced or run with a breakpoint directly behind it. To allow
    to continue tracing after it, a breakpoint must be set up at the "jcxz"
    instruction or later. There must not be a breakpoint on the "mov sp, ax"
    instruction. The "pop cx" instruction must not be traced with the Trace
    Flag set. Failure to honour these requirements may lock up the NEC
    CPUs, for example the one used in the HP 95LX, which then may require
    resetting the system with Ctrl-Shift-On. This also resets the system
    date and time.

    The 486 detection may wrongly detect a 386 instead of a 486+ when traced
    on some systems, such as some revisions of dosemu(2).

8: Parameter Reference
----------------------

8.1 Number

    Plain numbers are evaluated as expressions. Refer to section 9.
    Expressions consist of any number of the following:

     -  Unary operators

     -  Binary operators

     -  Operands

    Plain number parsing for an expression continues for as long as a valid
    expression is continued. For example, in the command "D 100 + 20 L 10"
    the starting address (its offset to be specific) is calculated as "100
    + 20". Then the expression evaluator encounters the "L", which is not a
    valid binary operator. Plain number expression parameters are used by a
    lot of commands. Sometimes, the plain number parameter type is called
    "count" or "value".

8.2 Address

    An address parameter is calculated with a default segment. First, a
    plain number is parsed. If it is followed by a colon, the first number
    is taken as segment, and then another number is parsed for the offset.
    If the first number is specified as a pointer type using the type
    keyword "POINTER" then its upper 16 bits are taken as segment and its
    lower 16 bits are taken as the offset. Otherwise, the first number is
    used as the offset. Offsets may be 16 bits or 32 bits wide, though 32-
    bit offsets are only valid for DebugX and only in 32-bit segments.

    If a segment or pointer type expression are prefixed by a dollar sign
    "$" then the specified segment is always taken as a Real/Virtual 86 Mode
    segment, even if DebugX is in Protected Mode. Otherwise, in Protected
    Mode a segmented address refers to a selector.

    Instead of an address, the address parameter may consist of the taken
    keywords: TAKEN or T for taken, and NOTTAKEN or NT for not taken. This
    is only valid if the current cs:(e)ip points at a conditional branch
    instruction, and will cause a parsing error otherwise. The taken
    keywords will evaluate to a segmented address pointing at the target
    of the conditional branch. The not taken keywords will evaluate to a
    segmented address pointing to behind the conditional branch instruction.

    Address parameters are used by a lot of commands.

8.3 Range

    A range parameter may have a default length, or it may be disallowed to
    omit a length. Parsing a range starts with parsing an address. Then,
    if the end of the line is not yet reached, an end for the range may be
    specified. The end may be a plain number, which is taken as the offset
    of the last byte to include in the range. The address of the last byte
    to include must be equal or above the address of the first byte that is
    included in the range.

    The end may instead be specified with an "L" or "LENGTH" keyword. In
    that case, the keyword is followed by a plain number and an optional
    item size keyword. A length of zero is not valid. The item size keyword
    may be "BYTES", "WORDS", "DWORDS", or "PARAS". For the latter three, the
    plain number will be multiplied by 2 or 4 or 16. The "BYTES" keyword is
    only provided for symmetry; currently all commands taking ranges default
    to byte size for the "LENGTH" number.

    For example, the command "DD 100 LENGTH 4 DWORDS" will dump memory from
    address 0100h (in the current data segment) in dword units, for a length
    of 4*4 = 16 bytes. The item size keywords were introduced primarily for
    the "DW" and "DD" commands (refer to section 10.11), but they can be
    used for any command that accepts a range.

    There is a new keyword called "END". This keyword may appear where the
    "L" or "LENGTH" keyword would be expected. After the "END" keyword the
    end offset is parsed. This is the same behaviour as if no keyword was
    present but crucially it allows an end offset starting with the text
    "L", which would otherwise be misparsed as an "L" keyword.

    Range parameters are used by a lot of commands.

8.4 Range with LINES keyword allowed

    This type of parameter is an extension of the range parameter type. Both
    the default length and the explicit length may be specified as a number
    of lines instead of an address length.

    An explicit "LINES" length is specified by prepending an "L" or "LENGTH"
    keyword (like an address length) but then specifying a unit as "LINES"
    instead. The number of lines specified must be nonzero and below 8000h.

    The exact details of how a lines length is used depend on the command
    in question. A range with lines length is allowed for the U command
    (section 10.50) and the D/DB/DW/DD commands (section 10.11).

8.5 List

    A list is made up of a sequence of items. Each item is either a plain
    number or a quoted string. List parsing continues until the end of
    the line. Each plain number represents a single byte. Quoted strings
    represent as many bytes as there are quoted. A quoted string can be
    delimited by single quotes ' or double quotes ". If the used delimiter
    quote mark occurs twice back to back while reading the quoted string,
    this is taken as an escape to include the delimiter mark itself as
    a byte of the string. List parameters are used by the E, F, and S
    commands. Refer to section 10.17, section 10.18, and section 10.45.

    A list may start with an AS keyword, followed by a size keyword WORDS
    or DWORDS. In this case, each number expression and each byte of quoted
    text are written to a full word or a full dword instead of to a byte.
    Text bytes are zero-extended. Numbers can calculate to any value fitting
    the specified size.

8.6 List or range

    A list or range can be specified for this parameter. The range is
    identified by a leading "RANGE" keyword. Otherwise, a list is parsed.
    A list or range parameter is as yet used by the S command and the F
    command, refer to section 10.45 and section 10.18.

8.7 Keyword

    A keyword is checked insensitive to capitalisation. Keywords depend on
    each command. Only the keywords used to specify a range's length are
    shared by all commands that parse ranges.

8.8 Index

    An index is a plain number that specifies a breakpoint index. It allows
    operating on one specific breakpoint. The index parameter type is used
    by the B commands, refer to section 10.7.

8.9 Segment

    A segment is a plain number for parsing purposes. The segment parameter
    type is used by the DM command and some BOOT commands, refer to section
    10.13 and section 15.11.

8.10 Breakpoint

    Each breakpoint is a single address, which defaults to the code
    segment. The address may instead be specified starting with an AT sign
    "@", followed by a blank or an opening parenthesis. In that case, the
    following plain number specifies the non-segmented linear address to
    use. The breakpoint parameter type is used by the B and G commands,
    refer to section 10.7 and section 10.19.

8.11 Label

    A label is a (not quoted) string keyword. It may start with an optional
    colon. A label can be used by the GOTO and Y commands, refer to section
    10.20 and section 10.56.

8.12 Port

    A port is a plain number for parsing purposes. The port parameter type
    is used by the I and O commands, refer to section 10.22 and section
    10.30.

8.13 Drive

    A drive may be either an alphabetic letter followed by a colon, or a
    plain number. The number zero corresponds to drive A: then. The drive
    parameter type is used by the L and W sector commands, refer to section
    10.26 and section 10.54. The N and Y commands (section 10.29 and
    section 10.56) also accept drive parameters, but only as part of their
    filenames. These must be in the drive letter followed by colon format.

8.14 Sector

    A sector is a plain number, which can be equal to any 32-bit value. The
    sector parameter type is used by the L and W sector commands, refer to
    section 10.26 and section 10.54. Some BOOT commands also use sector
    numbers, refer to section 15.11.

8.15 Condition

    A condition is a plain number. It is evaluated either to nonzero
    (true) or zero (false). The condition parameter type is used by the IF
    command, as well as the P, TP, and T commands when specified with a
    "WHILE" keyword. The BW and BP (with a "WHEN" keyword) commands also
    use conditions. Refer to section 10.23, section 10.31, section 10.47,
    section 10.7.3, section 10.7.1. The length of a condition for B commands
    is limited by how much space is left in the permanent breakpoint
    conditions buffer. This buffer currently defaults to 1024 bytes. It is
    shared for all conditions of all permanent breakpoints.

8.16 Register

    A register specifies an internal variable of the debugger. Most
    prominently these include the debuggee's registers as stored by the
    debugger in its data segment. A register or variable may be an operand
    in a plain number's expression. However, several forms of the R command
    also use register parameters. These allow reading and writing the
    register values. Refer to section 10.35.

8.17 Command

    Command is a special parameter type that is used only by the RE.APPEND,
    RE.REPLACE, RC.APPEND, and RC.REPLACE commands (section 10.35.2 and
    section 10.35.4). It is read verbatim and entered into the RE or RC
    command buffer. Semicolons within a command parameter are not parsed
    as end of line comment markers. Instead, they are converted to CR (13)
    codes in the buffer. This delimits the parts of the parameter into
    several commands. A semicolon may be prefixed by a backslash to escape
    it and thus enter a literal semicolon into the buffer.

8.18 ID

    ID is a special parameter type that is used only by the BP and BI
    commands (section 10.7.1 and section 10.7.2). Leading and trailing
    whitespace is ignored. An ID can be empty, or contain up to 63 bytes of
    data. The length of an ID is also limited by how much space is left in
    the permanent breakpoint ID buffer. This buffer currently defaults to
    384 bytes. It is shared for all IDs of all permanent breakpoints.

9: Expression Reference
-----------------------

9.1 Literals

    Literals consist of one or more digits. A literal must start with a
    digit or hash sign "#". Embedded underscores "_" are skipped. Literals
    must not overflow 4 giga binary minus 1, that is FFFF_FFFFh.

    The default base for literals is sixteen (hexadecimal). A hash sign "#"
    indicates a base change. If nothing preceeds the hash sign the base is
    changed to ten (decimal). Otherwise, the number before the hash sign
    is read in the prior base and taken as the base to change to. The base
    must be between 2 and 36. Multiple hash signs are allowed in the same
    literal.

9.2 String literals

    String literals consist of up to 4 bytes. The bytes are specified
    starting with a hash sign "#" followed by a single-quote mark ' or
    double-quote mark ". The same quote mark is used to end the string
    literal. If the delimiter quote mark occurs twice back to back while
    reading the string literal, that is handled as an escape to include the
    delimiter mark itself as a byte. Strings are read in a little-endian
    order, same as NASM does. That is, the first byte of a multi-byte string
    is read into the lowest byte of the numeric value. This matches the
    order obtained by writing the string to memory and reading it as a word,
    3byte, or dword.

9.3 Variables

    A variable consists of a variable name, possibly followed by parentheses
    with an index expression. Variable names are capitalisation insensitive.
    Variables differ in size, there are variables consisting of 8, 16,
    24, or 32 bits. Variables can be written to using the R command. Some
    variables are read-only. A few variables allow writing some but not all
    bits.

9.4 Indirection

    Indirection is indicated by square brackets. Within the brackets an
    address is parsed, defaulting to ds as the segment. The size of the
    indirect access can be specified with a type specifier before the
    brackets. The usual types are BYTE, WORD, 3BYTE, and DWORD. Like
    variables, indirection terms can be written to using the R command.

9.5 Parentheses

    Parentheses can be used to force a different order of operations.

9.6 LINEAR keyword

    A keyword reading LINEAR introduces an address to parse. The address
    defaults to ds as the segment. The address may be separated from
    subsequent text with a comma. If the expression is to be separated from
    a subsequent element using a comma after a LINEAR address then two
    commas are needed. Depending on the segmentation scheme of the current
    mode the segmented address is converted into a linear address. If DebugX
    is in Protected Mode and the segment base cannot be determined the
    expression is rejected as an error.

9.7 DESCTYPE keyword

    This keyword introduces a descriptor type read. The following expression
    is taken to be a selector specification. This keyword is only valid for
    (DPMI-enabled) lDebugX builds, and only while in Protected Mode.

    The value is read from a "lar" instruction on the following expression,
    and shifted to the right by 8. If the instruction indicates that the
    selector does not refer to a valid descriptor then the result of this
    keyword is zero.

9.8 VALUE IN construct

    A keyword reading VALUE starts a VALUE IN construct. Between
    the VALUE and subsequent IN keyword there is a single value
    expression, or a range of the form FROM expression TO expression or
    FROM expression LENGTH expression. Next follows the IN keyword. After
    this, there is a list of match ranges. A match range is either a single
    value expression, or a range of the form FROM expression TO expression
    or FROM expression LENGTH expression. After each match range a comma
    indicates another match range follows.

    In a FROM TO specification the first expression has to evaluate to
    unsigned below-or-equal the second expression. In a FROM LENGTH
    specification the length must be nonzero. If these conditions are not
    met then the value or match range in question is always considered as
    not matching.

    The entire VALUE IN construct evaluates to how many of the match ranges
    match the value range. The construct only evaluates to zero if no
    matches occurred. A nonzero value indicates that at least one match
    occurred.

9.8.1 VALUE IN construct keywords

    Instead of a value or match range as specified here, the keyword
    EXECUTING may be specified. This expands to the following input:

      FROM LINEAR cs:cip LENGTH abo - cip

    If the _MEMREF_AMOUNT build option is enabled and paired with the
    direction and stackhinting switches to mktables then additional keywords
    are available for VALUE IN match ranges. That is, these keywords must be
    specified behind the IN and cannot be specified between the VALUE and
    IN.

    These keywords are as follows:

    READING

        Expands to a comma-separated list of FROM readadr0 LENGTH readlen0
        constructs, for every read access variable pair (refer to section
        11.18).

    WRITING

        Expands to a comma-separated list of FROM writadr0 LENGTH writlen0
        constructs, for every write access variable pair (refer to section
        11.18).

    ACCESSING

        Expands to READING, WRITING, EXECUTING.

9.9 Conditional ?? :: construct

    The ternary conditional operator takes three operands. It is the only
    ternary operator.

    The first operand, the condition, is specified before the ?? keyword.
    Note that the ?? keyword must be terminated by a blank or an opening
    square bracket or round parenthesis.

    The second operand is specified between the ?? keyword and the ::
    keyword. Its value is used as the construct's return value if the
    condition is true.

    The third operand is specified after the :: keyword. Its value is used
    as the construct's return value if the condition is false.

    The conditional operator can be nested freely. The conditional operator
    must not be combined into the R command's assignment operator as in
    ??:=. The third operand may be separated from subsequent text with a
    comma. If the expression is to be separated from a subsequent element
    using a comma after a conditional's third operand then two commas are
    needed.

    Any side effects that may happen from parsing and reading the second
    operand or the third operand will always happen, even if the operand in
    question is not selected as the result by the construct.

9.10 Expression side effects

    Some uses of the expression evaluator may have side effects. These side
    effects may happen even if the parsing of an expression or a command
    ultimately fails. As a special case, side effects may occur up to twice
    if a machine mode command (section 10.28) is parsed.

    The ternary ?? :: operator and the VALUE IN construct will both always
    evaluate every operand that they're given, even if that operand is not
    selected as the result or does not contribute to the match count.

    Possible side effects include:

     -  LFSR and RLFSR variables will be stepped once each time they're
        read.

     -  Indirection can read access arbitrary memory in the current mode,
        making it possible to affect memory-mapped I/O if such memory is
        visible to the debugger. Other variables may also read memory, but
        not as arbitrary as indirection.

     -  If an address parsed within an address parameter or in indirection
        or in a LINEAR construct includes a dollar sign prefixed segment or
        pointer type expression, then lDebugX may request a selector from
        the DPMI host.

     -  If the symbolic build option is enabled, symbol table access in XMS
        or 86 Mode memory may occur.

10: Command Reference
---------------------

10.1 Empty command - Autorepeat

    Entering an empty command at an interactive prompt results in
    autorepeat. Empty means no content except for blanks. A line starting
    with a semicolon comment is not considered empty. Interactive prompts
    for this purpose include:

     -  the debugger as a DOS application (int 21h)

     -  the debugger in InDOS mode or as a bootloaded program
        (int 16h/int 10h)

     -  the debugger across a serial port (port I/O)

    Input that does not count as an interactive prompt includes:

     -  reading from a file redirected as stdin using DOS (int 21h)

     -  reading from a Y script file using DOS (int 21h)

     -  reading from a Y script file while bootloaded (int 13h)

     -  reading from the command line buffer

     -  reading from the RE buffer

    Autorepeat is not supported by all commands. The following commands
    support autorepeat:

    D/DB/DW/DD

        Continues memory dump behind the last prior dumped position.
        Continues with the same element size as the prior dump. As for
        if the command is executed with an address lacking a length, the
        default length is used. (It defaults to 128 bytes, refer to section
        11.5.)

    DZ/D$/D#/DW#

        Continues string dump behind the last prior dumped string. Continues
        with the same type of string as the prior dump.

    DX

        Continues memory dump.

    G

        Repeats a step running the debuggee. An equals address given to the
        prior Go command is not used again. The same G breakpoints as used
        by the prior Go command are used (same as G AGAIN). The exception is
        that wherever a breakpoint matches the CS:(E)IP at the start of the
        command's execution, it is skipped once.

    P

        Repeats a step running the debuggee. An equals address given to the
        prior Proceed command is not used again. A count given to the prior
        Proceed command is not used again, autorepeat always runs as if not
        given a count. (That means the PPC variable is used as the effective
        count. Refer to section 11.4.)

    T

        Repeats a step running the debuggee. An equals address given to the
        prior Trace command is not used again. A count given to the prior
        Trace command is not used again, autorepeat always runs as if not
        given a count. (That means the TTC variable is used as the effective
        count. Refer to section 11.4.)

    TP

        Repeats a step running the debuggee. An equals address given to the
        prior Trace/Proceed command is not used again. A count given to the
        prior Trace/Proceed command is not used again, autorepeat always
        runs as if not given a count. (That means the TPC variable is used
        as the effective count. Refer to section 11.4.)

    U

        Repeats disassembly behind the last prior disassembled instruction.
        As for if the command is executed with an address lacking a length,
        the default length is used. (It defaults to 32 bytes, refer to
        section 11.5.)

10.2 ? command

      Online help    ?

    The question mark command (?) lists the main online help screen.

    There are additional help topics that can be listed by using the
    question mark command with an additional letter or keyword. These
    keywords are as follows:

      Registers      ?R
      Flags          ?F
      Conditionals   ?C
      Expressions    ?E
      Variables      ?V
      R Extended     ?RE
      Run keywords   ?RUN
      Options pages  ?OPTIONS
      Options        ?O
      Boot loading   ?BOOT
      lDebug build   ?BUILD
      lDebug build   ?B
      lDebug sources ?SOURCE
      lDebug license ?L

    The full help pages are listed in section 15.

10.3 : prefix - GOTO label

    A leading colon indicates a destination label for GOTO, see section
    10.20.

10.4 . (dot) command - Immediate assembler

    A dot command can be used to invoke the immediate assembler. This is
    only available if the _IMMASM build option was enabled. Following the
    dot, an instruction is parsed which is assembled. If successful, then
    the assembled instruction is immediately run.

    Branches and instructions involving CS as a prefix or operand are
    handled specifically to do something equivalent to the assembled
    instruction, by a combination of special detection and modification
    or as-if handling. This includes jmp far/near/short, jcc, loop, call
    far/near, retf/retn/iret, mov to ds, mov from ds or cs, push cs,
    push ds, pop ds, lds, and all memory operands with cs prefix. (The
    instructions involving ds are handled specifically because a cs prefix
    is replaced by a ds prefix and ds is temporarily replaced by the cs
    value then.)

    Interrupt calls are always proceeded past, even if TM is set. The int
    instruction is run from a buffer internal to the debugger. Interrrupts
    which depend on the CS or (E)IP they're called from may not work as
    expected. Calls are usually traced, but can be proceeded past by
    including a comma after the dot command.

    Warning: It is generally not safe to modify SS or SP to relocate the
    stack with the immediate assembler. This will fail because the immediate
    assembler traces most of the instructions assembled with it, which uses
    the stack both before and after running the instruction. LSS SP or LSS
    ESP are okay if the stack is valid immediately after the instruction is
    traced. To relocate the stack otherwise you may use the R command to
    modify the SS and (E)SP debugger variables. This does not trace anything
    in between modifying the two variables.

10.5 A command - Assemble

      assemble        A [address]

    Starts assembly at the indicated address (which defaults to CS segment),
    or if no address is specified, at the "a_addr" (AAS:AAO variables).

    Assembly mode has its own prompt. Entering a single dot (.) or an empty
    line terminates assembly mode. Comments can be given with a prefixed
    semicolon. In assembly mode, whereever an immediate number occurs an
    expression can be given surrounded by parentheses ( and ). In such
    expressions, register names like AX are evaluated to the values held by
    the registers at assembly time. To refer to a register as an assembly
    operand, it must occur outside parentheses.

10.6 ATTACH command - Attach to process (Leave TSR mode)

      attach process  ATTACH psp

    While in resident mode, the ATTACH command can be used to attach the
    debugger to a process. This is the opposite operation to the TSR command
    (see section 10.49). The device driver mode starts out as detached while
    the application mode starts out as attached.

    The provided parameter must be a segment value, even if lDebugX is in
    Protected Mode. It refers to the PSP to attach to. This PSP must not be
    self-owned.

    To attach to a process, the debugger stores away the current PRA and
    parent of the process, and modifies both to point to the debugger
    instead.

    When attached to a process, commands like QA and the process-loading L
    command can be used sensibly. The Q command will also try to terminate
    the attached process.

    When detached, the Q command will continue to run the current debuggee
    context after the debugger has been uninstalled.

    The usual parameter to the attach command consists of the "PSP"
    variable, which will have the command try to attach to the current
    debuggee process. Other choices like ATTACH PARENT are also valid.

10.7 B commands - Permanent breakpoints

    There are a fixed number of permanent breakpoints provided by the
    debugger. The default is to provide 16 permanent breakpoints. They are
    specified by indices ranging from 00 to 0F. A breakpoint can be unused,
    used while enabled, or used while disabled. A breakpoint that is in use
    has a specific linear address. It is allowed, though not advised, for
    several breakpoints to be set to the same address.

    When running the debuggee with the commands G, T, TP, or P, hitting a
    permanent breakpoint stops execution, and indicates in a message "Hit
    permanent breakpoint XX" where XX is replaced by the hexadecimal byte
    index of the breakpoint. If the breakpoint counter is not equal to 8000h
    when the breakpoint is hit, then the "Hit" message is followed by a
    "counter=YYYY" indicator. If the breakpoint ID is not empty, then the ID
    is shown with an "ID: " prefix. The ID is shown either on the same line
    as the "Hit" message, or on the next line if the ID exceeds 28 bytes.
    After that message a register dump occurs, same as for default breaking
    for the Run commands.

    The exceptions are as follows:

     -  If the CS:(E)IP at the first step of a G command matches any
        breakpoints, then G does a TP-like step with all breakpoints other
        than the "cseip"-breakpoint written, while the "cseip"-breakpoint
        is not written. After that, the "cseip"-breakpoint is written and
        execution resumes as normal for G.

     -  If T.NB or TP.NB or P.NB is used, no permanent breakpoints are
        written at all.

     -  If T.SB or TP.SB or P.SB is used, then during the first step no
        permanent breakpoints are written. If a counter higher than 1 is
        given, then during subsequent steps permanent breakpoints are
        written.

    Each breakpoint has a breakpoint counter, which defaults to 8000h if not
    set explicitly by the BP or BN commands. The breakpoint counter behaves
    as follows:

     -  If (counter & 3FFFh) equals zero then the counter is considered to
        be at a terminal state.

     -  If the point breaks while the counter is not at a terminal state,
        then the counter is decremented.

     -  If the counter is decremented to 0 or 4000h, then the point is hit.

     -  If the counter is decremented to 8000h or C000h, or was already at
        either count without being decremented, then the point is hit.

     -  If the point is not hit but the bit (counter & 4000h) is set, then
        the point is passed.

    Example counter values:

    8000h (default)

        Always break

    4000h

        Always pass

    8003h

        Break on third time the breakpoint is reached, then break always

    0003h

        Break on third time the breakpoint is reached, but do not break
        again

    C006h

        Pass for five times, then on the sixth time the breakpoint is
        reached break on it, then break always

    The point being passed means that during running the debuggee with a
    Run command, execution is not stopped, but a message indicating "Passed
    permanent breakpoint XX, counter=YYYY" is displayed. As for the "Hit"
    message the ID, if any, is also shown. After that message, a register
    dump occurs. Then execution is continued in accordance with the command
    that is running debuggee code.

    Each breakpoint can have a breakpoint condition. If the condition
    expression evaluates to false when the point breaks, then the point is
    not considered hit or passed. The breakpoint counter is not stepped then
    either.

10.7.1 BP command - Set breakpoint

      set breakpoint  BP index|AT|NEW address
                        [[NUMBER=]number] [WHEN=cond] [ID=id]

    BP initialises the breakpoint with the given index. It must be a yet
    unused breakpoint. If the index is specified as the keyword NEW, the
    lowest unused breakpoint (if any) is selected. If there is the keyword
    AT instead of an index or a keyword NEW, then an existing breakpoint
    at the same linear address is reset, or a new one is added (same as if
    given the NEW keyword).

    The address can be given in a segmented format, which defaults to
    CS, and which in DebugX is subject to either PM or 86M segmentation
    semantics depending on which mode the debugger is in. The address can
    also be given with an @ specifier (followed by an opening parenthesis or
    whitespace) in which case it is specified as the 32-bit linear address.
    Debug without DPMI support limits breakpoints to 24-bit addresses, of
    which 21 bits are usable.

    The optional number, which defaults to 8000h, sets the breakpoint
    counter to that number.

    The optional WHEN keyword introduces a breakpoint condition. If the
    breakpoint is reached then the condition, if specified, is checked
    before stepping the counters. If the condition is false at that point
    the point is not considered hit or passed and its counter is not
    stepped.

    There is an optional OFFSET keyword (not shown in the example) which
    allows overriding the breakpoint's preferred offset. Refer to section
    10.7.4 for details.

    The optional ID keyword allows setting the breakpoint ID. The ID is
    displayed by BL and when a breakpoint is hit or passed. The default ID
    is an empty ID. Note that the ID extends for the remainder of the line.
    There cannot be a breakpoint counter number nor WHEN condition nor
    OFFSET after the ID keyword.

10.7.2 BI command - Set breakpoint ID

       set ID         BI index|AT address [ID=]id

    BI sets the breakpoint ID of the specified breakpoint. The ID is
    displayed by BL and when a breakpoint is hit or passed. The ID may be
    specified as empty.

10.7.3 BW command - Set breakpoint condition

       set condition  BW index|AT address [WHEN=]cond

    The BW command sets the breakpoint condition. If the WHEN keyword and
    the condition are absent then the condition is reset. That means the
    point is no longer conditional.

10.7.4 BO command - Set breakpoint preferred offset

       set offset     BO index|AT address [OFFSET=]number

    The BO command sets the breakpoint preferred offset. The preferred
    offset is used only by the BL command. It is used to determine the
    segmented address to display. The offset is a word variable for Debug
    and a dword variable for DebugX. If the OFFSET keyword and the number
    are absent then the offset is disabled, as if the breakpoint was
    specified with a linear address. (Internally this is done by setting the
    offset to all 1 bits. The offset can be explicitly set to FFFFh (Debug)
    or FFFF_FFFFh (DebugX) for the same effect.)

10.7.5 BN command - Set breakpoint number

       set number     BN index|AT address|ALL number

    BN sets the breakpoint counter of the specified breakpoint with the
    given index, or all used breakpoints when given the keyword ALL, or
    the first breakpoint with a matching linear address when given the AT
    keyword. The number defaults to 8000h.

10.7.6 BC command - Clear breakpoint

       clear          BC index|AT address|ALL

    BC clears the specified breakpoint with the given index, or all
    breakpoints when given the keyword ALL, or the first breakpoint with
    a matching linear address when given the AT keyword. This returns
    the specified breakpoint (or all of them) to the unused state. Any
    associated ID or condition is deleted by BC too.

10.7.7 BD command - Disable breakpoint

       disable        BD index|AT address|ALL

    Given an index or the keyword ALL or the keyword AT (like BC), BD
    disables breakpoints that are in use. A disabled breakpoint's address is
    retained and BP will not allow initialising it anew (except with AT),
    but it is otherwise skipped in breakpoint handling.

10.7.8 BE command - Enable breakpoint

       enable         BE index|AT address|ALL

    Like BD, but enables breakpoints.

10.7.9 BT command - Toggle breakpoint

       toggle         BT index|AT address|ALL

    Like BE and BD, but toggles breakpoints: A disabled breakpoint is
    enabled, while an enabled breakpoint is disabled.

10.7.10 BS command - Swap breakpoint

       swap           BS index1 index2

    This command is provided to allow re-ordering existing breakpoints.
    It takes two indices both of which must refer to valid breakpoints.
    However, it is allowed to specify the index of an unused breakpoint for
    either of the parameters (or even both). All data associated with the
    two breakpoints is swapped.

10.7.11 BL command - List breakpoints

       list           BL [index|AT address|ALL]

    BL lists a specific breakpoint given by its index, or all used
    breakpoints if given the keyword ALL or given neither an index nor the
    keyword. When given the AT keyword, all breakpoints with a matching
    linear address are listed. (This differs from all other B commands,
    which only select the first matching breakpoint when the AT keyword is
    given.)

    When listing all breakpoints only used breakpoints are displayed.

    The output format for unused breakpoints is as follows:

     -  "BP"

     -  The byte index given as two hexadecimal digits

     -  "Unused"

    The output format for used breakpoints is as follows:

     -  "BP"

     -  The byte index given as two hexadecimal digits

     -  A plus sign if the breakpoint is enabled, a minus sign if it is
        disabled.

     -  "Lin=" followed by the linear address of this breakpoint.

     -  The segmented address of this breakpoint. Only displayed if the
        breakpoint was initially specified with a segmented address, or it
        had a preferred offset specified with the BP OFFSET= keyword or to
        the BO command.

     -  The breakpoint content byte given in parentheses (generally "CC").

     -  "Counter=" followed by the breakpoint counter.

     -  "ID: " followed by the breakpoint ID, if any. Depending on the
        length the ID is shown on the first line or on a second line.

     -  "WHEN " followed by the breakpoint condition, if any. This is always
        written to a line on its own.

    Example output of BL:

      -bp at 100 id = start
      -bp at 103 counter = 4000
      -bp at 105 when al == 7
      -bl
      BP 00 + Lin=01_BB70  1BA7:0100 (CC) Counter=8000, ID: start
      BP 01 + Lin=01_BB73  1BA7:0103 (CC) Counter=4000
      BP 02 + Lin=01_BB75  1BA7:0105 (CC) Counter=8000
       WHEN al == 7
      -

10.8 BU command - Break Upwards

      break upwards   BU

    This command, which is only supported by Debuggable builds (DDebug) or
    Conditionally Debuggable builds (CDebug), causes the debugger to execute
    an int3 instruction in its own code segment. This breaks to the next
    debugger that was installed prior to DDebug or CDebug. Prior to the
    breakpoint, the message "Breaking to next instance." is displayed.

    In non-debuggable lDebug builds, the following error message is
    displayed instead:

      -bu
      Already in topmost instance. (This is no debugging build of lDebug.)
      -

    In conditionally debuggable builds, the following message is displayed
    instead if CDebug is currently not in debuggable mode:

      -bu
      Debuggable mode is disabled.
      Enable with this command: r DCO6 or= 0100
      -

10.9 BOOT commands - Boot loading support

    The BOOT commands are only available if the debugger is running in boot
    loaded mode.

10.9.1 BOOT PROTOCOL= command

      BOOT PROTOCOL=proto [parameters] [partition] [pathnames [cmdline]]

    This command is used to load a boot sector or kernel using the loaders
    implemented by the debugger. These loaders attempt to be highly
    compatible to the original loaders whose load protocols they simulate.

10.9.1.1 Specify protocol

    Using the keyword PROTOCOL, the load protocol to use as a base can be
    specified. This keyword is required, unless the special protocol named
    SECTOR is to be used.

10.9.1.2 Altering protocol parameters

    When specifying a protocol other than the special SECTOR protocol, the
    protocol parameters can be altered. Each protocol will set up defaults
    for all of those parameters. Each protocol can be completely described
    by a combination of parameters and default filenames. Every parameter
    is indicated by a keyword followed by a numeric expression, or in some
    cases followed by a segmented address.

    The following parameters are available:

    MINPARA

        Specify minimum amount of paragraphs to load from the first file. It
        is an error if a file is shorter than that.

    MAXPARA

        Specify maximum amount of paragraphs to load from the first file. It
        is valid for the file to be shorter or longer than this. If nonzero
        then it is an error if the file is so long that there is not enough
        memory to hold this amount of paragraphs. If zero, then as much of
        the file is loaded as fits.

    SEGMENT

        Specify load address of the data from the first file. The number
        specified is taken to be the segment of an address within memory.

    ENTRY

        Specify entrypoint to set up in the CS:IP registers. If a single
        numeric expression, it is taken as the offset (for IP) and the
        segment value is assumed as zero. That is, CS will be set up
        to equal the SEGMENT parameter in use. If a segmented address,
        the offset is used for IP and the segment is used as a relative
        adjustment to the SEGMENT that is in use to obtain the value for CS.
        It is valid for the segment value to be positive or negative.

    BPB

        Specify where to load the boot sector with (E)BPB. If a single
        numeric expression, it is taken as the offset in segment zero.
        If the segment is specified as 0FFFFh or -1, then the "auto-BPB"
        feature is used and the boot sector and stack is located at a high
        address that is not otherwise used. The offset is still set to the
        offset part in this case.

    CHECKOFFSET

        Specify offset of word value to check. Must not possibly cross a
        sector boundary. (This is checked by testing that the offset modulo
        32 is not equal to 31.) May not be higher than 0FFFEh.

    CHECKVALUE

        Specify value of word to check. If zero, no check occurs. It is an
        error if this value is nonzero and the check does not match.

    The following boolean parameters are available. Like the other
    parameters they read a numeric expression, but this is only checked to
    be true (non-zero) or false (zero).

    SET_DL_UNIT

        If true, set up the DL register with the load unit. This is used by
        several protocols.

    SET_BL_UNIT

        If true, set up the BL register with the load unit. This is used by
        the FreeDOS and EDR-DOS protocols.

    SET_SIDI_CLUSTER

        If true, initialise the DI (FAT12/FAT16) or SI:DI (FAT32) registers
        to hold the number of the first cluster of the first file. This is
        used by the MS-DOS v7 protocol.

    SET_DSSI_DPT

        If true, initialise DS:SI registers to point to the DPT. (Set equal
        to the interrupt 1Eh vector.) This may be used by the MS-DOS v6 and
        IBMDOS protocols.

    PUSH_DPT

        If true, initialise stack to hold a segmented (16:16) pointer to the
        interrupt 1Eh vector (always 0:78h) and then the DPT address (equal
        to the interrupt 1Eh vector). This may be used by the MS-DOS v6 and
        IBMDOS protocols, and is used by the MS-DOS v7 protocol.

    DATASTART_HIDDEN

        If true, modify the data start variable at dword [ss:bp - 4] to
        include the number of hidden sectors. (The hidden sectors are the
        partition's start offset in its unit.) This is used by the MS-DOS
        (v6/v7) and IBMDOS protocols.

    SET_AXBX_DATASTART

        If true, set the AX:BX register pair to the data start variable. If
        DATASTART_HIDDEN is also set, the registers will receive the value
        of the data start variable that includes the hidden sectors. This is
        used by the MS-DOS v6 and IBMDOS protocols.

    SET_DSBP_BPB

        If true, set up the DS register to equal SS. This makes DS:BP point
        to the boot sector with the (E)BPB. This is used by the EDR-DOS
        protocol.

    LBA_SET_TYPE

        If true, change the third byte of the boot sector to indicate the
        use of LBA access functions in the manner expected by the MS-DOS v7
        load protocol. That means a 90h (nop instruction) is written if to
        use CHS access, a 0Eh is written if the FAT type is not FAT32 and to
        use LBA access, and a 0Ch is written if the FAT type is FAT32 and to
        use LBA access.

    MESSAGE_TABLE

        If true, include the message table used by the MS-DOS v7 load
        protocol.

    SET_AXBX_ROOT_HIDDEN

        If true, pass the sector number of the root directory start
        including hidden sectors in the AX:BX register pair. This is used by
        the RxDOS.0 and RxDOS.1 protocols.

    NO_BPB

        If true, do not load the boot sector with BPB. This is used by the
        CHAIN protocol.

    SET_DSSI_PARTINFO

        If true, load sector with partition table to address 00600h and
        point DS:SI and DS:BP to the active partition table entry within the
        partition table. This is used by the CHAIN protocol.

    CMDLINE

        If true, allow a command line to be specified after the filenames.
        This is used by the RxDOS.2, RxDOS.3, and lDOS protocols. As an
        extension it may be enabled for the FreeDOS protocol, too.

10.9.1.3 Specifying protocol partition

    After the parameters, the debugger will try to parse a partition
    specification. Partition specifications are capitalisation-insensitive.
    A partition may be specified in the following ways:

    FDA

        Diskette-style (unpartitioned) file system on unit 00h

    FDB

        Diskette-style (unpartitioned) file system on unit 01h

    HDA1

        MBR-style (partitioned) file system on unit 80h, first primary
        partition

    HDA2

        MBR-style (partitioned) file system on unit 80h, second primary
        partition

    HDA5

        MBR-style (partitioned) file system on unit 80h, first logical
        partition

    HDA6

        MBR-style (partitioned) file system on unit 80h, second logical
        partition

    HDA(partnumber)

        MBR-style (partitioned) file system on unit 80h, with partition
        specified by partnumber.

    HDB1

        MBR-style (partitioned) file system on unit 81h, first primary
        partition

    LDP

        File system that the debugger loaded from

    YDP

        File system that the most recent Y command loaded from

    SDP

        Last used file system

    U00.

        Diskette-style (unpartitioned) file system on unit 00h

    U80.1

        MBR-style (partitioned) file system on unit 80h, first primary
        partition

    U(unitnumber).(partnumber)

        Unit specified by unitnumber with partition specified by partnumber.
        The specified partnumber may be specified as an expression in
        parentheses or as a literal number without parentheses. If it
        is an expression equal to zero in parentheses then that means
        unpartitioned.

    LD(partnumber)

        Unit that the debugger loaded from, with partition specified by
        partnumber.

    YD(partnumber)

        Unit that the most recent Y command loaded from, with partition
        specified by partnumber.

    SD(partnumber)

        Last used unit, with partition specified by partnumber.

    If no partition can be parsed, SDP is assumed. Note that partition
    numbers are parsed as decimal numbers, except if the partition number is
    specified as an expression with parentheses, in which case the default
    expression base is used (hexadecimal).

10.9.1.4 Specifying protocol filenames

    One or two pathnames may be specified to load, after the parameters or
    the partition specification. Both will have a default specified by the
    protocol. The default for the second name may be empty. If the second
    name is empty, no additional file is searched for.

    Each pathname may include subdirectory names, indicated by trailing
    slashes. If a pathname ends in a slash, the default filename is searched
    in the directory indicated by the pathname. The second pathname may be
    specified as two slashes to indicate no second file. If either pathname
    is specified as only one slash, then the default name is searched for in
    the root directory, exactly as if the pathname was not specified.

    The 32-byte directory entry of the first file is loaded to 00500h. The
    32-byte directory entry of the second file is loaded to 00520h. These
    entries are used by the MS-DOS v6 and IBMDOS protocols. If no second
    file is searched for, the 32 bytes at 00520h are filled with zeroes.

    The blank-padded FCB filenames of the two files are stored within the
    pseudo boot sector with (E)BPB that the loader sets up for the kernel.
    This supports kernels scanning the boot sector for informational
    filenames.

10.9.1.5 Specifying protocol command line

    If the CMDLINE boolean parameter is enabled, then after the two
    pathnames specifying filenames a command line is parsed. The command
    line should be separated from the second filename specification with
    one or more blanks. This command line is passed to the loaded kernel as
    specified for the lDOS load protocol. (The FreeDOS kernel was extended
    to also use a command line passed this way.)

    If the CMDLINE parameter is enabled but no command line content is
    specified, then an empty command line is passed. Note that this differs
    from passing no command line. To pass no command line, the CMDLINE
    parameter must be disabled.

    As a special case, semicolons are allowed within the specified command
    line and do not indicate comments.

10.9.2 BOOT LIST command

      BOOT LIST [unit|partition]

    This command is used to list partitions on an MBR-style partitioned
    unit.

10.9.3 BOOT DIR command

      BOOT DIR [partition] [pathname]

    This command is used to list files within a directory of a FAT12, FAT16,
    or FAT32 file system. A partition specification may be included. A
    pathname may be included; if it refers to a directory then the contents
    are listed, otherwise the specified file is listed.

10.9.4 BOOT READ and BOOT WRITE commands

      BOOT READ|WRITE [unit|partition] segment [[HIDDEN=sector] sector [count]]

    These commands are used to read or write sectors from disks. After
    the command keyword, a partition specification may be listed. Then, a
    segment must follow. This specifies the buffer to use.

    After the segment, an optional HIDDEN= keyword can be specified to
    specify a 32-bit sector number base. This is useful to implement 33-
    bit LBA access, but note it will overwrite the partition offset if a
    partition is specified. Instead of the HIDDEN= keyword, a HIDDENADD=
    keyword can be specified. It also reads a 32-bit sector number base.
    However, as opposed to HIDDEN=, HIDDENADD= will add to the hidden value
    of a specified partition, instead of replacing it. If a whole unit
    without a partition is specified then HIDDEN= and HIDDENADD= will result
    in the same offset being used.

    After the segment and optional hidden keywords, a 32-bit sector number
    may be specified. It defaults to zero. After the sector number, a 16-bit
    count may be specified. It defaults to one.

    Note that sectors are read or written one sector at a time. If the
    interrupt 13h function used returns an error 9 (boundary error), the
    debugger will attempt to use its auxiliary buffer to carry out the read
    or write, copying data as appropriate. The auxiliary buffer is aligned
    so as not to cross a 64 KiB boundary in memory. (Error 9 is usually
    returned if trying to access too many sectors at once or when diskette
    ISA DMA would cross a 64 KiB boundary.)

10.9.5 BOOT QUIT command

      BOOT QUIT

    This attempts to shut down the machine. A dosemu-specific callout will
    be attempted first, if dosemu is detected. Using APM will be attempted
    next, which works on qemu. If neither works, the debugger gives up.

10.10 C command - Compare memory

      compare         C range address

    Given a range, the address of which defaults to DS, and another address
    that also defaults to DS, this command compares strings of bytes, and
    lists the bytes that differ.

10.11 D command - Dump memory

      dump            D [range]
      dump bytes      DB [range]
      dump words      DW [range]
      dump dwords     DD [range]

    Given a range, the address of which defaults to DS, this command
    dumps memory in hexadecimal and as ASCII characters. The range may be
    specified with a lines length (refer to section 8.4). The default length
    if none is specified defaults to the number of lines specified in the
    variable DEFAULTDLINES if it is nonzero, or else the number of bytes
    specified in the variable DEFAULTDLEN.

    If a lines length is used, that many lines are dumped. The count of
    lines does not include the header or trailer if they're used. The count
    of lines will be inaccurate if the symbolic build is used and the dump
    lists symbols that point into the dumped data. (The amount of data in
    this case will match what it should be to produce the requested count of
    lines if no symbols were listed.) The count of lines will be accurate
    if either the 40-column friendly mode is enabled or not. If enabled,
    roughly half as much data is dumped for a given amount of lines, as the
    40-column mode dumps up to 8 bytes per line as opposed to the 80-column
    mode which dumps up to 16 bytes per line.

    If the DCO option 4 is set, text with the high bit set (80h to FFh, the
    top half of the 8-bit encoding space) is displayed as-is in the text
    dump. If a TOP keyword is used before the range, then top half text is
    displayed as-is as well. Otherwise, it will be treated like nonprintable
    text, which means it is replaced by dots in the text dump.

    If no range is specified, the D command continues dumping at "d_addr"
    (ADS:ADO), which is updated by each D command to point after the last
    shown byte. The default length is determined in the same way as for if
    a range without a length is specified. If autorepeat is used it behaves
    the same way as a D command without a range.

    The default is for D to dump bytes. After a DW or DD command, the
    autorepeat and plain D (without a range) default to the last-used size.
    If the default range should be used but the size should be reset to
    bytes, the DB command can be used. The D command with a range always
    acts the same as DB.

10.12 DI command - Dump Interrupts

      dump interrupts DI[R][M][L] interrupt [count]

    The DI command dumps interrupt vectors from the IVT (86M) or IDT (PM).
    In PM, for the vectors 00h to 1Fh, the exception handlers are also
    dumped. In 86 Mode, an interrupt chain is displayed if more than one
    entrypoint is reachable from the topmost handler. To make the next
    handler reachable, a handler must match one of several header / entry
    formats:

     -  IBM Interrupt Sharing Protocol (IISP) header (fully standard, with
        10EBh entrypoint and EBh jump to hardware reset - this matches what
        Ralf Brown's AMIS programs recognise)

     -  Non-standard IISP header

     -  iHPFS-style uninstalled IISP header (EA90h entrypoint)

     -  FreeDOS kernel relocation (near call followed by far jump immediate)

     -  Just a far jump immediate

    If the R is specified (directly after DI) then 86 Mode handlers are
    dumped even if in PM.

    If the M is specified then MCB names are displayed.

    If the L is specified then AMIS interrupt lists are queried for the
    interrupt number being dumped. This is so that the involved multiplex
    numbers and interrupt list indices can be displayed, and also so that
    hidden chains can be dumped. This means chains that are not reachable
    from the topmost IVT handler, but are found through the AMIS "Determine
    Chained Interrupts" call (either 03h pointer or 04h list return). The
    list index is displayed as FFFFh if the handler was found with 03h
    pointer return. Otherwise it indicates how many list entries precede the
    found handler's entry. For example, "list:0000h" means that the first
    list entry matched, and "list:0001h" means that the second list entry
    matched.

    Specifying the L makes the debugger use its auxiliary buffer. That means
    the DIL command cannot be used from the RE buffer if either a T/TP/P
    WHILE condition is used, or the T/TP/P silent buffer is used, or both.
    In addition, note that with the default buffer size, no more than about
    a 1000 handlers can be handled. (The actual limit may be as low as 500
    handlers if a lot of hidden chains occur.) If the limit is exceeded then
    the DIL command will display an error. The same error can also occur if
    the chain loops, or references a single handler from more than one other
    handler, or a single handler is listed by more than one multiplexer.

10.13 DM command - Dump MCBs

      dump MCB chain  DM [segment]

    The DM command dumps an MCB chain. If not given a start MCB segment, and
    the debugger is running as an 86-DOS application, the start of DOS's
    MCB chain is used. If given a start MCB segment, this is used as the
    starting MCB. (Note: In current RxDOS builds, the start MCB is always at
    segment 60h.)

    The DM command initially lists the debuggee's PSP. This is only valid
    when the debugger is running as an 86-DOS application.

    The MCB chain dump is continued until an MCB is encountered that has
    neither an M nor a Z signature letter, or the MCB address wraps around
    the 1 MiB boundary. In particular, this means that a disabled UMB link
    MCB (usually pointing to the MCB at segment 9FFFh if there is no EBDA
    nor any pre-boot-loaded programs) will not end the dump.

    Example output:

      -dm
      PSP: 1A73
      02B4 4D 0008 0016    352 B SD
      02CB 4D 02CC 00BC    2 KiB COMMAND
      0388 4D 039D 0013    304 B SYSTEM
      039C 4D 039D 0034    832 B SYSTEM
      03D1 4D 04A3 0013    304 B LDEBUG
      03E5 4D 03E6 00BC    2 KiB COMMAND
      04A2 4D 04A3 15CF   87 KiB LDEBUG
      1A72 5A 1A73 858C  534 KiB DEBUGGEE
      9FFF 4D 0008 3100  196 KiB SC
      D100 4D 0008 1EFF  123 KiB SC
      F000 4D 02CC 0040   1024 B COMMAND
      F041 4D 0000 0492   18 KiB
      F4D4 4D 0000 0619   24 KiB
      FAEE 4D 0000 0090    2 KiB
      FB7F 5A 03E6 0080   2048 B COMMAND
      -

    The columns are as follows:

     1. Segment address of MCB in hexadecimal. Always one less than the
        segment of the memory block contents.

     2. Signature letter in hexadecimal. Usually 4D ("M") for linking MCB
        and 5A ("Z") otherwise.

     3. Owner of the MCB in hexadecimal. Values below 50h are special system
        values. 0 indicates an unused MCB. 8 is the usual SC/SD/S system
        MCB owner. Higher values are generally process segments. A process
        segment is usually a memory block that is preceded by an MCB, which
        is owned by that block itself.

     4. Size in paragraphs of the MCB in hexadecimal. A value of zero is
        valid and indicates an MCB with an empty corresponding memory block.

     5. Size in bytes or kibibytes, in decimal.

     6. Name of the owner of this MCB. Free MCBs do not have a name. System
        MCBs have a name that is up to two letters long. Otherwise, the name
        is read from the MCB owner's own MCB. In this case the name is up to
        8 letters long.

10.14 DZ/D$/D#/DW# commands - Dump strings

      display strings DZ/D$/D[W]# [address]

    The D string commands each dump a string at a specified address, which
    defaults to DS as the segment.

     -  DZ displays an ASCIZ string, terminated by a byte with the value 0.

     -  D$ displays a CP/M-style string, terminated by a dollar sign
        character $.

     -  D# displays a Pascal-style string with a length count in the first
        byte.

     -  DW# displays a string with a length count in the first word.

10.15 D.A/D.D/D.B/D.L/D.T commands - Descriptor modification

    These commands are only available in lDebugX (DPMI-enabled) builds. They
    can only be used in Protected Mode. RC is set to 800h when attempting to
    use any of these commands while not in Protected Mode.

      Descriptor modification commands:
       (only valid in Protected Mode)
        Allocate      D.A
        Deallocate    D.D selector
        Set base      D.B selector base
        Set limit     D.L selector limit
        Set type      D.T selector type

10.15.1 D.A command - Allocate descriptor

        Allocate      D.A

    Allocates an LDT descriptor from the DPMI host. Sets the variable
    DARESULT to the selector if successful, else FFFFh. Sets RC to 801h or a
    DPMI error code (>= 8000h) on failure.

10.15.2 D.D command - Deallocate descriptor

        Deallocate    D.D selector

    Deallocates an LDT descriptor. Sets RC to 802h or a DPMI error code (>=
    8000h) on failure.

10.15.3 D.B command - Set descriptor base

        Set base      D.B selector base

    Sets the base of an LDT descriptor. A useful shorthand is to use a
    construct like "LINEAR cs:0" to get the base of a descriptor referenced
    by another selector. Sets RC to 803h or a DPMI error code (>= 8000h) on
    failure.

10.15.4 D.L command - Set descriptor limit

        Set limit     D.L selector limit

    Sets the limit of an LDT descriptor. Limits beyond FFFFFh must be 4 KiB
    aligned (low 12 bits set). Sets RC to 804h or a DPMI error code (>=
    8000h) on failure.

10.15.5 D.T command - Set descriptor type

        Set type      D.T selector type

    Sets the type of an LDT descriptor. 00FAh is a 16-bit code segment,
    4000h is the D/B bit (Default size / Big), so 40FAh is a 32-bit
    code segment. 00F2h is a 16-bit data segment. 8000h is the G bit
    (Granularity); modifying it may change the limit. The DESCTYPE keyword
    can be used in an expression to read the current type of a descriptor,
    refer to section 9.7. Sets RC to 805h or a DPMI error code (>= 8000h) on
    failure.

10.16 DT command - Dump text table

      dump text table DT [T] [number]

    Without a number parameter and without the T specifier, an ASCII table
    (codepoints 00h to 7Fh) is listed with short names for unprintable ASCII
    but the text itself for printable ASCII. The table lists the decimal
    and hexadecimal numbers. Without a number parameter but with the T
    specifier, a similar table depicting the top half of the 8-bit codepoint
    space is listed (values 80h to FFh).

    With a parameter, each byte of the specified number is displayed in
    decimal, hexadecimal, and the short name or the text itself (quoted). If
    the T specifier is present, top half text (value >= 80h) is displayed
    quoted, otherwise it instead displays as "top". The command will loop
    starting with the least-significant byte of the number, then continue
    with subsequent bytes until all remaining bytes are equal to zero. All
    up to four bytes are listed on the same line.

    Note that without the T specifier, no codepage dependent text is
    displayed. The T stands for "top".

10.17 E command - Enter memory

      enter           E [address [list]]

    The E command is used to enter values into memory. If the list is
    specified, its contents are written to the address specified. Otherwise,
    the interactive enter mode starts at the address specified. If no
    address is specified then interactive enter mode starts at the last used
    address. This is behind the last byte written by a prior E command, or
    at the last byte displayed in interactive enter mode.

    In the interactive enter mode, the segmented address is displayed, and
    then the current byte value (2 hexadecimal digits) found at that address
    yet. Following the value a dot is displayed. For example:

      -e 100
      1FFE:0100  C3.

    At this point the debugger accepts several different inputs:

     -  One or two hexadecimal digits: To enter a new value to be written at
        this address

     -  A blank: To write the new value (if any) and proceed to the next
        byte

     -  A minus: To write the new value (if any) and proceed to the prior
        byte

     -  Carriage Return, Line Feed, or a period: To write the new value (if
        any) and quit interactive enter mode

     -  Backspace: To delete the most recently entered digit of a candidate
        new value

     -  All other inputs are ignored

    After entering a blank, the debugger will either display the next byte's
    current value in the same line or start a new line with the current
    segmented address and then the current byte value. A new line is started
    if the current offset is divisible by 8. For example, after entering 8
    blanks:

      -e 100
      1FFE:0100  C3.     CC.     CC.     CC.     CC.     CC.     CC.     CC.
      1FFE:0108  CC.

    After entering a minus, the minus is displayed on the current line and
    then (always) a new line is started to display the new segmented address
    (with its offset decremented). For example, entering a new value ("A0"),
    then a blank, then a minus, and then another new value ("A1"), then a
    CR:

      -e 100
      1FFE:0100  C3.A0   CC.-
      1FFE:0100  A0.A1
      -

10.18 F command - Fill memory

      fill            F range [RANGE range|list]

    The F command fills memory with a byte pattern. The first parameter
    is the range to fill. The next parameter can be a list, in which case
    it provides the pattern with which to fill. If the RANGE keyword is
    provided then the pattern is read from memory as indicated by the range
    parameter that follows the keyword. The pattern is repeated so as to
    fill the destination. If the RANGE keyword is used, then the length of
    the pattern address range is optional. If the length is absent, it is
    assumed to equal that of the destination range.

10.19 G command - Go

      go              G [=address] [breakpts]

    The G command runs the debuggee. It can be given a start address (the
    segment of which defaults to CS), prefixed by an equals sign, in which
    case CS:EIP is set to that start address upon running. Note that if
    there is an error parsing the command line, CS:EIP is not changed.
    Further, if a breakpoint fails to be written initially, CS:EIP also is
    not changed.

    The G command allows specifying breakpoints, which are either segmented
    addresses (86M or PM addresses depending on DebugX's mode) or linear
    addresses prefixed by an "@ " or "@(", similar to how the BP command
    allows a breakpoint specification. G breakpoints are identified by their
    position in the command line, as the 1st, 2nd, 3rd, etc. By default, 16
    G breakpoints are supported.

    The G AGAIN command re-uses the breakpoints given to the last
    (successfully parsed) G command. It also allows an equals-sign-prefixed
    start address like the plain G command, in front of the AGAIN keyword.
    After the AGAIN keyword, additional breakpoints may be specified.

    If the command repetition of G is used, it is handled as if "G AGAIN"
    was entered, that is it re-uses the same breakpoints as those given to
    the prior G command.

    A G command that fails to parse will not modify the stored G breakpoint
    list. If an error occurs during writing breakpoints, the list will have
    been modified already however.

    The G LIST command lists the breakpoints given to the last (successfully
    parsed) G command.

    The "content" byte in G LIST is usually CCh (the int3 instruction
    opcode), but retains its original value if a failure occurs during
    breakpoint byte restoration.

    Example output of G LIST:

      -g 100 103 105
      AX=3000 BX=0000 CX=0200 DX=0000 SP=FFFE BP=0000 SI=0000 DI=0000
      DS=1BA7 ES=1BA7 SS=1BA7 CS=1BA7 IP=0103 NV UP EI PL ZR NA PE NC
      1BA7:0103 CD21              int     21
      -g list
         1st G breakpoint, linear 0001_BB70  1BA7:0100, content CC
         2nd G breakpoint, linear 0001_BB73  1BA7:0103, content CC (is at CS:IP)
         3rd G breakpoint, linear 0001_BB75  1BA7:0105, content CC
      -

    The output is as follows:

     -  The 1-based index ordinal of the point.

     -  The linear address of the point. (21-bit for Debug, 32-bit for
        DebugX.)

     -  The segmented address of the point. Only listed if the point was
        specified in a segmented form. That is, if the point was specified
        with a "@ " or "@(" prefix then no segmented address is saved along
        with it. (Internally, the word or dword "preferred offset" variable
        is set to all 1 bits then.) In Protected Mode, the segment is
        specified as "CS:" if the code segment's base matches the preferred
        offset. Otherwise, an R86M segment is shown with a dollar sign "$"
        prefix if the preferred offset matches any R86M segment. Failing
        that the offset is shown with a prefix reading "????:".

     -  The content byte. This is usually CCh. However, if a breakpoint
        failed to be restored then the original value is displayed here.

     -  Indicator that this point matches the current CS:IP or CS:EIP.
        This is only displayed if such a match is applicable. Running G
        AGAIN when this is applicable will step one time to bypass the
        corresponding point.

    There is another G command: After any equals sign, AGAIN keyword, and/or
    specified breakpoints, the line can be ended with a REMEMBER keyword.
    This saves the specified G breakpoint list and then returns control
    to the user. (The equals address, if any, is discarded.) It allows
    preparing a G breakpoint list ahead of its use. Auto-repeat, if enabled,
    will run like G AGAIN and actually run the debuggee after a G REMEMBER
    command.

10.20 GOTO command - Control flow branch

      goto            GOTO :label

    The GOTO command can only be used when executing from a script file, the
    command line buffer, or the RE buffer. It lets execution continue at a
    different point in the file or buffer. Labels are identified by lines
    that start with a colon, followed by the alphanumeric label name, and
    optionally followed by a trailing colon. The destination label of the
    GOTO command may be specified with or without the leading colon.

    There are several special cases:

     -  If the destination label is :SOF (Start Of File) then the file or
        buffer completely rewinds to its start.

     -  If the destination label is :EOF (End Of File) then the file or
        buffer is closed.

     -  If the destination label is not found then the file or buffer is
        closed, along with an error message.

10.21 H command - Hexadecimal add/subtract values

      hex add/sub     H value1 [value2 [...]]
      base display    H BASE=number [GROUP=number] [WIDTH=number] value

    The H command performs calculation and displays the result. If a single
    expression is given then its value is displayed, in hexadecimal and
    then in decimal. If more than one expression is given then two results
    are displayed, in hexadecimal only. The first result is that which is
    calculated by adding all expressions. The second result is calculated
    by subtracting all subsequent expressions from the first expression's
    value.

    If a value is above or equal to 8000_0000h then along each display of
    that value, the value interpreted as a negative two's complement number
    is listed in parentheses.

    If the form with the BASE keyword is given then only one number is
    displayed. The specified base may be between 2 and 36, inclusive. If the
    GROUP keyword is also used then digits are grouped. The group separator
    is the underscore, "_". The grouping number must be below or equal 32
    (20h). The default grouping is none, same as GROUP=0. If the WIDTH
    keyword is also used then at least that many digits are displayed. The
    width must be below or equal 32 (20h). The default width is one digit,
    same as WIDTH=0 or WIDTH=1.

    Examples:

      -h 1
      0001  decimal: 1
      -h 1 1
      0002  0000
      -h 1 1 1
      0003  FFFFFFFF (-0001)
      -h 1 + 2 * 3
      0007  decimal: 7
      -h cs * 10
      0001A730  decimal: 108336
      -h -26
      FFFFFFDA (-0026)  decimal: 4294967258 (-38)
      -h base=2 group=8 AA55
      10101010_01010101
      -h base=2 group=4 width=#16 #1234
      0000_0100_1101_0010
      -h base=#10 group=3 400*400
      1_048_576
      -h base=3 group=3 FFFF_FFFF
      102_002_022_201_221_111_210
      -

10.22 I command - Input from port

      input           I[W|D] port

    The I commands input from an x86 port. The port can be any number
    between 0 and FFFFh. Plain I inputs a byte from the specified port. The
    IW and ID commands input a word or dword respectively.

10.23 IF command - Control flow conditional

      if numeric      IF [NOT] (cond) THEN cmd
      if script file  IF [NOT] EXISTS Y file [:label] THEN cmd
      if variable     IF [NOT] EXISTS R variablename THEN cmd

    The IF command allows specifying a conditionally executed command. This
    is especially useful for creating conditional control flow branches with
    the GOTO command (see section 10.20).

    For the first form, the condition is a numeric expression. If it
    evaluates to non-zero it is considered true. If the NOT keyword is
    absent then a true condition expression leads to executing the THEN
    command. With the NOT keyword present the logic is reversed. Note
    that if an error occurs in parsing, the THEN command is not executed,
    regardless of whether the NOT keyword is present.

    The second form specifies a script file in the same format as accepted
    by the Y command (refer to section 10.56). A label may be specified
    behind the filename, as for the Y command. If the file is found,
    and contains the specified label if any, then the EXISTS clause is
    considered true. Depending on the presence of the NOT keyword the THEN
    command is executed next, or skipped. Note that if an error occurs in
    parsing, the THEN command is not executed, regardless of whether the NOT
    keyword is present.

    Likewise, if an unanticipated error occurs during access then the THEN
    command is not executed. Anticipated errors include:

     1. The drive or ROM-BIOS unit cannot be accessed at all. (Determined by
        sector 0 being unreadable.)

     2. The specified partition is not found.

     3. A specified directory is not found.

     4. The file is not found.

     5. A DOS error occurs opening the file.

     6. The file is empty.

     7. A specified label is not found.

    The third form checks for a variable name being recognised like for
    the R variable access command. If the variable name is recognised the
    condition is considered true. Otherwise, the candidate name is skipped
    by scanning for the first blank or comma, except for parenthetical index
    expressions which are parsed as expressions. The condition is considered
    false if no variable is recognised.

10.24 INSTALL command - Install optional features

    This command can be used to enable certain optional features. The
    parameters are a list of comma-separated keywords. First the entire list
    will be parsed. Upon successful parsing of all keywords the command will
    then start to handle the keywords.

    Save for the "AREAS" keyword, these features can be accessed by using
    the corresponding DCO flags as well. The allowed keywords are:

    INT2F

    DPMIHOOK

        (lDebugX-only) Enable installing debugger's interrupt 2Fh hook to
        intercept the DPMI entrypoint function call. The interrupt hook will
        actually occur upon running any debuggee code in Real/Virtual 86
        Mode. This hook is enabled by default. This keyword controls DCO4
        flag 0002h.

    INT08

    INT8

    TIMER

        Install debugger's interrupt 8 hook for the timer tick IRQ. This
        enables the Interrupt 8 Control pressed detection depending on the
        INT8CTRL variable (refer to section 11.24) as well as the double
        Control-C via serial I/O detection. This keyword controls DCO4 flag
        0004h.

    INT2D

    AMIS

        Install debugger's AMIS interface on interrupt 2Dh. A free multiplex
        number must be available and the existing interrupt vector must be
        valid for this to succeed. This keyword controls DCO4 flag 0008h.

    AREAS

        (lDDebugX-/lCDebugX-only) Install this debugger's exception areas
        into another debugger. The other debugger must have its AMIS
        interface installed at the point in time that this command is run.
        This keyword does not correspond to any DCO flags.

    SERIAL

        Install serial I/O for the debugger interface. Configuration must be
        ready, refer to section 11.10. This keyword controls DCO flag 4000h.

    INDOS

        Enter force InDOS mode. The debugger will avoid calling DOS in this
        mode, helping in debugging DOS or the interrupt 21h or 2Fh handlers.
        This keyword controls DCO flag 0008h.

    GETINPUT

        Enter the use DOS getinput mode. When DOS is available and used
        for I/O, this mode enables use of the debugger's getinput function
        rather than using the DOS interrupt 21h service 0Ah line editor to
        read from standard input. The debugger's line editor includes proper
        line editing, allows overlong input with a horizontally scrolling
        view of the buffer, and enables history recall. This keyword
        controls DCO flag 0800h.

    RHIGHLIGHT

        Enable R command register change highlighting. This keyword controls
        DCO3 flag 04_0000h.

    AUTOREPEAT

        Enable autorepeat while reading from a terminal. This feature is
        enabled by default. This keyword controls DCO3 flag 1000_0000h (in
        reverse).

    BIOSOUTPUT

        Prefer to output to video ROM-BIOS terminal using interrupt 10h
        services instead of to the DOS interrupt 21h. This keyword controls
        DCO6 flag 0200h.

    FLATBINARY

        Enable flat binary read mode, in which MZ .EXE files and .HEX files
        are read and written as if they were flat binaries. This feature is
        also controlled by the /F+ or /F- switches. This keyword controls
        DCO6 flag 0400h.

    BIGSTACK

        Enable .BIG style stack mode, in which flat binaries are loaded with
        the stack set up in a separate segment. This allows to execute .BIG
        style flat format executables like used in the build process of the
        debugger itself. This feature is also controlled by the /E+ or /E-
        switches. This keyword controls DCO6 flag 0800h.

    RH

        Enable RH mode. In RH (Register dump History) mode, a number of the
        last R, RE, T, TP, P, or G outputs are buffered in the auxiliary
        buffer. (The auxiliary buffer is about 8 KiB large by default.) The
        RH command can then be used to display all or some of the steps of
        the buffered contents. Other commands that use the auxiliary buffer,
        like RN and RM, cannot run when this mode is enabled. Enabling RH
        mode will clear the RH/silent buffer. This keyword controls DCO6
        flag 10_0000h.

    DEBUG

        (lCDebug-only) Enable debuggable mode. The conditionally debuggable
        debugger defaults to start up in debuggable mode. This feature is
        also controlled by the /D+ or /D- switches. This keyword controls
        DCO6 flag 0100h.

10.25 L command - Load Program

      load program    L [address]

10.26 L command - Load Sectors

      load sectors    L address drive sector count

10.27 M command - Move memory

      move            M range address

10.28 M command - Set Machine mode

      80x86/x87 mode  M [0..6|C|NC|C2|?]

    An M command without parameters, with a single "?" parameter, with an
    "NC" parameter, or a single expression parameter is a get or set machine
    mode command.

    The machine mode is used by the assembler and disassembler to show
    machine requirements exceeding the current machine.

    A plain "M" or "M ?" command displays the current machine.

    An "M NC" or "M C0" command sets the current coprocessor to absent.

    An "M C" command sets the current coprocessor to present. It is set to
    the coprocessor type corresponding to the current machine.

    An "M C2" command sets the current coprocessor to present, and the
    coprocessor type to 287. This command is only valid if the current
    machine is a 386.

    An M command with an expression evaluating to 0 to 6 sets the current
    machine to the specified numeric value. It also sets the current
    coprocessor type corresponding to the specified numeric value.
    Coprocessor presence is not modified by this command however.

    Note that all machine mode commands that parse a numeric expression (not
    "M", "M ?", nor "M NC") will actually parse the expression twice due
    to the internal dispatching between the machine mode commands and the
    move memory command. If the expression has side-effects then these side-
    effects will also occur twice. (An example of a side effect is reading
    the LFSR variable, which will step the LFSR.)

10.29 N command - Set program Name

      set name        N [[drive:][path]progname.ext [parameters]]

    This command sets up the filename and parameters to use when setting up
    a new process using the L (Load program) command. If the filename ends
    in .COM or .EXE it will be loaded as a DOS program using the interrupt
    21h service 4B01h. Otherwise the file is loaded as a flat binary by the
    debugger itself. In any case, the PSP of the process created by the
    L command will receive the command line tail, which starts after the
    filename.

    Unlike Microsoft's Debug the executable filename is not included in the
    command line tail, and an existing process won't be modified by the N
    command. It only sets the filename and tail for L to use.

10.30 O command - Output to port

      output          O[W|D] port value

    The O commands output to an x86 port. The port can be any number between
    0 and FFFFh. Plain O outputs a byte to the specified port. The OW and
    OD commands output a word or dword respectively. The value to write is
    specified by the second expression.

10.31 P command - Proceed

      proceed         P [=address] [count [WHILE cond] [SILENT [count]]]

    The P command causes debuggee to run a proceed step. This is the same as
    tracing (T command) for most instructions, but behaves differently for
    "call", "loop", and repeated string instructions. For these, a proceed
    breakpoint is written behind the instruction (similarly to how the G
    command writes breakpoints), and the debuggee is run without the Trace
    Flag set.

    As an exception, if a near immediate "call" (opcode E8h) is to be
    executed and its callee is a "retf" or "iret" instruction, then the
    "call" instruction is traced and not proceeded past. (This supports some
    relocation sequences.)

    Like for the G command, a start address can be given to P prefixed by an
    equals sign. Next, a count may be specified, which causes the command to
    execute as many P steps as the count indicates.

    After a count, a WHILE keyword may be specified, which must be followed
    by a conditional expression. Execution will only continue if the WHILE
    expression evaluates to true.

    After a count (when no WHILE is given) or after a WHILE condition,
    a SILENT keyword and optional count may be given. In this case, the
    debugger buffers the register dump and disassembly output of the
    executed steps, until control returns to the debugger command line.
    Then, the last dumps stored in the buffer are displayed. If a non-zero
    count is given, at most that many register dumps are displayed.

10.32 Q command - Quit

      quit            Q

10.33 QA command - Quit attached process

      quit process    QA

    The QA command tries to quit an attached process. It does this by
    resetting the current cs:eip, ss:esp, efl, and (only for DebugX) all
    segment registers. Then it runs interrupt 21h service 4C00h in the
    context of the current debuggee. Afterwards it reports on how the
    debugger regained control and whether the attached process terminated.

    (If between the current debuggee's process and the debugger's process
    there is any process that is self-parented, or a breakpoint interrupt or
    trace interrupt is caused by the current process having terminated, then
    the attached process may be considered not terminated.)

    The same underlying function is used by the program-loading L command
    and the default Q command (except if the debugger is running in TSR
    mode).

10.34 QB command - Quit and break

      quit and break  QB

    The QB command is composed of a Q command with a B flag. It indicates to
    the debugger to quit as usual, but to then run a breakpoint just before
    the debugger returns the control flow to either the OS, the application
    that executed the debugger, or (when resident as TSR, device driver, or
    bootloaded) the current debuggee.

    When successful, this instance of the debugger has already uninstalled
    all its interrupt hooks, so the breakpoint will run the interrupt 3
    handler that was installed prior to the debugger having been installed.

10.35 R command - Display and set Register values

      register        R [register [value]]

    The R command without any register specified dumps the current
    registers, either displayed as 16-bit or 32-bit values (depending on the
    RX option), and disassembles the instruction at the current CS:(E)IP
    location.

    R with a register, named debugger variable, or memory variable (of the
    form BYTE/WORD/3BYTE/DWORD [segment:offset]) displays the current value
    of the specified variable. It then displays a prompt, allowing the user
    to enter a new value for that variable. Entering a dot (.) or an empty
    line returns to the default debugger command line.

    R with a variable, followed by a dot (.), only displays the current
    value of that variable.

    R with a variable, followed by an optional equals sign, and followed by
    an expression, evaluates the expression and assigns its resulting value
    to the variable. The equals sign may instead be a binary operator with a
    trailing equals sign, which is handled as an assignment operator.

    Examples:

      -r ax .
      AX 0000
      -r ax
      AX 0000  :1
      -r ax
      AX 0001  :.
      -r ax += 4
      -r ax
      AX 0005  :
      -r word [cs:0]
      WORD [1867:0000] 20CD  :
      -r dif .
      DIF 0100B00B
      -

10.35.1 RE command - Run register dump Extended

      Run R extended  RE

    The RE command runs the RE buffer commands. Refer to section 15.7.

10.35.2 RE buffer commands

      RE commands     RE.LIST|APPEND|REPLACE [commands]

    RE.LIST lists the RE buffer contents in a way that can be re-used as
    input to RE.REPLACE.

    RE.APPEND appends the following commands to the RE buffer.

    RE.REPLACE replaces the RE buffer with the following commands.

    The RE buffer usage is described in the ?RE help page (section 15.7).

10.35.3 RC command - Run Command line buffer

      Run Commandline RC

    The RC command runs the command line buffer commands. This is similar to
    the RE command, except it uses a different buffer. Upon initialisation
    of the debugger the RC buffer is filled with the content of the /C
    switch (if any) in case the debugger is loaded as a DOS application, or
    else the contents of the kernel command line (if any) or the default
    kernel command line contents. Then the equivalent to an RC command is
    run.

    Command line buffer commands are displayed with a prompt consisting of
    an ampersand & or, for DDebug or for CDebug while in debuggable mode, a
    tilde followed by an ampersand ~&. When both RE and RC are running out
    of their respective buffers, the RE buffer contents take precedence.

10.35.4 RC buffer commands

      RC commands     RC.LIST|APPEND|REPLACE [commands]

    RC.LIST lists the command line buffer contents in a way that can be re-
    used as input to RC.REPLACE.

    RC.APPEND appends the following commands to the command line buffer.

    RC.REPLACE replaces the command line buffer with the following commands.

10.36 RH command - Display Register dump History steps

      regdump history RH [IN value, value, ...|value]

    The RH command displays steps from the RH/silent buffer while RH mode
    is enabled. RH mode can be enabled using the INSTALL RH command. (Refer
    to section 10.24.) The parameter to the RH command can be the keyword
    IN, followed by one or more comma-separated match ranges, or by a single
    number, or no parameter at all.

    The no parameter form displays all steps still saved in the RH buffer.

    The one parameter form displays a single step from the RH buffer. The
    number 0 refers to the most-recent saved step. The number 1 refers to
    the second most-recent saved step. And so on.

    The RH IN form accepts one or more match ranges. A match range can be:

     -  A single number. (Must be below 1_0000h.)

     -  The keyword FROM followed by a number followed by the keyword TO
        followed by a number. (The second number must be above-or-equal the
        first number. Both must be below 1_0000h.)

     -  The keyword FROM followed by a number followed by the keyword LENGTH
        followed by a number. (The length number plus the first number must
        be below-or-equal 1_0000h. A zero-length is valid, and will produce
        no output.)

    The RH IN command will treat each match range by displaying the
    corresponding steps from the RH buffer, but in chronological order. For
    instance, the following two commands are equivalent:

      rh in from 2 length 4

      rh in 5,4,3,2

    When parameters specify a number that is above the oldest still saved
    step in the RH buffer, the behaviour is not certain and may yet change.
    (For now, each older step will display the one oldest step once. This
    still may be subject to change.)

    The RH command defaults to page its output, if paging is enabled. Paging
    can be disabled for the RH command using the silent buffer output paging
    control. (This will, of course, also affect the silent buffer output.)
    The command r dco3 = dco3 clr 200 or 100 will instruct the RH command to
    not page its output.

    As an exception, if the RH buffer is empty then any valid RH command
    will produce no output at all.

    If RH mode is not enabled then the RH command may display stale or
    corrupted output, except when run directly after a silent-buffered
    T/TP/P command. In the latter case, the RH command will operate on the
    contents stored by the last run command.

10.37 RM command - Display MMX Registers

      MMX register    RM [BYTES|WORDS|DWORDS|QWORDS]

    This command dumps all 8 MMX registers. It is only available if MMX is
    supported by the machine. The optional size keyword specifies an item
    size, which defaults to BYTES. The BYTES size will match memory order of
    the byte values, displaying the least significant byte's value first. A
    size keyword of WORD will display the least significant word first, and
    so on.

10.38 RN command - Display FPU Registers

      FPU register    RN

10.39 RX command - Toggle 386 Register Extensions display

      toggle 386 regs RX

10.40 RV command - Show sundry variables

    This command shows the first 16 user-defined variables (refer to section
    11.15), the current options variables DCO (that is DCO1), DCS, DAO,
    DAS, the internal flags DIF (that is DIF1), as well as the debugger
    process segment (DPR), the debugger parent return address (DPI), and
    the debugger parent process (DPP). lDebugX also shows the debugger
    process selector (DPS), which is zero in 86 Mode and a selector value in
    Protected Mode. (All of these variables can be queried manually, the RV
    command lists them merely for convenience.)

    Additionally, in the last line the RV command displays the current
    debuggee's mode. This is either Real 86 Mode, Virtual 86 Mode, or
    (lDebugX only) Protected Mode with either a 16-bit CS or a 32-bit CS.

10.41 RVV command - Show nonzero user-defined variables

    This command shows all user-defined variables (refer to section 11.15)
    that are not currently zero. Variables are always shown four to a line,
    so a single non-zero variable will additionally show up to 3 variables
    that are currently zero.

10.42 RVM command - Show debugger segments

    This command shows various segments (and, in Protected Mode, selectors)
    used by the debugger. It currently shows the following:

     -  Code segment

     -  Code2 segment (only if _DUALCODE build)

     -  Data segment

     -  Entry segment (same as data segment but with a code selector in PM)

     -  Auxbuff segment

     -  History segment

10.43 RVP command - Show process information

    This command shows the debugger's mode as well as some client and
    debugger process addresses. The mode is one of:

     -  Boot loaded

     -  Device driver

     -  Application

     -  Application installed as TSR

    The process addresses include:

    PSP

        Process Segment Prefix (always a 86M segment value)

    Parent

        Parent of the PSP (for the debugger the would-be parent for
        termination, however note that during normal operation the debugger
        is self-parented)

    Parent Return Address

        16:16 far pointer (a segmented 86M far address) of the process's
        interrupt 22h value, the entrypoint to return to the parent (again
        for the debugger this is the would-be PRA for termination, during
        normal operation the debugger sets up its actual PRA to return
        control to the debugger itself)

    PSP Selector (only displayed for lDebugX)

        A selector or segment value, appropriate for the current mode, to
        address the PSP

    The process addresses can all be accessed individually too, using the
    following variables:

    PSP

        PSP (client), DPSP (debugger)

    Parent

        PARENT (client), DPARENT (debugger)

    Parent Return Address

        PRA (client), DPRA (debugger)

    PSP Selector (always a segment if not lDebugX)

        PSPSEL (client), DPSPSEL (debugger)

    The DPARENT and DPRA variables read as all zeros when the debugger is
    loaded in bootloaded, device driver, or resident application (TSR) mode.

10.44 RVD command - Show device information

    This command shows the device header (segmented 86M) far address as well
    as the size of the device's allocation, in paragraphs. If the debugger
    is not loaded in device mode then instead a message indicating this is
    displayed.

    The two variables can be accessed individually, too. These are the
    DEVICEHEADER and DEVICESIZE variables. Both of them read as all zeros
    when the debugger is not loaded in device mode.

10.45 S command - Search memory

      search          S range [REVERSE] [SILENT number] [RANGE range|list]

    The S command searches memory for a byte string. The first range
    specifies the search space. By default, searching will begin at the
    bottom of the search space and move upwards. If a REVERSE keyword is
    specified after the range then searching will begin at the top of the
    search space moving downwards. The search string is specified either
    with the RANGE keyword followed by another range, or as a list of byte
    values.

    If the SILENT keyword is specified, a silent number must be parsed
    before the list or range parameter. The number specifies how many result
    lines are displayed at most. It is a 32-bit unsigned number that may
    take any value in the range, including zero. If the number is zero, only
    the amount of matches is displayed.

    The read-only variable SRC (Search Result Count) will receive the 32-
    bit value that is the amount of matched occurrences. The variable SRS0
    receives the first Search Result Segment. Likewise SRO0 receives the
    first Search Result Offset. SRO1 to SROF hold subsequent Search Result
    Offsets. SRO is an alias to SRO0. SRO variables are 32-bit in the _PM
    build lDebugX, 16-bit otherwise. Unused SRO variables are zeroed out
    by a successful search. The COUNT variable is set to the length of the
    search string.

    The display of search results is as follows:

     -  First, the result's segmented address.

     -  Then, the displacement of the following dump. This is displayed with
        a leading plus sign and some amount of hexadecimal digits (2, 4, 6,
        or 8 digits). The number is the length of the search pattern (which
        is also written to the COUNT variable).

     -  Then, a hexadeximal dump of the up to 16 bytes that follow the
        search string match at this point.

     -  Finally, the ASCII character dump of these up to 16 bytes.

    There is an option to disable the data dump so as to only display the
    match addresses. If the bit 80_0000h is set in the DCO variable then the
    data dump is suppressed.

10.46 SLEEP command

      sleep           SLEEP count [SECONDS|TICKS]

    The SLEEP command sleeps for the indicated length. The duration defaults
    to seconds. If the TICKS keyword is specified then the duration is taken
    to mean timer ticks. (A timer tick is about 1/18 seconds.) If the input
    is from DOS or serial I/O then Control-C from the input terminal may be
    used to cancel the sleep.

10.47 T command - Trace

      trace           T [=address] [count [WHILE cond] [SILENT [count]]]

    The T command is similar to the P command. However, T traces most
    instructions. Depending on the TM option (section 10.48), interrupt
    instructions are also traced (into the interrupt handler) or proceeded
    past.

10.47.1 TP command - Trace/Proceed past string ops

      trace (exc str) TP [=address] [count [WHILE cond] [SILENT [count]]]

    The TP command is alike the T command, but proceeds past repeated string
    instructions like the P command would.

10.48 TM command - Show or set Trace Mode

      trace mode      TM [0|1]

    This instruction accesses the DCO flag 2. If run without an expression
    then the current status is displayed. Otherwise tracing into interrupts
    (for the T and TP commands) is enabled (nonzero expression) or disabled
    (zero expression).

10.49 TSR command - Enter TSR mode (Detach from process)

      enter TSR mode  TSR

    This command tries to find the PSP to which the debugger is attached. It
    starts the search at the current PSP and walks up the parent processes
    until finding the debugger. If a self-owned process is encountered the
    search is aborted.

    Once found, the attached PSP is patched with the PRA and parent process
    noted down for the debugger itself. That is, the debugger's would-be
    parent is made the parent of the attached process. The debugger's fields
    for original PRA and parent are cleared. Thus the TSR command, if it
    succeeds, switches the debugger into resident mode.

    The reverse operation is performed by the ATTACH command (see section
    10.6). The TSR command can be used right away in application mode, or
    can be used in device driver mode after the debugger has been attached
    to a process using the ATTACH command. The default state of the device
    driver mode debugger is resident mode.

10.50 U command - Disassemble

      unassemble      U [range]

    Given a range, the address of which defaults to CS, this command
    disassembles instructions from memory. The range may be specified with
    a lines length (refer to section 8.4). The default length if none is
    specified defaults to the number of lines specified in the variable
    DEFAULTULINES if it is nonzero, or else the number of bytes specified in
    the variable DEFAULTULEN.

    If a lines length is used, that many lines are disassembled. However,
    if a single instruction does not fit within one line due to a too long
    string of machine code, then the lines used for this instruction will
    count as one line as concerns the lines length. If an address length is
    specified, all instructions that are contained within or start within
    the specified range are disassembled.

    If no range is specified, the U command continues disassembling at
    "u_addr" (AUS:AUO), which is updated by each U command to point after
    the last disassembled byte. The default length is determined in the same
    way as for if a range without a length is specified. If autorepeat is
    used it behaves the same way as a U command without a range.

10.51 UNINSTALL command - Uninstall optional features

    This command can be used to disable certain optional features. The
    parameters are a list of comma-separated keywords. First the entire list
    will be parsed. Upon successful parsing of all keywords the command will
    then start to handle the keywords.

    The available keywords are documented for the INSTALL command, refer to
    section 10.24.

10.52 V command - Video screen swapping

      view screen     V [ON|OFF [KEEP|NOKEEP]]

    The V commands allow to enable or disable video screen swapping. When
    enabled, the debugger takes care that screen output of debuggee and
    debugger are strictly separated. This is useful to debug fullscreen text
    mode programs.

    The screen will be swapped whenever the debuggee is run with a run
    command (T/TP/P/G), or when the plain V command is used. The plain V
    command is provided to watch the debuggee screen while the debugger is
    active. It ends upon the user entering any key to the debugger terminal.

    Video screen swapping currently requires an XMS driver, and the debugger
    will allocate an XMS memory block of 32 KiB.

    V OFF KEEP will disable video screen swapping but keep the current
    debugger screen contents. V OFF NOKEEP (and the default for V OFF if the
    keep flag has not been set) will instead return to the debuggee screen
    contents. When the Q command succeeds, it executes the equivalent of V
    OFF. That is it will use the current keep flag.

10.53 W command - Write Program

      write program   W [address]

10.54 W command - Write Sectors

      write sectors   W address drive sector count

10.55 X commands - Expanded Memory (EMS) commands

      expanded mem    XA/XD/XM/XR/XS, X? for help

10.56 Y command - Run script file

      run script      Y [partition/][scriptfile] [:label]

    The Y command runs a script file. The script file is specified in two
    different ways, depending on whether the debugger is running as an 86-
    DOS application or as a boot-loaded kernel replacement.

     -  If running as an application, the script name is a regular pathname.
        It may be quoted with doublequotes if the pathname includes blanks.
        If the indicated drive supports long filenames (LFNs) then the
        debugger will first try to open the pathname as an LFN.

     -  Otherwise, the script name may start with a partition specification
        to use. (Refer to the ?BOOT help page in section 15.11 for partition
        specifications.) Then, the pathname relative to that partition's
        root directory follows. Long filenames are not supported. Note that
        it is not valid to run an empty script file when boot-loaded.

    Further, a label may be specified to cause execution to start at that
    label instead of at the start of the file. This is equivalent to placing
    a "GOTO :label" command at the start of the script file. The colon to
    indicate a label is required.

    If execution already is within a script file, then the Y command may be
    run with only a label (again with the colon required). In that case, the
    current script file is opened in a subsequent level (handle or boot-
    loaded script file context) and execution starts at that label.

    Opening a script file as DOS application only works while DOS is
    available (InDOS not set). Additionally, if during script file execution
    DOS becomes unavailable (InDOS is set) then the script file execution
    is paused. It is resumed once DOS becomes available again. (Control-
    C with a non-zero IOL variable may still be used to cancel script file
    execution. DOS is called to close affected handles only if DOS is
    available.)

10.57 Z commands - Symbolic debugging support

    These commands are only supported if the _SYMBOLIC build option is
    enabled.

10.57.1 Z /S=size - Allocate, resize, or free symbol tables

    The /S switch allows to change the symbol table allocation. The symbol
    tables may take up up to 256 KiB of 86 Mode memory (below 1024 KiB)
    or up to 2 MiB of XMS memory. XMS use implies an additional 65 KiB is
    allocated for padding and a transfer buffer.

    XMS use can be forced by using a letter X behind the /S. 86 Mode memory
    use can be forced by using a letter R instead. The prior selection can
    be undone using an asterisk *, returning to the default behaviour.
    That means allocate XMS if available, and fall back to 86 Mode memory
    otherwise.

    After the equals sign a size is to be specified. The size can be an
    immediate number or an expression, or the keyword MAX to use the maximum
    size. An expression must be surrounded by round parentheses. The size
    specifies the amount of kibibytes to allocate. The size may be zero,
    which signals to free all symbol tables. This deletes all symbols yet
    defined. Otherwise, new symbol tables are allocated. Existing symbols
    will be transferred from the old symbol tables, if there are any. It is
    an error to specify a symbol table size that is not large enough to hold
    all currently defined symbols, except for specifying a zero size.

    Multiple /S switches can be specified within the same Z command. They
    are processed one by one, that is an error during parsing or execution
    of a subsequent switch will not make it so a prior switch is skipped.

10.57.2 Z STAT - Show symbol table statistics

    This command shows statistics on the current symbol table sizes,
    including the amount of total, used, and free units. Each of the symbol
    main array, symbol hash array, and symbol string heap are listed.

10.57.3 Z ADD - Add a symbol

    This command is used to add a new symbol. It can be followed by several
    parameters. These are:

    SYMBOL= or S=

        Name of the symbol, may be quoted

    OFFSET= or O=

        Offset of the symbol

    LINEAR= or L=

        Linear address of the symbol

    FLAGS= or F=

        Flags of the symbol

    No keyword

        Segmented address of the symbol to specify the linear address and
        offset

10.57.4 Z DEL - Delete a symbol

    This command deletes a symbol. It can be followed by the symbol name
    to delete, or a RANGE keyword and an address range parameter, or an
    UNREFSTRING keyword. The latter is to clean up the symbol string heap by
    deleting entries that are no longer used.

10.57.5 Z COMMIT - Commit temporary symbols

    Z ADD will batch up new symbols as temporary symbols. They are committed
    into the symbol tables upon several conditions, such as no more space
    for temporary symbols or execution of a command other than Z ADD or Z
    ABORT. The Z COMMIT command is for forcing the temporary symbols be
    committed. This should not usually be required.

10.57.6 Z ABORT - Discard temporary symbols

    This command discards all temporary symbols batched by prior Z ADD
    commands if they were not yet committed. If the debugger responds to
    every command with the error message "Invalid symbol table data!" then
    something went wrong with the committing of temporary symbols. In this
    case the Z ABORT command may help to return the debugger to a usable
    state.

10.57.7 Z LIST - List symbols

10.57.8 Z MATCH - Match symbols

10.57.9 Z RELOC - Relocate symbols

11: Variable Reference
----------------------

11.1 Registers

    All debuggee registers can be accessed numerically:

     -  al, cl, dl, bl, ah, ch, dh, bh

     -  ax, cx, dx, bx, sp, bp, si, di

     -  eax, ecx, edx, ebx, esp, ebp, esi, edi

     -  es, cs, ss, ds, fs, gs

     -  fl, efl, ip, eip

    Each 16-bit register can be used in a register pair, such as:

     -  dxax

     -  bxcx (used by L load program and W write program commands)

     -  sidi

     -  csip

11.2 MMX registers - MMxy

    If MMX is available, the debuggee's MMX registers can be accessed as
    variables. However, as the debugger only supports 32-bit numbers, only
    half of a 64-bit MMX register can be accessed. The "x" is a digit from 0
    to 7. The "y", if present, is one of the following letters:

    L

        Access only low 32 bits

    H

        Access only high 32 bits

    Z

        Read low 32 bits, write full 64 bits with zero extension to qword

    S

        Read low 32 bits, write full 64 bits with sign extension to qword

    Letter absent

        Same as letter Z

11.3 Options

11.3.1 DCO - Debugger Common Options

    DCO1 (alias DCO) to DCO6. Dword. Writable.

11.3.2 DCS - Debugger Common Startup options

    DCS1 (alias DCS) to DCS6. Dword. Read-only.

11.3.3 DIF - Debugger Internal Flags

    DIF1 (alias DIF) to DIF6. Dword. Read-only.

11.3.4 DAO - Debugger Assembly Options

    Dword. Writable.

11.3.5 DAS - Debugger Assembly Startup options

    Dword. Read-only.

11.3.6 DPI - Debugger Parent Interrupt 22h

    Alias DPRA. Dword. Read-only. Always a 86M segmented pointer. 0 if in
    TSR mode, or loaded as a device driver, or in bootloaded mode.

11.3.7 DPR - Debugger PRocess

    Alias DPSP. Word. Read-only. Always a 86M segment.

11.3.8 DPP - Debugger Parent Process

    Alias DPARENT. Word. Read-only. Always a 86M segment. 0 if in TSR mode,
    or loaded as a device driver, or in bootloaded mode.

11.3.9 DPS - Debugger Process Selector

    0 while in Real or Virtual 8086 Mode, debugger process selector
    otherwise. (The process selector addresses DebugX's PSP and DATA ENTRY
    section.) This variable does not exist on non-DPMI lDebug builds.

11.3.10 DPSPSEL - Debugger PSP Segment/Selector

    The debugger's PSP segment while in 86 Mode, a selector pointing to the
    same base while in Protected Mode. This variable exists even on non-DPMI
    builds, where it is always the same as DPSP.

11.4 Default step counts

    PPC

        Proceed command (section 10.31) default step count

    TPC

        Trace/Proceed command (section 10.47.1) default step count

    TTC

        Trace command (section 10.47) default step count

    All of these are doublewords and default to 1. For the respective
    commands, these counts specify the number of steps to take if none is
    specified explicitly. This includes when a command is run by autorepeat,
    refer to section 10.1. If one of these is set to zero then it is an
    error to not specify a count explicitly for the corresponding command.

11.5 Default lengths

    DEFAULTDLEN

        Word. Default length of D/DB/DW/DD commands in bytes (section
        10.11). Only used if DEFAULTDLINES is zero. Default is 128.

    DEFAULTDLINES

        Word. Default length of D/DB/DW/DD commands in lines (section
        10.11). Not used if zero. This is a word variable, but setting it to
        a value higher than 7FFFh is invalid. Default is zero.

    DEFAULTULEN

        Word. Default length of U command in bytes (section 10.50). Only
        used if DEFAULTULINES is zero. Default is 32.

    DEFAULTULINES

        Word. Default length of U command in lines (section 10.50). Not used
        if zero. This is a word variable, but setting it to a value higher
        than 7FFFh is invalid. Default is zero.

11.6 Limits

11.6.1 RELIMIT - RE buffer execution command limit

    Doubleword. Default is 256. If this many commands are executed from the
    RE buffer, the execution is aborted and the command that called RE is
    continued.

11.6.2 RECOUNT - RE buffer execution command count

    Doubleword. This is reset to zero when RE buffer execution starts.
    Each time a command is executed from the RE buffer, this variable is
    incremented. If it reaches the value of RELIMIT, RE buffer execution is
    aborted.

11.6.3 RCLIMIT - RC buffer execution command limit

    Doubleword. Default is 4096. If this many commands are executed from the
    RC buffer, the execution is aborted.

11.6.4 RCCOUNT - RC buffer execution command count

    Doubleword. This is reset to zero when RC buffer execution starts.
    Each time a command is executed from the RC buffer, this variable is
    incremented. If it reaches the value of RCLIMIT, RC buffer execution is
    aborted.

11.7 Return Codes

11.7.1 RC - Return Code

    Word. This holds the most recent command's return code. If the most
    recent command succeeded, then this is zero.

11.7.2 ERC - Error Return Code

    Word. This holds the most recent non-zero return code.

11.8 Addresses

11.8.1 A address (AAS:AAO)

    AAS: word, AAO: doubleword. Default address for the assembler. Updated
    to point after each assembled instruction.

11.8.2 D address (ADS:ADO)

    Default address for memory dumping. Updated to point after each dumped
    memory content.

11.8.3 Address behind R disassembly (ABS:ABO)

11.8.4 U address (AUS:AUO)

    Default address for the disassembler.

11.8.5 E address (AES:AEO)

    Default address for memory entry.

11.8.6 DZ address (AZS:AZO)

    Default address for DZ command, ASCIZ strings. Terminated by zero byte.

11.8.7 D$ address (ACS:ACO)

    Default address for D$ command, CP/M strings. Terminated by dollar sign
    "$".

11.8.8 D# address (APS:APO)

    Default address for D# command, Pascal strings. Prefixed by length count
    byte.

11.8.9 DW# address (AWS:AWO)

    Default address for DW# command. Prefixed by length count word.

11.8.10 DX address (AXO)

    Default address for DX command. (Only included in DebugX.)

11.9 I/O configuration

11.9.1 IOR - I/O Rows

    Byte. Default 1. Sets the number of rows of the terminal used by DOS or
    BIOS output. Setting this to zero disables paging to the DOS or BIOS
    output. Setting this to 1 uses the automatic selection. That means the
    BIOS Data Area byte at address 484h, plus one, is used. If using that
    byte and it is zero, paging is disabled.

11.9.2 IOC - I/O Columns

    Byte. Default 1. Sets the number of columns of the terminal used by
    BIOS input. Setting this to zero selects a default (80). Setting this
    to 1 uses the automatic selection. That means the BIOS Data Area word
    at address 44Ah is used. This is used by the line input handling if
    inputting from the BIOS terminal (int 16h, int 10h), or if inputting
    from a DOS terminal when DCO flag 800h is set. A value between 2 and 39,
    inclusive, is not recommended.

11.9.3 IOCLINE - I/O Columns for splitting lines in raw input

    Byte. Default 0. Sets the number of columns of the terminal at which to
    split overlong lines after the user submits an input line with the raw
    input line editor. If this is zero, splitting overlong lines is disabled
    and it is assumed that the terminal will split lines as desired.
    Otherwise, overlong lines (ie those extending past the IOC width) will
    be split to have no more than the amount of bytes specified by the
    IOCLINE variable. Makes most sense to set this equal to IOC or DSC, or
    else to zero. Any nonzero value is allowed.

11.9.4 IOS - I/O Circular Keypress Buffer Start

    Word. Default 0 or 1Eh. Indicates where the ROM-BIOS's circular
    keypress buffer starts. Value can be nonzero to force a particular
    offset in segment 40h. Value can be zero to force using the value at
    word [40h:80h], using an extension not available on all systems.

    On startup the debugger checks whether the extension values are valid.
    If they are then the default of the IOS variable is left as zero.
    Otherwise, the default is set to 1Eh, which is the default buffer
    location.

    This variable is used to check for Ctrl-C keypresses if the InDOS mode
    is on (either InDOS flag set, DCO flag 8 set, or in bootloaded mode) and
    serial I/O is not in use and the flag DCO3 2000_0000h is set. Setting
    this variable nonzero and equal to IOE disables Ctrl-C checking.

    Modifying this variable should only be done while it is not in use.
    That means using DOS for input, using serial I/O for input, or clearing
    the DCO3 flag 2000_0000h. Modifying this variable and the IOE variable
    should be done together, so that they are valid together when in use.

11.9.5 IOE - I/O Circular Keypress Buffer End

    Word. Default 0 or 3Eh. Indicates where the ROM-BIOS's circular
    keypress buffer ends. Value can be nonzero to force a particular
    offset in segment 40h. Value can be zero to force using the value at
    word [40h:82h], using an extension not available on all systems.

    Refer to IOS description above.

11.9.6 IOL - I/O Amount of Script Levels to Cancel

    Word. Default 255. Indicates how many levels of script files and RE
    buffer execution to cancel when a Control-C input or critical DOS error
    is detected by the debugger. The effective value will be incremented by
    one if IOF flag 1 is set and RE buffer execution is in progress.

    Zero indicates to only cancel the current command. One indicates to
    cancel the current command, plus the RE buffer execution if any, else
    up to one level of script file execution. Two indicates to cancel two
    levels of execution: either the RE buffer execution and one level of
    script file execution, or up to two levels of script file execution.

    The debugger always cancels RE buffer execution first if it is in
    progress. Next, the innermost script file execution is cancelled, if
    any.

11.9.7 IOF - I/O Flags

    Word. Default 1. Flags for I/O handling. Currently defined:

    1

        Extra IOL level for RE buffer execution. If set, RE buffer execution
        being in progress increments the effective value of the IOL
        variable.

11.10 Serial configuration

11.10.1 DSR - Debugger Serial Rows

    Byte. Default 24. Sets the number of rows of the terminal connected via
    serial port. Setting this to zero disables paging to the serial port.
    Setting this to 1 uses the IOR variable handling.

11.10.2 DSC - Debugger Serial Columns

    Byte. Default 80. Sets the number of columns of the terminal connected
    via serial port. Setting this to zero selects a default (80). Setting
    this to 1 uses the IOC variable handling. This is used by the line input
    handling. A value between 2 and 39, inclusive, is not recommended.

11.10.3 DST - Debugger Serial Timeout

    Byte. Default 15. This gives the number of seconds that the KEEP prompt
    upon serial connection waits. Setting this to zero waits at the prompt
    forever.

11.10.4 DSF - Debugger Serial FIFO size

    Byte. Default 16. This gives the size of the 16550A's built-in TX FIFO
    to use. Set to 15 if using dosemu before revision gc7f5a828 2019-01-22,
    see https://github.com/stsp/dosemu2/issues/748.

11.10.5 DSPVI - Debugger Serial Port Variable Interrupt number

    Byte. Default 0Bh, corresponding to COM2. Use 0Ch for COM1. This
    specifies the interrupt number to hook so as to be notified of serial
    events. The use of this variable occurs only when connecting to serial
    I/O. The value at that point in time is cached for as long as the serial
    connection is in use.

11.10.6 DSPVM - Debugger Serial Port Variable IRQ Mask

    Word. Default 0000_1000b, corresponding to COM2. Use 0001_0000b for
    COM1. This specifies the IRQ mask of which IRQs to enable. The low 8
    bits correspond to IRQ #0 to #7 and the high 8 bits correspond to IRQ
    #8 to #15. If any bit of the high 8 bits is set then generally the bit
    0100b should be set too, to enable the chained PIC. This circumstance is
    not automatically detected. The use of this variable occurs only when
    connecting to serial I/O. The value at that point in time is cached for
    as long as the serial connection is in use.

11.10.7 DSPVP - Debugger Serial Port Variable base Port

    Word. Default 02F8h, corresponding to COM2. Use 03F8h for COM1. This
    specifies the I/O port base to address the UART. The use of this
    variable occurs only when connecting to serial I/O. The value at that
    point in time is cached for as long as the serial connection is in use.

11.10.8 DSPVD - Debugger Serial Port Variable Divisor latch

    Word. Default 12, corresponding to 9600 baud. This specifies the DL
    value to set during initialisation. The use of this variable occurs only
    when connecting to serial I/O.

11.10.9 DSPVS - Debugger Serial Port Variable Settings

    Byte. Default 0000_0011b, corresponding to 8n1. (8n1 = 8 data bits, no
    parity, 1 stop bit.) This specifies the settings to set up in LCR. The
    high bit (80h) generally must be clear. The use of this variable occurs
    only when connecting to serial I/O.

11.10.10 DSPVF - Debugger Serial Port Variable FIFO select

    Byte. Default 0. This specifies what to write to the FCR. The low 3 bits
    (07h) generally must be clear. The use of this variable occurs only when
    connecting to serial I/O. The value at that point in time is cached for
    as long as the serial connection is in use.

11.11 Timer configuration

    These variables control some details of the debugger's timers used for
    waiting in a few places. The affected timers are:

     -  SLEEP command

     -  KEEP prompt timeout during serial I/O connection

     -  Serial output send wait if buffer full

    Unaffected timers include:

     -  DCO3 flag 0400_0000h (delay for a tick before writing breakpoints),
        this only waits until one tick change is observed

     -  Interrupt 8 Control pressed check, this does not count tick changes
        but rather counts interrupt calls

11.11.1 GREPIDLE - getc repeat idle count

    Byte. Default 0. If the getc function invokes the idle handling, it
    will repeatedly call the idle function if this variable holds a nonzero
    value. The value specifies the amount of repetitions past the first
    call. This variable is intended for debugging.

11.11.2 SREPIDLE - Sleep repeat idle count

    Byte. Default 0. If the SLEEP command invokes the idle handling, it
    will repeatedly call the idle function if this variable holds a nonzero
    value. The value specifies the amount of repetitions past the first
    call. This variable is intended for debugging.

11.11.3 SMAXDELTA - Maximum encountered delta ticks

    Word. This value is set anew whenever a wait handler has found a delta
    ticks larger than the prior value of this variable. After any wait
    iteration the variable inevitably will be nonzero.

11.11.4 SDELTALIMIT - Delta ticks limit

    Word. Default 5. This variable specifies the upper limit of the delta
    between tick low words accepted as being accurate.

    Note that at midnight the tick low word goes from 00AFh or 00B0h to
    0000h. The delta appears to be FF51h or FF50h ticks at that point.
    Therefore the limit should be set small enough that the total wait time
    is not majorly skewed at midnight.

    However, it is possible that the idle handling takes so long that more
    than one tick has actually gone by until the wait handling is run again.
    For such system setups it can be desirable to set the limit to more than
    1.

    A good compromise is to set the limit to between 1 and 6, inclusive. A
    limit of 6 ticks only skews for 1/3 of a second at midnight.

11.12 _DEBUG1 variables

    These variables are not supported by default. The build option _DEBUG1
    must be enabled to include them. The Test Counter variables work
    similarly to permanent breakpoint counters:

     -  If the counter AND-masked with 7FFFh is zero, it is at a terminal
        state.

     -  If the counter is not yet at a terminal state, it is decremented.

     -  If the counter is decremented to zero, it triggers.

     -  If the counter is decremented to 8000h or already at 8000h, it
        triggers.

    The default values for all counters and addresses is zero.

11.12.1 TRx - Test Readmem variables

    If a fault is injected into readmem, it returns the value given in TRV.

    TRC - Test Readmem Counter

        Word. Each of the TRC0 to TRCF counters gives one counter for
        readmem fault injection testing.

    TRA - Test Readmem Address

        Doubleword. Each of the TRA0 to TRAF counters gives one linear
        address for readmem fault injection testing.

    TRV - Test Readmem Value

        Byte. Default 0. If a readmem fault is injected, this byte value is
        returned by the read instead of the actual memory content.

11.12.2 TWx - Test Writemem variables

    If a fault is injected into writemem, it returns failure (CY).

    TWC - Test Writemem Counter

        Word. Each of the TWC0 to TWCF counters gives one counter for
        writemem fault injection testing.

    TWA - Test Writemem Address

        Doubleword. Each of the TWA0 to TWAF counters gives one linear
        address for writemem fault injection testing.

11.12.3 TLx - Test getLinear variables

    If a fault is injected into getlinear, it returns failure (CY).

    TLC - Test getLinear Counter

        Word. Each of the TLC0 to TLCF counters gives one counter for
        getlinear fault injection testing.

    TLA - Test getLinear Address

        Doubleword. Each of the TLA0 to TLAF counters gives one linear
        address for getlinear fault injection testing.

11.12.4 TSx - Test getSegmented variables

    If a fault is injected into getsegmented, it returns failure (CY).

    TSC - Test getSegmented Counter

        Word. Each of the TSC0 to TSCF counters gives one counter for
        getsegmented fault injection testing.

    TSA - Test getSegmented Address

        Doubleword. Each of the TSA0 to TSAF counters gives one linear
        address for getsegmented fault injection testing.

11.13 _DEBUG3 variables

    These variables are not supported by default. The build option _DEBUG3
    must be enabled to include them. These variables are used to test the
    read-only masking. Read-only masking makes it so that bits given in the
    mask are read-only. Bits that are clear in the mask are writable.

11.13.1 MT0 - Mask Test 0

    Doubleword. Default 0. Mask AA55_AA55h.

11.13.2 MT1 - Mask Test 1

    Doubleword. Default 0011_0022h. Mask 00FF_00FFh.

11.14 Y command variables

    Y command variables can be used when the Y command (as application
    or bootloaded) has been used to open a script file. YSx (Y Script)
    variables are generic and refer to whatever Y file is opened. YBx (Y
    Bootloaded script) variables refer to opened Y files while bootloaded.
    YHx (Y Handle script) variables refer to opened Y files as application.

11.14.1 YSF - Y Script Flags

    Word. Partially read-write, partially read-only.

    Flag 4000h controls whether script file input is displayed or not.
    Prepending an AT sign (@) to a line that is read from a script file will
    hide the input of that line. Setting YSF flag 4000h will hide all input
    lines instead. The effect is similar to prepending @ to every line.

    YSF variables are only available while executing script files.

11.15 V variables - Variables with user-defined purpose

    Doubleword. Default zero. V0 to VF or V00 to VFF each specify one
    variable. It is valid to refer to any V variable using an index
    expression. Index expression means that the variable name (V) is
    immediately followed by an opening parenthesis, followed by a numeric
    expression which evaluates to a number below 100h.

11.16 PSP variables

    All of these are read-only. All of them are zero if in bootloaded mode.

11.16.1 PSP - Process Segment Prefix

    Word. Always a segment,

11.16.2 PPR - Process PaRent

    Alias PARENT. Word. Always a segment.

11.16.3 PPI - Process Parent Interrupt 22h

    Alias PRA. Dword. Always a 86 Mode segmented address.

11.16.4 PSPSEL - PSP segment or selector

    Alias PSPS. Word. Segment or selector according to mode.

11.17 SR variables - Search Results

11.17.1 SRC - Search Result Count

    Doubleword. Read only. Amount of matches found by last S command.

11.17.2 SRS - Search Result Segment

    Word. Read only. SRS0 to SRSF each specify one variable. Search result
    segments of last S command's matches.

11.17.3 SRO - Search Result Offset

    Word or doubleword (DebugX). Read only. SRO0 to SROF each specify one
    variable. Search result offsets of last S command's matches. It is valid
    to refer to any SRO variable using an index expression. Index expression
    means that the variable name (SRO) is immediately followed by an opening
    parenthesis, followed by a numeric expression which evaluates to a
    number below 10h.

11.18 Access variables

    These variables can be left out of the build. The build option
    _MEMREF_AMOUNT must be enabled to include them.

11.18.1 READADR

    Doubleword. Read only. READADR0 to READADR3 each specify one variable.
    (Amount of READADR variables can be configured at build time with the
    option _ACCESS_VARIABLES_AMOUNT, which defaults to 4.) Linear addresses
    of string, stack, or explicit memory operand reads. Initialised by the
    R command. Unused variables are reset to zero by the R command. It
    is valid to refer to any READADR variable using an index expression.
    Index expression means that the variable name (READADR) is immediately
    followed by an opening parenthesis, followed by a numeric expression
    which evaluates to a number below 4.

11.18.2 READLEN

    Doubleword. Read only. READLEN0 to READLEN3 each specify one variable.
    Length of string, stack, or explicit memory operand reads. Initialised
    by the R command. Unused variables are reset to zero by the R command.
    It is valid to refer to any READLEN variable using an index expression.

11.18.3 WRITADR

    Doubleword. Read only. WRITADR0 to WRITADR3 each specify one variable.
    Linear addresses of string, stack, or explicit memory operand writes.
    Initialised by the R command. Unused variables are reset to zero by the
    R command. It is valid to refer to any WRITADR variable using an index
    expression.

11.18.4 WRITLEN

    Doubleword. Read only. WRITLEN0 to WRITLEN3 each specify one variable.
    Length of string, stack, or explicit memory operand writes. Initialised
    by the R command. Unused variables are reset to zero by the R command.
    It is valid to refer to any WRITLEN variable using an index expression.

11.19 Machine type variables

    MMT - Maximum Machine Type encountered

        Set whenever the disassembler encounters an instruction requiring
        a machine type that is higher than this variable's current value.
        Writable.

    MACHX86 - Machine type for assembler and disassembler

        Current machine type to use for assembler and disassembler. Read-
        only, use M commands to modify.

    MACHX87 - Coprocessor encoded machine type

        Contains valid argument to M command: C0h if no coprocessor, 0Ch if
        coprocessor matching machine, C2h if machine is a 386 with a 287
        coprocessor. Read-only, use M commands to modify.

11.20 LFSR variables

    These variables provide access to a simple LFSR (Linear Feedback Shift
    Register). The default taps are chosen so that a full-range 32-bit LFSR
    is in use. That means there are 4 giga binary steps, minus one, and all
    possible 32-bit values are in use except for the all zeros value. A step
    of the LFSR is done by shifting the old value to the right once. If the
    bit shifted out is a 1, then the new value is obtained by applying the
    LFSR taps as a XOR mask to the shift result. If the bit shifted out is a
    0, then the new value is simply the shift result.

    LFSR - Forward LFSR variable

        Whenever this variable is read, it first executes an LFSR step from
        the variable's prior value. What is actually read is the new value
        after the step. This variable is initialised to the constant 2 on
        startup of the debugger. That means that with the default taps, the
        first read will return 1, the second 8020_0003h, etc.

    LFSRTAP - Taps to use for the LFSR

        This variable determines the tap bits to use for the LFSR. The
        default is 8020_0003h, leading to a full-range 32-bit LFSR.
        Different values may be chosen. The highest bit of the taps value
        determines how wide the forward LFSR is.

    RLFSR - Reverse LFSR variable

        Similar to the forward LFSR variable, except it runs backwards. This
        also uses the LFSRTAP variable, however the taps are shifted to the
        left once, and the least-significant bit is set to 1. In addition,
        the RLFSRTOP variable is used to get the check mask, by shifting
        left the constant 1 by RLFSRTOP binary digits places. The check mask
        is used to determine whether to XOR mask with the taps or not. The
        check mask also indicates what bit to clear in the taps in order to
        create the reverse taps.

    RLFSRTOP - Reverse LFSR top bit count

        This variable indicates what bit to check in order to determine
        whether the reverse LFSR should tap or not. It also indicates what
        bit to clear in the creation of the reverse taps. Its default is
        1Fh (31), which lends itself to a 32-bit taps value. Setting this
        to a number higher than 1Fh (31) is invalid, and may be subject to
        behaviour as yet undetermined.

11.21 RIxxy - Real 86 Mode Interrupt vectors

    These read-only variables provide access to the 86 Mode interrupt
    vectors in a more accessible format.

    The xx must be a single or two hexadecimal digits, or an index
    expression in parentheses which evaluates to a number below 256.

    The y must be one of the following letters:

     -  P - Read vector as a 16:16 segmented pointer (dword), ready for
        use as a pointer-type expression. (Actual use as a pointer-type
        expression still requires a PTR type keyword.)

     -  S - Read vector's segment. (Word.)

     -  O - Read vector's offset. (Word.)

     -  L - Read vector as a linear address. (3byte.)

11.22 FL.xF - Flag status

    These read-only variables support reading the flag status of certain
    flags.

    The x must be one letter to form one of the following names:

    CF

        Carry Flag

    PF

        Parity Flag

    AF

        Auxiliary carry Flag

    ZF

        Zero Flag

    SF

        Sign Flag

    IF

        Interrupt Flag

    DF

        Direction Flag

    OF

        Overflow Flag

    Note that the FL.xF flags are read-only. To write to a flag with the R
    command, it is valid to specify just xF as the variable name, but this
    is not valid within expressions to read the flag status. (It cannot
    be supported in expressions because some of the flag names are all
    hexadecimal digits, such as CF.)

11.23 HHRESULT - H command result

    Dword. Result of most recent H command. (If H twofold operation is used
    then the addition result is stored in the variable.)

11.24 INT8CTRL - Interrupt 8 Control pressed detection time

    Word. Number of ticks to wait with Control pressed until breaking into
    the debugger. This variable is only used if the interrupt 8 handler is
    installed. If the handler detects that Control is pressed continuously
    for this length of time while not in the debugger then the handler will
    break into the debugger. Default is set up for about 5 seconds (5 times
    18). Set to 0 to disable Control pressed detection.

11.25 Device mode variables

    DEVICEHEADER

        Dword. Read-only. Gives segmented 16:16 address of device header
        installed by the debugger. Zero if not in device mode.

    DEVICESIZE

        Word. Read-only. Gives amount of paragraphs allocated to device.
        Zero if not in device mode.

11.26 QQCODE - Q command termination return code

    Byte. Default 0. This variable is used to set the return code used by
    the debugger to terminate itself with interrupt 21h service 4Ch. This
    only happens if the debugger is in application mode and not in TSR mode.

11.27 TERMCODE - Debuggee termination return code

    Word. Debugger sets this value when it is entered from a debuggee having
    terminated. The value is what interrupt 21h service 4Dh returned.

12: Interrupt Reference
-----------------------

12.1 Mandatory interrupt hooks

     -  Interrupt 0 - Divide error

     -  Interrupt 1 - Trace

     -  Interrupt 3 - Breakpoint

     -  Interrupt 6 - Invalid opcode

     -  Interrupt 18h - Diskless boot hook

     -  Interrupt 19h - Boot load

    These interrupts are always hooked by the debugger. For the non-_DEBUG
    builds they are hooked during initialisation and the debugger attempts
    to unhook them when quitting. The highest 8 bits of the dword variable
    DCO4 control whether they are unhooked only if reachable (bits in DCO4
    zero), or forcibly so if not reachable (bits in DCO4 ones). If not
    forcibly unhooking and an interrupt handler is not reachable then the Q
    command fails.

    For DDebug, these interrupts are hooked within the run function and
    unhooked before the run function returns. This unhooking in DDebug is
    always forcible; that is, if not reachable then the interrupts are
    unhooked by simply updating the IVT entries with whatever handlers are
    stored as the next vectors in DDebug's entrypoints.

    CDebug can run in debuggable mode (like DDebug) or with debuggable mode
    disabled. If the cmd3 loop detects a change in the DCO6 flag 100h then
    it will toggle debuggable mode to match the flag. This will involve
    hooking the mandatory handlers or unhooking them (forcibly).

    As a special exception, if the debugger detects that it is running on an
    HP 95LX, then interrupt 6 is never hooked. This supports the different
    use of this software interrupt by the software or firmware on this type
    of device.

12.2 Serial interrupt

    This interrupt hook is optional. Setting the DCO flag 4000h (enable
    serial I/O) instructs the debugger to set up this interrupt hook.
    Clearing the flag or using the Q command instructs the debugger to
    unhook its handler. The DCO4 flag 1_0000h controls whether the interrupt
    unhooking is forcible (flag set) or not (flag clear).

    The exact interrupt number used as serial interrupt depends on the
    DSPVI variable at the point in time at which serial I/O is enabled. The
    default is interrupt 0Bh, corresponding to COM2.

12.3 Interrupt 2Fh - Multiplex (DPMI entrypoint)

    This interrupt is only hooked by DebugX. This interrupt hook is
    optional. Setting the DCO4 flag 2 instructs the debugger to set up this
    interrupt hook. The debugger tries to hook this interrupt if it runs
    application code in Real or Virtual 86 Mode. Clearing the flag, entering
    Protected Mode, or using the Q command instructs the debugger to unhook
    its handler. The DCO4 flag 2_0000h controls whether the interrupt
    unhooking is forcible (flag set) or not (flag clear).

    This interrupt is hooked to intercept calls to function 1687h, used to
    detect the DPMI entrypoint. DebugX attempts to hook this service to
    return its own entrypoint to the caller. The hook may fail if the DPMI
    host handles interrupt 2Fh calls before chaining to the 86 Mode handler
    chain. (MS Windows 4.x and older dosemu are reported to do this.)

12.4 Interrupt 8 - Timer

    This interrupt hook is optional. Setting the DCO4 flag 4 instructs the
    debugger to set up this interrupt hook. Clearing the flag or using the
    Q command instructs the debugger to unhook its handler. The DCO4 flag
    4_0000h controls whether the interrupt unhooking is forcible (flag set)
    or not (flag clear).

    This interrupt is used to detect the double Control-C via serial I/O
    condition. If the serial I/O handler of the debugger receives two
    Control-C keypresses while the debugger is busy running an application
    then the interrupt 8 hook will interrupt the run.

    This interrupt is also used to detect the Control pressed for 5 seconds
    condition. Similarly to the serial I/O double Control-C condition, this
    will make the debugger interrupt the current run.

12.5 Interrupt 2Dh - Alternate Multiplex Interrupt

    This interrupt hook is optional. Setting the DCO4 flag 8 or running an
    INSTALL AMIS command instructs the debugger to set up this interrupt
    hook. Clearing the flag or running UNINSTALL AMIS or using the Q command
    instructs the debugger to unhook its handler. The DCO4 flag 8_0000h
    controls whether the interrupt unhooking is forcible (flag set) or not
    (flag clear).

    This interrupt allows other programs to detect the debugger in the AMIS
    interface. The vendor string is "ecm" and the product string "lDebug".
    The description string contains the same display name and version as
    the command line help. There are two real uses of this. First, the AMIS
    function 4, which will return the list of interrupt entrypoints of the
    debugger. Second, lDebug's private AMIS functions 30h, 31h, and 33h.
    They are described in the next sections.

    This interrupt hook only succeeds if the current handler is valid.
    That is, an offset not equal to FFFFh and a segment not equal to zero.
    Another condition is that the debugger needs to detect an unused AMIS
    multiplex number to allocate. This is done automatically when hooking
    the interrupt. If either condition fails then a message is displayed and
    the debugger clears the DCO4 flag 8 on its own.

    The TRYAMISNUM variable is a writable byte variable. It defaults to 0.
    Its content is tried first when searching a free multiplex number. After
    that the debugger currently will search starting from number 0 up to
    255.

    The AMISNUM variable is a read-only byte variable. It contains the
    actually used multiplex number while the DIF4 flag 8 is set. Otherwise
    its content is not used and likely stale.

    Note that the AMIS interface is not AMIS-compliant in a few ways:

     -  The uninstall function returns 00h (not implemented).

     -  If lDDebug or lCDebug are in debuggable mode, their mandatory
        handlers will still be listed in the AMIS function 4 interrupt list
        despite not being installed. (Their downlink fields will contain
        FFFFh:FFFFh then.)

     -  If the build option _CATCHSYSREQ is enabled then the SysReq hook
        will not be listed for AMIS function 5. The interrupt 8 Control
        pressed hook is also not listed.

12.5.1 AMIS private function 30h - Update IISP Header

    This function is provided for use by our programs that use AMIS
    multiplexers and interrupt handler entrypoints with IISP headers. All
    TSRs (including RxANSI, lClock, SEEKEXT, KEEPHOOK, FDAPM, FreeDOS SHARE)
    and SHUFHOOK use this function. (The debugger itself also uses this
    function, if it is provided by another resident debugger.)

      lDebug - Update IISP Header
      INP:    al = 30h
              ds:si -> source IISP header (or pseudo header)
              es:di -> destination IISP header
      OUT:    al = FFh to indicate suppported,
               si and di both incremented by 6
               destination's ieNext field updated from source
              al != FFh if not supported,
               si and di unchanged
      CHG:    -
      REM:    This function is intended to aid in debugging
               handler re-ordering, removal, or insertion.
               The 32-bit far pointer needs to be updated
               as atomically as possible to avoid using
               an incorrect pointer.
              Test case: Run a program such as our TSRs'
               uninstaller or SHUFHOOK and step through it
               with "tp fffff" when operating on something
               crucial such as interrupt 21h. Without this
               function the machine will crash!
              To enable this function to be called, first run
               the command "r dco4 or= 8", or "INSTALL AMIS"
                (install our AMIS multiplexer handler).
              Other workaround: Use SILENT for TP and disable
               DCO3 flag 4000_0000 (do not call int 21.0B to
               check for Ctrl-C status).
              Yet another workaround: Set flag DCO 8 (enable
               fake InDOS mode, avoid calling int 21h).
      REM:    The source may be a pseudo IISP header. In this
               case the ieEntry field should hold 0FEEBh
               (jmp short $) and the ieSignature field
               should indicate the source, eg "VT" for the IVT
               or "NH" for inserting a New Handler.

12.5.2 AMIS private function 31h - Install DPMI entrypoint hook

    This function is for use by lDDebugX (or lCDebugX). It instructs lDebugX
    (or lCDebugX) to install its DPMI entrypoint hook. It is called by the
    debuggable debugger right before it tries to install its own hook. Non-
    zero return values in AL indicate the function is supported. A return
    value of 0FFh in AL indicates success. Other non-zero return values
    indicate that no hook occurred. Non-DPMI builds of lDebug return zero.
    This function should be called only while the InDOS flag is zero.

      lDebugX - Install DPMI hook
      INP:    al = 31h
      OUT:    al = FFh if installed
              al = FEh..F0h if not installed but call is supported
              al = 00h if not supported
      CHG:    -
      STT:    not in DOS

12.5.3 AMIS private function 32h - Reserved for lDebugX

      lDebugX - Reserved
      INP:    al = 32h

12.5.4 AMIS private function 33h - Install fault areas

    This function is by default provided by lDebugX (including the variants
    lCDebugX and lDDebugX) and is for use by lDDebugX as well as lCDebugX
    (in debuggable mode). It is called when the debuggable debugger is
    instructed to INSTALL AREAS.

      lDebugX - Install fault areas
      INP:    al = 33h
              dx:bx -> fault area structure of client
      OUT:    al = FFh if installed
              al = FEh..01h if not installed but call is supported
              al = 00h if not supported
      CHG:    al, bx, cx, dx, si, di, es, ds
      REM:    The area structure is defined in the lDebug sources'
               debug.mac file. The first 32 bytes of the structure
               start with a signature word, which is equal to the
               word value CBF9h (encoding the instruction sequence
               of stc \ retf) if the structure is not currently
               installed into any debugger. The remainder of the
               32 bytes, as well as the details of how the first
               two bytes are used otherwise, are private to the
               debugger that provides this service (the server).
              The area structure may be far-called in 86 Mode. The
               only currently defined function (in al) for this call
               is function 00h, which attempts to uninstall the area
               structure which is being called. It is valid for
               either the server or the client to uninstall an
               area structure if they so wish.
              The fields of the structure behind the first 32 bytes
               point to a number of sub-structures and area function
               lists and area lists. All of these structures are
               to be accessed using the same segment as the main
               area structure. They contain linear start and linear
               end addresses, which the client sets up before it
               tries to install the areas. The linear start address
               is also assumed to point to the segment base address
               which is used as the reference for the area functions
               and areas. (They do not have to match the offset part
               actually used to run the code, but the lists must be
               based on the linear start address.)

13: Service Reference
---------------------

    These are the services called by the debugger.

13.1 Interrupt 10h

    Used for output while InDOS, DCO flag 8 set, or bootloaded.

    Function 02h

        Set cursor position (only used if highlighting)

    Function 03h

        Get cursor position (only used if highlighting, indicates to
        highlight to int 10h if supported)

    Function 08h

        Get video attribute (only used if highlighting)

    Function 09h

        Set video attribute (only used if highlighting)

    Function 0Eh

        Teletype output

    Function 0Fh

        Get video mode and page

13.2 Interrupt 16h

    Used for input while InDOS, DCO flag 8 set, or bootloaded.

    Function 00h

        Read keypress (wait until keypress available, consume it)

    Function 01h

        Read keypress (return if no keypress available, retain it if any)

13.3 Interrupt 2Fh

    Function 1261h

        PTS-DOS: Get first UMCB

    Function 1680h

        Idle (Release timeslice to multitasker)

    Function 1687h

        Get DPMI entrypoint (used and hooked by lDebugX)

    Function 4300h, 4310h

        XMS detection and get entrypoint

    Function 4A06h

        RPL adjust base memory size (called by booted debugger if RPL
        signature present)

13.4 Interrupt 12h

    Called by booted debugger to determine base memory size.

13.5 Protected Mode Interrupt 31h

    Used by lDebugX while in Protected Mode.

    Function 0000h

        Allocate LDT descriptor

    Function 0001h

        Free LDT descriptor

    Function 0002h

        Get selector from segment

    Function 0003h

        Get next selector increment value

    Function 0006h

        Get segment base

    Function 0007h

        Set segment base

    Function 0008h

        Set segment limit

    Function 0009h

        Set descriptor access rights

    Function 000Ah

        Create alias descriptor

    Function 000Bh

        Get descriptor

    Function 000Ch

        Set descriptor

    Function 0200h

        Get 86M interrupt vector

    Function 0201h

        Set 86M interrupt vector

    Function 0202h

        Get PM exception vector

    Function 0203h

        Set PM exception vector

    Function 0204h

        Get PM interrupt vector

    Function 0205h

        Set PM interrupt vector

    Function 0300h

        Call Real/Virtual 86 Mode interrupt

    Function 0301h

        Call Real/Virtual 86 Mode far function

    Function 0305h

        Get raw mode switch save state addresses

    Function 0306h

        Get raw mode switch addresses

    Function 0900h

        Disable Virtual Interrupt Flag

    Function 0901h

        Enable Virtual Interrupt Flag

    Function 0902h

        Get Virtual Interrupt Flag

13.6 Protected Mode Interrupt 2Fh

    Function 1680h

        Idle (Release timeslice to multitasker)

    Function 168Ah

        Determine whether DOS extender is available.

13.7 Protected Mode Interrupt 21h

    Function 7305h

        Read/write sectors from/to DOS drive. Used to implement L and W
        command.

    Function 4Ch

        Terminate DPMI client and process

13.8 Protected Mode Interrupt 25h

    Read sectors from DOS drive. Used to implement L command.

13.9 Protected Mode Interrupt 26h

    Write sectors to DOS drive. Used to implement W command.

13.10 Interrupt E6h

    Function bx = 0, ax = -1

        Used by booted debugger to implement BOOT QUIT command when running
        in dosemu2.

13.11 Interrupt 15h

    Function 87h

        Used by DX command to read memory.

    Function 5301h, 530Eh, 5307h

        Used by booted debugger to implement BOOT QUIT command when running
        in qemu.

    Function 4DD4h, bx = 0

        Detect HP 95LX

13.12 Interrupt 13h

    Used by the booted debugger to load scripts or kernel executables.

    Function 00h

        Reset disk system

    Function 02h

        Read sector with CHS addressing

    Function 03h

        Write sector with CHS addressing

    Function 08h

        Query CHS geometry

    Function 41h

        Detect LBA extensions support

    Function 42h

        Read sector with LBA

    Function 43h

        Write sector with LBA

13.13 Interrupt 19h

    Boot load. Used if booting the debugger fails.

13.14 Interrupt 2Dh

    Used to access Alternate Multiplex Interrupt Specification TSRs. Can be
    used while bootloaded too.

    Function 00h

        Installation check. Determines whether an AMIS number is in use.

    Function 04h

        Determine chained interrupts. Determines interrupt entrypoints.

    AMIS private functions 30h, 31h, 33h of lDebug (refer to section 12.5)

13.15 Interrupt 25h

    Read sectors from DOS drive. Used to implement L command. Only used if
    the debugger is loaded as a DOS application.

13.16 Interrupt 26h

    Write sectors to DOS drive. Used to implement W command. Only used if
    the debugger is loaded as a DOS application.

13.17 Interrupt 21h

    DOS services. Only used while not InDOS. (Only used if the debugger is
    loaded as a DOS application.)

    Function 08h

        Get standard input keypress

    Function 0Ah

        Line buffered standard input

    Function 0Bh

        Check standard input available / Check Control-C

    Function 19h

        Get default drive

    Function 25h

        Set interrupt vector

    Function 29h

        Parse filename

    Function 3000h

        Get DOS version

    Function 3306h

        Get true DOS version

    Function 34h

        Get InDOS flag address

    Function 35h

        Get interrupt vector

    Function 3700h

        Get switch character

    Function 3Ch

        Create file

    Function 3Dh

        Open file

    Function 3Eh

        Close file

    Function 3Fh

        Read from file

    Function 40h

        Write to file (Used to write to stdout too)

    Function 41h

        Delete file

    Function 42h

        Seek in file

    Function 45h

        Duplicate file handle

    Function 4400h

        Used in initialisation to determine whether handle is to a device

    Function 440Dh

        Used to lock and unlock drives by L or W commands

    Function 48h

        Allocate memory

    Function 4Ah

        Resize memory

    Function 4B01h

        Load executable and return to debugger

    Function 4Ch

        Terminate process

    Function 4Dh

        Get process return code

    Function 50h

        Set PSP

    Function 51h

        Get PSP

    Function 52h

        Get List of Lists

    Function 55h

        Create child PSP

    Function 58h

        Get or set memory allocation strategy and UMB link status

    Function 5D06h

        Get DOS SDA address (used to switch active PSP)

    Function 6Ch

        Extended open/create

    Function 716Ch

        Extended open/create with LFN

    Function 71A0h

        Get LFN volume information

    Function 7305h

        Read/write sectors from/to DOS drive. Used to implement L and W
        command.

13.18 Interrupt 67h

    EMS services. Used by X commands.

14: Command help
----------------

14.1 lDebug help

      lDebug (YYYY-MM-DD), debugger.
      
      Usage: LDEBUG[.COM] [/C=commands] [[drive:][path]progname.ext [parameters]]
      
      /C=commands   semicolon-separated list of commands (quote spaces)
      /IN           discard command line buffer, do not run config
      /A=MAX        expand auxiliary buffer to maximum, 24576 Bytes
      /A=MIN        restrict auxiliary buffer to minimum, 8208 Bytes
      /A=number     set auxiliary buffer size to number of bytes
      /A            alias for /A=MAX
      /B            run a breakpoint within initialisation
      /F[+|-]       always treat executable file as a flat binary
      /E[+|-]       for flat binaries set up Stack Segment != PSP
      /V[+|-]       enable/disable video screen swapping
      progname.ext  (executable) file to debug or examine
      parameters    parameters given to program
      
      For a list of debugging commands, run LDEBUG and type ? at the prompt.

14.2 INSTSECT help

      INSTSECT: Install boot sectors. 2018 by C. Masloch
      
      Usage of the works is permitted provided that this
      instrument is retained with the works, so that any entity
      that uses the works is notified of this instrument.
      
      DISCLAIMER: THE WORKS ARE WITHOUT WARRANTY.
      
      Options:
      
      a:              load or update boot sectors of specified drive
      /M=filename     operate on FS image file instead of drive
      /MN             operate on drive instead of image file (default)
      /MS=number      set sector size of FS image file (default 512)
      /MO=number      set offset in image file in bytes (default 0)
      /MOx=number     set offset (x = S sectors, K 1024, M 1024 * 1024)
      
      /Fx=filename    replace Xth name in the boot sector, X = 1 to 4
      /F=filename     alias to /F1=filename
      
      /U KEEP         keep default/current boot unit handling (default)
      /U AUTO         patch boot loader to use auto boot unit handling
      /U xx           patch boot loader to use XXh as a fixed unit
      
      /P KEEP         keep default/current part info handling (default)
      /P AUTO         patch boot loader to use auto part info handling
      /P NONE         patch boot loader to use fixed part info
      
      /Q KEEP         keep default/current query geometry handling (default)
      /Q AUTO         patch boot loader to use auto query geometry handling
      /Q NONE         patch boot loader to use fixed geometry
      
      /L KEEP         keep default/current LBA handling (default)
      /L AUTO         patch boot loader to use auto LBA handling
      /L AUTOHDD      patch boot loader to use auto LBA (HDD-only) handling
      /L NONE         patch boot loader to use only CHS
      
      /SR             do not read boot sector from source file (default)
      /S=filename     read boot sector loader from source file
      /S12=filename   as /S=filename but only for FAT12 (also /S16, /S32)
      /SV             validate boot sector jump and FS ID (default)
      /SN             do not validate boot sector jump and FS ID
      
      /BS             write boot sector to drive's boot sector (default)
      /B=filename     write boot sector to file, not to drive
      /BN             do not write boot sector
      /BR             replace boot sector loader with built-in one (default)
      /BO             keep original boot sector
      /BC             restore boot sector from backup copy
      
      Only applicable for FAT32 with sector size below or equal to 512 bytes:
      
      /IS             write FSIBOOT to drive's FSINFO sector (default)
      /I=filename     write FSIBOOT to file, not to drive
      /IB             write FSIBOOT to boot sector file (see /B=filename)
      /IN             do not write FSIBOOT
      /IR             replace reserved field with built-in FSIBOOT (default)
      /IO             keep original reserved fields (including FSIBOOT area)
      /IC             restore FSINFO from backup copy
      /IZ             zero out reserved fields (including FSIBOOT area)
      /II             leave invalid FSINFO structure
      /IV             make valid FSINFO if there is none (default)
      
      Only applicable for FAT32:
      
      /C              force writing to backup copies
      /CB             force writing sector to backup copy
      /CI             force writing info to backup copy
      /CN             disable writing to backup copies
      /CNB            disable writing sector to backup copy
      /CNI            disable writing info to backup copy
      /CS             only write backup copies if writing sectors (default)
      /CSB            only write sector to backup copy if writing sector
      /CSI            only write info to backup copy if writing sector

15: Online help pages
---------------------

15.1 ? - Main online help

      lDebug (YYYY-MM-DD) help screen
      assemble        A [address]
      set breakpoint  BP index|AT|NEW address
                        [[NUMBER=]number] [WHEN=cond] [ID=id]
       set ID         BI index|AT address [ID=]id
       set condition  BW index|AT address [WHEN=]cond
       set offset     BO index|AT address [OFFSET=]number
       set number     BN index|AT address|ALL number
       clear          BC index|AT address|ALL
       disable        BD index|AT address|ALL
       enable         BE index|AT address|ALL
       toggle         BT index|AT address|ALL
       swap           BS index1 index2
       list           BL [index|AT address|ALL]
      compare         C range address
      dump            D [range]
      dump bytes      DB [range]
      dump words      DW [range]
      dump dwords     DD [range]
      dump interrupts DI[R][M][L] interrupt [count]
      dump MCB chain  DM [segment]
      display strings DZ/D$/D[W]# [address]
      dump text table DT [T] [number]
      enter           E [address [list]]
      fill            F range [RANGE range|list]
      go              G [=address] [breakpts]
      goto            GOTO :label
      hex add/sub     H value1 [value2 [...]]
      base display    H BASE=number [GROUP=number] [WIDTH=number] value
      input           I[W|D] port
      if numeric      IF [NOT] (cond) THEN cmd
      if script file  IF [NOT] EXISTS Y file [:label] THEN cmd
      load program    L [address]
      load sectors    L address drive sector count
      move            M range address
      80x86/x87 mode  M [0..6|C|NC|C2|?]
      set name        N [[drive:][path]progname.ext [parameters]]
      set command     K [[drive:][path]progname.ext [parameters]]
      output          O[W|D] port value
      proceed         P [=address] [count [WHILE cond] [SILENT [count]]]
      quit            Q
      quit process    QA
      quit and break  QB
      register        R [register [value]]
      Run R extended  RE
      RE commands     RE.LIST|APPEND|REPLACE [commands]
      Run Commandline RC
      RC commands     RC.LIST|APPEND|REPLACE [commands]
      MMX register    RM [BYTES|WORDS|DWORDS|QWORDS]
      FPU register    RN
      toggle 386 regs RX
      search          S range [REVERSE] [SILENT number] [RANGE range|list]
      sleep           SLEEP count [SECONDS|TICKS]
      trace           T [=address] [count [WHILE cond] [SILENT [count]]]
      trace (exc str) TP [=address] [count [WHILE cond] [SILENT [count]]]
      trace mode      TM [0|1]
      enter TSR mode  TSR
      unassemble      U [range]
      view screen     V [ON|OFF [KEEP|NOKEEP]]
      write program   W [address]
      write sectors   W address drive sector count
      expanded mem    XA/XD/XM/XR/XS, X? for help
      run script      Y [partition/][scriptfile] [:label]
      
      Additional help topics:
       Registers      ?R
       Flags          ?F
       Conditionals   ?C
       Expressions    ?E
       Variables      ?V
       R Extended     ?RE
       Run keywords   ?RUN
       Options pages  ?OPTIONS
       Options        ?O
       Boot loading   ?BOOT
       lDebug build   ?BUILD
       lDebug build   ?B
       lDebug sources ?SOURCE
       lDebug license ?L

15.2 ?R - Registers

      Available 16-bit registers:             Available 32-bit registers: (386+)
      AX      Accumulator                     EAX
      BX      Base register                   EBX
      CX      Counter                         ECX
      DX      Data register                   EDX
      SP      Stack pointer                   ESP
      BP      Base pointer                    EBP
      SI      Source index                    ESI
      DI      Destination index               EDI
      DS      Data segment
      ES      Extra segment
      SS      Stack segment
      CS      Code segment
      FS      Extra segment 2 (386+)
      GS      Extra segment 3 (386+)
      IP      Instruction pointer             EIP
      FL      Flags                           EFL

    Enter ?F to display the recognized flags.

15.3 ?F - Flags

    Recognized flags:

      Value   Name                      Set                     Clear
      0800  OF  Overflow Flag         OV  Overflow            NV  No overflow
      0400  DF  Direction Flag        DN  Down                UP  Up
      0200  IF  Interrupt Flag        EI  Enable interrupts   DI  Disable interrupts
      0080  SF  Sign Flag             NG  Negative            PL  Plus
      0040  ZF  Zero Flag             ZR  Zero                NZ  Not zero
      0010  AF  Auxiliary Flag        AC  Auxiliary carry     NA  No auxiliary carry
      0004  PF  Parity Flag           PE  Parity even         PO  Parity odd
      0001  CF  Carry Flag            CY  Carry               NC  No carry

    The short names of the flag states are displayed when dumping registers
    and can be entered to modify the symbolic F register with R. The short
    names of the flags can be modified by R.

15.4 ?C - Conditionals

    In the register dump displayed by the R, T, P and G commands,
    conditional jumps are displayed with a notice that shows whether the
    instruction will cause a jump depending on its condition and the current
    register and flag contents. This notice shows either "jumping" or "not
    jumping" as appropriate.

    The conditional jumps use these conditions: (second column negates)

       jo             jno             OF
       jc jb jnae     jnc jnb jae     CF
       jz je          jnz jne         ZF
       jbe jna        jnbe ja         ZF||CF
       js             jns             SF
       jp jpe         jnp jpo         PF
       jl jnge        jnl jge         OF^^SF
       jle jng        jnle jg         OF^^SF || ZF
       j(e)cxz                        (e)cx==0
       loop                           (e)cx!=1
       loopz loope                    (e)cx!=1 && ZF
       loopnz loopne                  (e)cx!=1 && !ZF

    Enter ?F to display a description of the flag names.

15.5 ?E - Expressions

    Recognized operators in expressions:

      |       bitwise OR              ||      boolean OR
      ^       bitwise XOR             ^^      boolean XOR
      &       bitwise AND             &&      boolean AND
      >>      bit-shift right         >       test if above
      >>>     signed bit-shift right  <       test if below
      <<      bit-shift left          >=      test if above-or-equal
      ><      bit-mirror              <=      test if below-or-equal
      +       addition                ==      test if equal
      -       subtraction             !=      test if not equal
      *       multiplication          =>      same as >=
      /       division                =<      same as <=
      %       modulo (A-(A/B*B))      <>      same as !=
      **      power

    Implicit operater precedence is handled in the listed order, with
    increasing precedence: (Brackets specify explicit precedence of an
    expression.)

       boolean operators OR, XOR, AND (each has a different precedence)
       comparison operators
       bitwise operators OR, XOR, AND (each has a different precedence)
       shift and bit-mirror operators
       addition and subtraction operators
       multiplication, division and modulo operators
       power operator

    Recognized unary operators: (modifying the next number)

      +       positive (does nothing)
      -       negative
      ~       bitwise NOT
      !       boolean NOT
      ?       absolute value
      !!      convert to boolean

    Note that the power operator does not affect unary operator handling.
    For instance, "- 2 ** 2" is parsed as "(-2) ** 2" and evaluates to 4.

    Although a negative unary and signed bit-shift right operator
    are provided the expression evaluator is intrinsically unsigned.
    Particularly the division, multiplication, modulo and all comparison
    operators operate unsigned. Due to this, the expression "-1 < 0"
    evaluates to zero.

    Recognized terms in an expression:

       32-bit immediates
       8-bit registers
       16-bit registers including segment registers (except FS, GS)
       32-bit compound registers made of two 16-bit registers (eg DXAX)
       32-bit registers and FS, GS only if running on a 386+
       32-bit variables V00..VFF
       32-bit special variables DCO, DCS, DAO, DAS, DIF, DPI, PPI
       16-bit special variables DPR, DPP, PSP, PPR
        (fuller variable reference in the manual)
       byte/word/3byte/dword memory content (eg byte [seg:ofs], where both the
        optional segment as well as the offset are expressions too)

    The expression evaluator case-insensitively checks for names of
    variables and registers as well as size specifiers.

    Enter ?R to display the recognized register names. Enter ?V to display
    the recognized variables.

15.6 ?V - Variables

    Available lDebug variables:

     -  V0..VF User-specified usage

     -  DCO Debugger Common Options

     -  DAO Debugger Assembler/disassembler Options

    The following variables cannot be written:

     -  PSP Debuggee Process

     -  PPR Debuggee's Parent Process

     -  PPI Debuggee's Parent Process Interrupt 22h

     -  DIF Debugger Internal Flags

     -  DCS Debugger Common Startup options

     -  DAS Debugger Assembler/disassembler Startup options

     -  DPR Debugger Process

     -  DPP Debugger's Parent Process (zero in TSR mode)

     -  DPI Debugger's Parent process Interrupt 22h (zero in TSR mode)

    Enter ?O to display the options and internal flags.

15.7 ?RE - R Extended

    The RUN commands (T, TP, P, G) and the RE command use the RE command
    buffer to run commands. Most commands are allowed to be run from the
    RE buffer. Disallowed commands include program-loading L, A, E that
    switches the line input mode, TSR, Q, Y, RE, and further RUN commands.
    When the RE buffer is used as input during T, TP, or P with either of
    the WHILE or SILENT keywords, commands that use the auxbuff are also
    disallowed and will emit an error noting the conflict.

    RE.LIST shows the current RE buffer contents in a format usable by the
    other RE commands. RE.APPEND appends the following commands to the
    buffer, if they fit. RE.REPLACE appends to the start of the buffer. When
    specifying commands, an unescaped semicolon is parsed as a linebreak
    to break apart individual commands. Backslashes can be used to escape
    semicolons and backslashes themselves.

    Prefixing a line with an @ (AT sign) causes the command not to be shown
    to the standard output of the debugger when run. Otherwise, the command
    will be shown with a percent sign % or ~% prompt.

    The default RE buffer content is @R. This content is also detected and
    handled specifically; if found as the only command the handler directly
    calls the register dump implementation without setting up and tearing
    down the special execution environment used to run arbitrary commands
    from the RE buffer.

15.8 ?RUN - Run keywords

    T (trace), TP (trace except proceed past string operations), and P
    (proceed) can be followed by a number of repetitions and then the
    keyword WHILE, which must be followed by a conditional expression.

    The selected run command is repeated as many times as specified by the
    number, or until the WHILE condition evaluates no longer to true.

    After the number of repetitions or (if present) after the WHILE
    condition the keyword SILENT may follow. If that is the case, all
    register dumps done during the run are buffered by the debugger and the
    run remains silent. After the run, the last dumps are replayed from the
    buffer and displayed. At most as many dumps as fit into the buffer are
    displayed. (The buffer is currently up to 8 KiB sized.)

    If a number follows behind the SILENT keyword, only at most that many
    dumps are displayed from the buffer. The dumps that are displayed are
    always those last written into the buffer, thus last occurred.

15.9 ?OPTIONS - Options pages

    Enter one of the following commands to get a corresponding help page:

     -  ?O1 DCO1 - Options

     -  ?O2 DCO2 - More Options

     -  ?O3 DCO3 - More Options

     -  ?O4 DCO4 - Interrupt Hooking Options

     -  ?O6 DCO6 - More Options

     -  ?OI DIF - Internal Flags

     -  ?OA DAO - Assembler/Disassembler Options

15.10 ?O - Options

    Available options: (read/write DCO, read DCS)

     -  0001 RX: 32-bit register display

     -  0002 TM: trace into interrupts

     -  0004 allow dumping of CP-dependant characters

     -  0008 always assume InDOS flag non-zero, to debug DOS or TSRs

     -  0010 disallow paged output to StdOut

     -  0020 allow paged output to non-StdOut

     -  0040 display raw hexadecimal content of FPU registers

     -  0100 when prompting during paging, do not use DOS for input

     -  0200 do not execute HLT instruction to idle

     -  0400 do not idle, the keyboard BIOS idles itself

     -  0800 use getinput function for int 21h interactive input

     -  1000 in disp_*_size use SI units (kB = 1000, etc). overrides 2000!

     -  2000 in disp_*_size use JEDEC units (KB = 1024)

     -  4000 enable serial I/O (port 02F8h interrupt 0Bh)

     -  8000 disable serial I/O when breaking after 5 seconds Ctrl pressed

     -  0001_0000 gg: do not skip a breakpoint (bb or gg)

     -  0002_0000 gg: do not auto-repeat

     -  0004_0000 T/TP/P: do not skip a (bb) breakpoint

     -  0008_0000 gg: do not auto-repeat after bb hit

     -  0010_0000 T/TP/P: do not auto-repeat after bb hit

     -  0020_0000 gg: do not auto-repeat after unexpectedinterrupt

     -  0040_0000 T/TP/P: do not auto-repeat after unexpectedinterrupt

     -  0080_0000 S: do not dump data after matches

     -  1000_0000 R: do not repeat disassembly

     -  2000_0000 R: do not show memory reference in disassembly

     -  4000_0000 quiet command line buffer input

     -  8000_0000 quiet command line buffer output

    More options: (read/write DCO2, read DCS2)

     -  0001 DB: show header

     -  0002 DB: show trailer

     -  0010 DW: show header

     -  0020 DW: show trailer

     -  0100 DD: show header

     -  0200 DD: show trailer

     -  0800 use getinput function for int 21h interactive input in DPMI

     -  1000 H: stay compatible to MS-DOS Debug

     -  2000 idle and check for Ctrl-C in getc

     -  4000 idle and check for Ctrl-C in getc in DPMI

     -  8000 T/TP/P/G: cancel run after RE command buffer execution

     -  01_0000 N: operate in MS Debug style instead of K command alike

     -  02_0000 N: capitalise command line tail

     -  04_0000 explicit 0-length ranges operate in partial MS Debug style

     -  08_0000 R: 16-bit 80-column register dump in MS Debug style

     -  10_0000 R: do variable prompts in MS Debug style

     -  20_0000 R: do variable prompts with underscore separator

     -  40_0000 display linebreak before R command register dump

    More options: (read/write DCO3, read DCS3)

     -  0001 T: do not page output

     -  0002 TP: do not page output

     -  0004 P: do not page output

     -  0008 G: do not page output

     -  0100 T/TP/P: modify paging for silent dump

     -  0200 T/TP/P: if 0100 set: turn paging on, else off

     -  01_0000 R: highlight changed digits (needs ANSI for DOS output)

     -  02_0000 R: highlight escape sequences to int 10h, else video
        attributes

     -  04_0000 R: highlight changed registers (overrides 01_0000)

     -  08_0000 R: include highlighting of EIP

     -  10_0000 set PM ss B bit

     -  20_0000 break on entering Protected Mode

     -  0100_0000 highlight prefix/suffix in getinput if text parts are not
        visible

     -  0200_0000 do not call int 2F.1680 for idling

     -  0400_0000 delay for a tick before writing breakpoints

     -  0800_0000 do not call other lDebug instance's Update IISP Header
        call

     -  1000_0000 disable auto-repeat

     -  2000_0000 check int 16h buffer for Control-C if inputting from int
        16h

     -  4000_0000 call DOS service 0Bh to check for Control-C

     -  8000_0000 when Q command is used while TSR, leave TF as is

    More options: (read/write DCO4, read DCS4)

     -  0002 enable interrupt 2Fh hook while in 86 Mode

     -  0004 enable interrupt 8 hook

     -  0008 enable interrupt 2Dh hook

     -  0001_0000 force serial interrupt unhooking

     -  0002_0000 force interrupt 2Fh unhooking

     -  0004_0000 force interrupt 8 unhooking

     -  0008_0000 force interrupt 2Dh unhooking

     -  0100_0000 force interrupt 0 unhooking

     -  0200_0000 force interrupt 1 unhooking

     -  0400_0000 force interrupt 3 unhooking

     -  0800_0000 force interrupt 6 unhooking

     -  1000_0000 force interrupt 18h unhooking

     -  2000_0000 force interrupt 19h unhooking

    More options: (read/write DCO6, read DCS6)

     -  0001 enable video screen swapping

     -  0002 keep video screen when disabling swapping

     -  0010 read key from interrupt 16h when swapping (V command)

     -  0100 enable debug mode (and BU command)

     -  0200 use ROM-BIOS output even when DOS available

     -  0400 load and write .EXE and .COM files like flat .BIN files (/F+)

     -  0800 for loading flat .BIN files set up Stack Segment != PSP (/E+)

     -  1000 enable 40-column friendly mode

     -  2000 in 40-column mode indent odd D lines more

     -  4000 in 40-column mode display dashes at half of D length

     -  01_0000 allow to share serial IRQ handler

     -  0100_0000 use ROM-BIOS I/O even when DOS available (disables script
        file read)

     -  2000_0000 display flags in style 2 for R command register dump

     -  4000_0000 display flags in style 3 for R command register dump

     -  8000_0000 linebreak before R register dump if not column 0 (int 10h
        only)

    Internal flags: (read DIF)

     -  00_0001 Int25/Int26 packet method available

     -  00_0002 Int21.7305 packet method available

     -  00_0004 VDD registered and usable

     -  00_0008 internal flag for paged output

     -  00_0010 DEBUG's input isn't StdIn

     -  00_0020 DEBUG's input is a file

     -  00_0040 DEBUG's output isn't StdOut

     -  00_0080 DEBUG's output is a file

     -  00_1000 state of debuggee's A20

     -  00_2000 state of debugger's A20 (not implemented: same as previous)

     -  00_4000 debugger booted independent of a DOS

     -  00_8000 CPU is at least a 386 (32-bit CPU)

     -  01_0000 internal flag for tab output processing

     -  02_0000 running inside NTVDM

     -  10_0000 internal flag for paged output

     -  40_0000 in TSR mode (detached debugger process)

     -  0100_0000 running inside dosemu

     -  0400_0000 T/TP/P: while condition specified

     -  0800_0000 TP: P specified (proceed past string ops)

     -  1000_0000 T/TP/P: silent mode (SILENT specified)

     -  2000_0000 T/TP/P: silent mode is active, writing to silent buffer

    Available assembler/disassembler options: (read/write DAO, read DAS)

     -  01 Disassembler: lowercase output

     -  02 Disassembler: output blank behind comma

     -  04 Disassembler: output addresses in NASM syntax

     -  08 Disassembler: lowercase referenced memory location segreg

     -  10 Disassembler: always show SHORT keyword

     -  20 Disassembler: always show NEAR keyword

     -  40 Disassembler: always show FAR keyword

     -  80 Disassembler: NEC V20 repeat rules (for segregs)

     -  0100 Disassembler: 40-column friendly mode (only 4 bytes machine
        code per line)

     -  0200 Disassembler: do not indent disassembly operands

     -  0400 Disassembler: MS Debug style opcode field width

     -  1000 Disassembler: access data in a16 referenced memory operand

     -  2000 Disassembler: access data in a32 referenced memory operand

     -  4000 Disassembler: simulate repeated a16 scas/cmps string operation

     -  8000 Disassembler: simulate repeated a32 scas/cmps string operation

15.11 ?BOOT - Boot loading

    Boot loading commands:

     -  BOOT LIST HDA

     -  BOOT DIR [partition] [dirname]

     -  BOOT READ|WRITE [partition] segment [[HIDDEN=sector] sector] [count]

     -  BOOT QUIT [exits dosemu or shuts down using APM]

     -  BOOT [PROTOCOL=SECTOR] partition

     -  BOOT PROTOCOL=proto [opt] [partition] [filename1] [filename2]
        [cmdline]

     -  the following partitions may be specified:

         -  HDAnum first hard disk, num = partition (1-4 primary, 5+
            logical)

         -  HDBnum second hard disk (etc), num = partition

         -  HDA first hard disk (only valid for READ|WRITE|PROTOCOL=SECTOR)

         -  FDA first floppy disk

         -  FDB second floppy disk (etc)

         -  LDP partition the debugger loaded from

         -  YDP partition the most recent Y command loaded from

         -  SDP last used partition (default if no partition specified)

         -  filename2 may be double-slash // for none

         -  cmdline is only valid for lDOS, RxDOS.2, RxDOS.3 protocols

         -  files' directory entries are loaded to 500h and 520h

    Available protocols: (default filenames, load segment, then entrypoint)

     -  LDOS LDOS.COM or L[D]DEBUG.COM at 200h, 0:400h

     -  FREEDOS KERNEL.SYS or METAKERN.SYS at 60h, 0:0

     -  DOSC IPL.SYS at 2000h, 0:0

     -  EDRDOS DRBIO.SYS at 70h, 0:0

     -  MSDOS6 IO.SYS + MSDOS.SYS at 70h, 0:0

     -  MSDOS7 IO.SYS at 70h, 0:200h

     -  IBMDOS IBMBIO.COM + IBMDOS.COM at 70h, 0:0

     -  NTLDR NTLDR at 2000h, 0:0

     -  BOOTMGR BOOTMGR at 2000h, 0:0

     -  RXDOS.0 RXDOSBIO.SYS + RXDOS.SYS at 70h, 0:0

     -  RXDOS.1 RXBIO.SYS + RXDOS.SYS at 70h, 0:0

     -  RXDOS.2 RXDOS.COM at 70h, 0:400h

     -  RXDOS.3 RXDOS.COM at 200h, 0:400h

     -  CHAIN BOOTSECT.DOS at 7C0h, -7C0h:7C00h

     -  SECTOR (default) load partition boot sector or MBR

     -  SECTORALT as SECTOR, but entry at 07C0h:0

    Available options:

     -  MINPARA=num load at least that many paragraphs

     -  MAXPARA=num load at most that many paragraphs (0 = as many as fit)

     -  SEGMENT=num change segment at that the kernel loads

     -  ENTRY=[num:]num change entrypoint (CS (relative) : IP)

     -  BPB=[num:]num change BPB load address (segment -1 = auto-BPB)

     -  CHECKOFFSET=num set address of word to check, must be even

     -  CHECKVALUE=num set value of word to check (0 = no check)

    Boolean options: [opt=bool]

     -  SET_DL_UNIT set dl to load unit

     -  SET_BL_UNIT set bl to load unit

     -  SET_SIDI_CLUSTER set si:di to first cluster

     -  SET_DSSI_DPT set ds:si to DPT address

     -  PUSH_DPT push DPT address and DPT entry address

     -  DATASTART_HIDDEN add hidden sectors to datastart var

     -  SET_AXBX_DATASTART set ax:bx to datastart var

     -  SET_DSBP_BPB set ds:bp to BPB address

     -  LBA_SET_TYPE set LBA partition type in BPB

     -  MESSAGE_TABLE provide message table pointed to at 1EEh

     -  SET_AXBX_ROOT_HIDDEN set ax:bx to root start with hidden sectors

     -  NO_BPB do not load BPB

     -  SET_DSSI_PARTINFO load part table to 600h, point ds:si + ds:bp to it

     -  CMDLINE pass a kernel command line (recent FreeDOS extension)

15.12 ?BUILD - lDebug build (only revisions)

      lDebug (YYYY-MM-DD)
      Source Control Revision ID: hg xxxxxxxxxxxx (vvvv ancestors)
      Uses yyyyyyyy: Revision ID hg zzzzzzzzzzzz (www ancestors)
      [etc]

15.13 ?B - lDebug build (with options)

      lDebug (YYYY-MM-DD)
      Source Control Revision ID: hg xxxxxxxxxxxx (vvvv ancestors)
      Uses yyyyyyyy: Revision ID hg zzzzzzzzzzzz (www ancestors)
      [etc]
      
      DI command
      DM command
      D string commands
      S match dumps line of following data
      RN command
      Access SDA current PSP field
      Load NTVDM VDD for sector access
      X commands for EMS access
      RM command and reading MMX registers as variables
      Expression evaluator
       Indirection in expressions
      Variables with user-defined purpose
      Debugger option and status variables
      PSP variables
      Conditional jump notice in register dump
      TSR mode (Process detachment)
      Boot loader
      Permanent breakpoints
      Intercepted interrupts: 00, 01, 03, 06, 18, 19
      Extended built-in help pages

15.14 ?X - EMS commands

      Expanded memory (EMS) commands:
        Allocate      XA count
        Deallocate    XD handle
        Map memory    XM logical-page physical-page handle
        Reallocate    XR handle count
        Show status   XS

15.15 ?SOURCE - lDebug source reference

    The original lDebug sources can be obtained from the repo located at
    https://hg.pushbx.org/ecm/ldebug (E. C. Masloch's repo)

    Releases of lDebug are available via the website at
    https://pushbx.org/ecm/web/#projects-ldebug

    The most recent manual is hosted at https://pushbx.org/ecm/doc/ in the
    files ldebug.htm, ldebug.txt, and ldebug.pdf

15.16 ?L - lDebug license

    lDebug - libre 86-DOS debugger

     -  Copyright (C) 1995-2003 Paul Vojta

     -  Copyright (C) 2008-2021 C. Masloch

    Usage of the works is permitted provided that this instrument is
    retained with the works, so that any entity that uses the works is
    notified of this instrument.

    DISCLAIMER: THE WORKS ARE WITHOUT WARRANTY.

    All contributions by Paul Vojta or C. Masloch to the debugger are
    available under a choice of three different licenses. These are the Fair
    License, the Simplified 2-Clause BSD License, or the MIT License.

    This is the license and copyright information that applies to lDebug;
    but note that there have been substantial contributions to the code base
    that are not copyrighted (public domain).

16: Comparison of lDebug to MS-DOS Debug
----------------------------------------

    This section lists some benefits of lDebug, as compared to MSDebug. It
    originates in the MSDebug manual. MSDebug is based on the Debug of the
    2018 free software release of MS-DOS version 2.

    First, there are some differences between MSDebug and the original MS-
    DOS Debug which make MSDebug more similar to lDebug:

     -  K command to modify only the internal buffers for the program load
        filename, the PSP command line tail, and the PSP FCBs

     -  Child process allocated using interrupt 21h function 48h and
        initialised using function 55h

     -  After termination of debuggee a new child process is created

     -  Restores interrupt 1 and 3 vectors (similar to lDDebug)

     -  BU command like lDDebug's

     -  .HEX file read ends on NUL byte (0), EOF byte (1Ah), or End Of File

     -  Bugfix: Move command M will correctly move forwards or backwards
        based on the linear address, fixing overlapping moves in which the
        segments differ in the opposite way to the linear addresses

    Here's the advantages of lDebug as compared to MSDebug:

     -  Expression evaluator can be used whereever a number is to be parsed

     -  D, U, T, TP, P, G commands can be repeated with autorepeat

     -  Permanent breakpoints (B commands)

     -  G command can re-use prior breakpoints list with G AGAIN command (or
        autorepeat)

     -  Several variables beyond the 16-bit registers to control the
        debugger or store calculation results

     -  Paging to allow reading longer outputs

     -  686 level assembler and disassembler

     -  DPMI build lDebugX for debugging DPMI clients, supporting 32-bit
        offsets in segments

     -  InDOS mode to switch to ROM-BI0S video and keyboard I/O rather than
        DOS's standard output and input

     -  Line editor and line history (if not using the DOS line input
        function)

     -  Can be boot loaded for debugging Real/Virtual 86 Mode kernels

     -  Can be installed as a device driver in CONFIG.SYS

     -  Script for lDebug file reading using the Y command

     -  Serial I/O mode

     -  Conditional tracing for the T, TP, and P commands using a condition
        after a WHILE keyword

     -  Buffered tracing for T, TP, and P using a SILENT keyword

     -  T defaults to proceeding past software interrupt calls, can be
        modified using Trace Mode (TM command)

     -  TP command which proceeds past repeated string instructions

     -  DM command to list MCBs

     -  DI command to dump interrupt handler chains

     -  DW and DD commands to dump data in words or dwords

     -  32-bit numeric handling

     -  F and S commands can use a memory source instead of a list, using a
        RANGE keyword

     -  H command can display an expression result in hexadeximal, decimal,
        or one arbitrary base of choice

     -  I and O commands have IW/OW and ID/OD variants for word and
        doubleword port I/O

     -  R command can be switched to display 32-bit and 386 registers

     -  Machine type can be set to make the assembler and disassembler
        display when the machine does not support an instruction

     -  QA command can be used to try to terminate an attached process

     -  S command can search backwards using the REVERSE keyword

     -  Provides a number of online help pages

     -  RN command to dump 8087 registers

     -  RM command to dump MMX registers, and variables to read and write
        them

     -  RE command buffer to run commands from T, TP, P, or G dump calls

     -  RC command buffer to run commands at startup or group several
        commands later on

     -  Numeric inputs can be specified with a hash sign "#" modifier to
        enter in arbitrary numeric bases

     -  Access variables and VALUE IN constructs to detect memory
        accesses before they are actually carried out (requring to trace
        instructions)

     -  TSR and ATTACH commands to detach from or attach to a process

     -  IF command to conditionally run another command

     -  Timer and AMIS interrupt hooks (optional)

    Furthermore, lDebug can be built using the free software Netwide
    Assembler, rather than relying on a binary-only Microsoft Macro
    Assembler. (The assembler executable shipped with MSDebug is technically
    free, but it does not have sources.)

    However, there are some disadvantages to lDebug as well:

     -  Memory use and executable size can easily reach as much as ten times
        that of MSDebug

     -  Less compatibility to original MS-DOS Debug

     -  Performance may be worse

     -  May require some MS-DOS version 3 or version 5 features

17: Additional usage conditions
-------------------------------

    The program executables can be compressed with a choice of different
    compressors. The files then contain a decompression stub. Some of
    these stubs have their own usage conditions. The following stub usage
    conditions apply, if one of these stubs is used.

17.1 BriefLZ depacker usage conditions

    BriefLZ - small fast Lempel-Ziv

    8086 Assembly lDOS iniload payload BriefLZ depacker

    Based on: BriefLZ C safe depacker

    Copyright (c) 2002-2016 Joergen Ibsen

    This software is provided 'as-is', without any express or implied
    warranty. In no event will the authors be held liable for any damages
    arising from the use of this software.

    Permission is granted to anyone to use this software for any purpose,
    including commercial applications, and to alter it and redistribute it
    freely, subject to the following restrictions:

     1. The origin of this software must not be misrepresented; you must not
        claim that you wrote the original software. If you use this software
        in a product, an acknowledgment in the product documentation would
        be appreciated but is not required.

     2. Altered source versions must be plainly marked as such, and must not
        be misrepresented as being the original software.

     3. This notice may not be removed or altered from any source
        distribution.

17.2 LZ4 depacker usage conditions

    8086 Assembly lDOS iniload payload LZ4 depacker

        by C. Masloch, 2018

    Usage of the works is permitted provided that this instrument is
    retained with the works, so that any entity that uses the works is
    notified of this instrument.

    DISCLAIMER: THE WORKS ARE WITHOUT WARRANTY.

17.3 Snappy depacker usage conditions

    8086 Assembly lDOS iniload payload Snappy depacker

        by C. Masloch, 2018

    Usage of the works is permitted provided that this instrument is
    retained with the works, so that any entity that uses the works is
    notified of this instrument.

    DISCLAIMER: THE WORKS ARE WITHOUT WARRANTY.

17.4 Exomizer depacker usage conditions

    8086 Assembly lDOS iniload payload exomizer raw depacker

        by C. Masloch, 2020

    Copyright (c) 2005-2017 Magnus Lind.

    This software is provided 'as-is', without any express or implied
    warranty. In no event will the authors be held liable for any damages
    arising from the use of this software.

    Permission is granted to anyone to use this software for any purpose,
    including commercial applications, and to alter it and redistribute it
    freely, subject to the following restrictions:

     1. The origin of this software must not be misrepresented * you
        must not claim that you wrote the original software. If you use
        this software in a product, an acknowledgment in the product
        documentation would be appreciated but is not required.

     2. Altered source versions must be plainly marked as such, and must not
        be misrepresented as being the original software.

     3. This notice may not be removed or altered from any distribution.

     4. The names of this software and/or it's copyright holders may not
        be used to endorse or promote products derived from this software
        without specific prior written permission.

17.5 X compressor depacker usage conditions

    MIT License

    Copyright (c) 2020 David Barina

    Permission is hereby granted, free of charge, to any person obtaining
    a copy of this software and associated documentation files (the
    "Software"), to deal in the Software without restriction, including
    without limitation the rights to use, copy, modify, merge, publish,
    distribute, sublicense, and/or sell copies of the Software, and to
    permit persons to whom the Software is furnished to do so, subject to
    the following conditions:

    The above copyright notice and this permission notice shall be included
    in all copies or substantial portions of the Software.

    THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
    EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
    MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
    IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
    CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
    TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
    SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.

17.6 Heatshrink depacker usage conditions

    8086 Assembly lDOS iniload payload heatshrink depacker

        by C. Masloch, 2020

    Usage of the works is permitted provided that this instrument is
    retained with the works, so that any entity that uses the works is
    notified of this instrument.

    DISCLAIMER: THE WORKS ARE WITHOUT WARRANTY.

17.7 Lzd usage conditions

    Lzd - Educational decompressor for the lzip format

        Copyright (C) 2013-2019 Antonio Diaz Diaz.

    This program is free software. Redistribution and use in source and
    binary forms, with or without modification, are permitted provided that
    the following conditions are met:

     1. Redistributions of source code must retain the above copyright
        notice, this list of conditions and the following disclaimer.

     2. Redistributions in binary form must reproduce the above copyright
        notice, this list of conditions and the following disclaimer in the
        documentation and/or other materials provided with the distribution.

    This program is distributed in the hope that it will be useful,
    but WITHOUT ANY WARRANTY; without even the implied warranty of
    MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.

17.8 LZO depacker usage conditions

    8086 Assembly lDOS iniload payload LZO depacker

        by C. Masloch, 2020

    Usage of the works is permitted provided that this instrument is
    retained with the works, so that any entity that uses the works is
    notified of this instrument.

    DISCLAIMER: THE WORKS ARE WITHOUT WARRANTY.

17.9 LZSA2 depacker usage conditions

    8086 Assembly lDOS iniload payload LZSA2 depacker

        by C. Masloch, 2021

        based on:

    decompress_small.S - space-efficient decompressor implementation for
    8088

    Copyright (C) 2019 Emmanuel Marty

    This software is provided 'as-is', without any express or implied
    warranty. In no event will the authors be held liable for any damages
    arising from the use of this software.

    Permission is granted to anyone to use this software for any purpose,
    including commercial applications, and to alter it and redistribute it
    freely, subject to the following restrictions:

     1. The origin of this software must not be misrepresented; you must not
        claim that you wrote the original software. If you use this software
        in a product, an acknowledgment in the product documentation would
        be appreciated but is not required.

     2. Altered source versions must be plainly marked as such, and must not
        be misrepresented as being the original software.

     3. This notice may not be removed or altered from any source
        distribution.

17.10 aPLib depacker usage conditions

    8086 Assembly lDOS iniload payload aPLib depacker

        by C. Masloch, 2021

        based on:

    aplib_8088_small.S - size-optimized aPLib decompressor for 8088 - 145
    bytes

    Copyright (C) 2019 Emmanuel Marty

    This software is provided 'as-is', without any express or implied
    warranty. In no event will the authors be held liable for any damages
    arising from the use of this software.

    Permission is granted to anyone to use this software for any purpose,
    including commercial applications, and to alter it and redistribute it
    freely, subject to the following restrictions:

     1. The origin of this software must not be misrepresented; you must not
        claim that you wrote the original software. If you use this software
        in a product, an acknowledgment in the product documentation would
        be appreciated but is not required.

     2. Altered source versions must be plainly marked as such, and must not
        be misrepresented as being the original software.

     3. This notice may not be removed or altered from any source
        distribution.

17.11 bzpack depacker usage conditions

    8086 Assembly lDOS iniload payload bzpack depacker

        by C. Masloch, 2021

    BSD 2-Clause License

    Copyright (c) 2021, Milos Bazelides

    All rights reserved.

    Redistribution and use in source and binary forms, with or without
    modification, are permitted provided that the following conditions are
    met:

     1. Redistributions of source code must retain the above copyright
        notice, this list of conditions and the following disclaimer.

     2. Redistributions in binary form must reproduce the above copyright
        notice, this list of conditions and the following disclaimer in the
        documentation and/or other materials provided with the distribution.

    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
    "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
    LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
    A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
    HOLDER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
    SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED
    TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR
    PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
    LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
    NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
    SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Source Control Revision ID
--------------------------

    hg a62bc3bcdce1, from commit on at 2023-08-03 16:49:01 +0200

    If this is in ecm's repository, you can find it at
    https://hg.pushbx.org/ecm/ldebug/rev/a62bc3bcdce1

